<?xml version="1.0" encoding="utf-8"?>
<JingJiBiao Xmbh="xm001" Xmmc="中新苏滁高新区超级电容智能制造基地二期项目" Version="2.0" Jsfs="一般计税" Jsdw="滁州苏滁产城开发有限公司" Zjzmj="32333.32" Zhgddj="基本级">
  <ZhaoBiaoXx Zbr="滁州苏滁产城开发有限公司 " Zxr="安徽求是工程建设咨询有限公司" ZbrDb="1" ZxrDb="洪从胜" Bzr="李磊、夏雯豪、徐利" Fhr="黄思东" BzRq="2026-08-05" FhRq="2026-08-25" />
  <Dxgcxx Dxgcmc="厂房三" Dxgcbh="dx001" Je="0" Bkjzf="0" Aqwmf="0" Zgj="0" Jzmj="27397.32" Aqsczrbxf="0">
    <Dwgcxx Dwgcbh="00001" Dwgcmc="厂房三（土建）" Zylb="1" Jzmj="27397.32" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B9767C6F3B122686496A" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="0101" Mc="土石方工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="010101001001" Mc="平整场地" Xmtz="1．土壤类别：综合，不分类别" Gcnr="" Jsgz="按建筑物首层建筑面积，以面积计算" Dw="m2" Sl="7694.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="010101004001" Mc="挖基坑土方、挖沟槽土方" Xmtz="1．土壤类别：自行考虑&#xD;&#xA;2．挖土深度：5m以内&#xD;&#xA;3．部位：基础、基础梁、集水坑等&#xD;&#xA;4．开挖过程中所遇淤泥、建筑垃圾、房屋基础、设备基础、障碍物等投标单位自行考虑在报价中，中标后不予调整&#xD;&#xA;5．运距：控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示尺寸基坑底面积乘以挖土深度，以体积计算" Dw="m3" Sl="6744.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="WB010101011001" Mc="人工清底" Xmtz="1．清底范围：按施工所需清底的面积&#xD;&#xA;2．土壤类别：综合，不分类别&#xD;&#xA;3．清底要求：在接近设计标高时必须预留一定厚度的土层使用人工清理，预留土层厚度按施工规范执行，投标单位综合考虑报价，中标后不予调整" Gcnr="" Jsgz="按需清底的范围，以面积计算" Dw="m2" Sl="2355.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="010103001001" Mc="回填方" Xmtz="1．部位：基础回填&#xD;&#xA;2．夯填（碾压）:素土夯实,压实系数≥0.94&#xD;&#xA;3．运距：控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示尺寸,以体积计算" Dw="m3" Sl="5055.64" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0103" Mc="桩基工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="5" Qdbm="010301002001" Mc="预制钢筋混凝土管桩（试桩）" Xmtz="1．地层情况：自行考虑&#xD;&#xA;2．桩种类、规格、型号：PHC500AB100&#xD;&#xA;3．混凝土强度等级：C80&#xD;&#xA;4．桩长度：20m、21m&#xD;&#xA;5．包含送桩费用" Gcnr="" Jsgz="按设计图示截面积乘以桩长（包括桩尖），以体积计算" Dw="m" Sl="61.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="WB010301007001" Mc="接桩（试桩）" Xmtz="1．桩类型：预应力高强混凝土管桩&#xD;&#xA;2．桩径：500mm&#xD;&#xA;3．预制桩应尽量减少接桩接头数量" Gcnr="" Jsgz="按接头数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="WB010301006001" Mc="管桩填心（试桩）" Xmtz="1．桩种类、规格、型号：PHC500AB100&#xD;&#xA;2．填心深度：1.5m&#xD;&#xA;3．填心材料：C40微膨胀混凝土" Gcnr="" Jsgz="按设计取土（填土）体积计算" Dw="m3" Sl="0.32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="WB010301003001" Mc="钢桩尖制作、安装（试桩）" Xmtz="1．类型：锥形闭口型钢桩尖" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.277" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="010515004001" Mc="钢筋笼制安（试桩）" Xmtz="1．钢筋种类、规格：参图集《先张法预应力混凝土管桩》(23G409)&#xD;&#xA;2．托盘：4-5mm厚圆薄钢板" Gcnr="" Jsgz="按设计图示钢筋（网）长度（面积）乘单位理论质量计算。" Dw="t" Sl="0.083" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="010301004001" Mc="截（凿）桩头（试桩）" Xmtz="1．桩类型、桩头截面：PHC500AB100&#xD;&#xA;2．混凝土强度等级：C80&#xD;&#xA;3．有无钢筋：有&#xD;&#xA;4．含桩头废料的清理、外弃" Gcnr="" Jsgz="1.灌注混凝土桩凿桩头，按设计桩截面乘以桩头长度，以体积计算2.预制方（管）桩截（凿）桩头，按设计图示数量计算" Dw="根" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="010301002002" Mc="预制钢筋混凝土管桩" Xmtz="1．地层情况：自行考虑&#xD;&#xA;2．桩种类、规格、型号：PHC500AB100&#xD;&#xA;3．混凝土强度等级：C80&#xD;&#xA;4．桩长度：20m、21m&#xD;&#xA;5．包含送桩费用" Gcnr="" Jsgz="按设计图示截面积乘以桩长（包括桩尖），以体积计算" Dw="m" Sl="9666.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="WB010301007002" Mc="接桩" Xmtz="1．桩类型：预应力高强混凝土管桩&#xD;&#xA;2．桩径：500mm&#xD;&#xA;3．预制桩应尽量减少接桩接头数量" Gcnr="" Jsgz="按接头数量计算" Dw="个" Sl="483" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="WB010301006002" Mc="管桩填心" Xmtz="1．桩种类、规格、型号：PHC500AB100&#xD;&#xA;2．填心深度：1.5m&#xD;&#xA;3．填心材料：C40微膨胀混凝土" Gcnr="" Jsgz="按设计取土（填土）体积计算" Dw="m3" Sl="51.19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="WB010301003002" Mc="钢桩尖制作、安装" Xmtz="1．类型：锥形闭口型钢桩尖" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="44.629" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="010515004002" Mc="钢筋笼制安" Xmtz="1．钢筋种类、规格：参图集《先张法预应力混凝土管桩》(23G409)&#xD;&#xA;2．托盘：4-5mm厚圆薄钢板" Gcnr="" Jsgz="按设计图示钢筋（网）长度（面积）乘单位理论质量计算。" Dw="t" Sl="13.275" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="010301004002" Mc="截（凿）桩头" Xmtz="1．桩类型、桩头截面：PHC500AB100&#xD;&#xA;2．混凝土强度等级：C80&#xD;&#xA;3．有无钢筋：有&#xD;&#xA;4．含桩头废料的清理、外弃" Gcnr="" Jsgz="1.灌注混凝土桩凿桩头，按设计桩截面乘以桩头长度，以体积计算2.预制方（管）桩截（凿）桩头，按设计图示数量计算" Dw="根" Sl="483" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="010904002001" Mc="预制管桩头防水" Xmtz="1．涂膜厚度、遍数：2.0厚水泥基防水涂料&#xD;&#xA;2．钢筋混凝土桩头(清理干净)" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="379.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0104" Mc="砌筑工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="18" Qdbm="010401001001" Mc="砖基础" Xmtz="1．部位：地面以下或防潮层以下直接与土接触的墙体&#xD;&#xA;2．砖品种、规格、强度级：MU20的混凝土普通实心砖&#xD;&#xA;3．砂浆强度级：DM M10预拌砂浆砌筑" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="15.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="010401001002" Mc="砖胎膜" Xmtz="1．砖品种、规格、强度级：非黏土实心砖&#xD;&#xA;2．砂浆强度级：DM M10预拌砂浆砌筑" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="25.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="010402001001" Mc="砌块墙" Xmtz="1．部位：内外隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：100mm(高度3.6m以下）&#xD;&#xA;4．砂浆强度级：M5.0专用混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="10.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="010402001002" Mc="砌块墙" Xmtz="1．部位：内外隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：100mm(高度3.6m以上）&#xD;&#xA;4．砂浆强度级：M5.0专用混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="4.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="010402001003" Mc="砌块墙" Xmtz="1．部位：内外隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以下）&#xD;&#xA;4．砂浆强度级：M5.0专用混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="519.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="010402001004" Mc="砌块墙" Xmtz="1．部位：内外隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以上）&#xD;&#xA;4．砂浆强度级：M5.0专用混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="315.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="010402001005" Mc="砌块墙" Xmtz="1．部位：卫生间隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：100mm(高度3.6m以下）&#xD;&#xA;4．砂浆强度级：M5.0混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="8.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="010402001006" Mc="砌块墙" Xmtz="1．部位：卫生间隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以下）&#xD;&#xA;4．砂浆强度级：M5.0混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="71.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="010402001007" Mc="砌块墙" Xmtz="1．部位：卫生间隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以上）&#xD;&#xA;4．砂浆强度级：M5.0混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="23.27" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="WB010401016001" Mc="砖砌台阶" Xmtz="1．部位：出屋面台阶&#xD;&#xA;2．砖品种、规格、强度级：MU20页岩多孔砖&#xD;&#xA;3．砂浆强度级：M5.0砌筑砂浆&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1.44" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="WB010401015001" Mc="墙基防潮层" Xmtz="1．部位：在室内地坪下0.06m处&#xD;&#xA;2．防潮层材料种类：60厚C20细石混凝土掺4%~5%防水剂" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="20.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0105" Mc="混凝土工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="29" Qdbm="010404001001" Mc="垫层" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．材料品种及比例：C20混凝土" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="178.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="010501003001" Mc="独立基础及桩承台" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C40" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1223.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="010501004001" Mc="满堂基础" Xmtz="1．部位：电梯基坑、沉淀池底板等&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35 防水混凝土，抗渗等级为P10" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="19.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="010501004002" Mc="满堂基础" Xmtz="1．部位：提升基坑、漏液收集坑、电缆井底板等&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30防水混凝土，抗渗等级为P10" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="3.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="010501006001" Mc="设备基础" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="3.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="010502001001" Mc="矩形柱" Xmtz="1．柱规格形状：矩形1.6m以内&#xD;&#xA;2．周长：1.6m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="24.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="010502001002" Mc="矩形柱" Xmtz="1．柱规格形状：矩形1.6m以内&#xD;&#xA;2．周长：1.6m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C35" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="18.38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="010502001003" Mc="矩形柱" Xmtz="1．柱规格形状：矩形1.6m以内&#xD;&#xA;2．周长：1.6m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C40" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="24.22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="37" Qdbm="010502001004" Mc="矩形柱" Xmtz="1．柱规格形状：矩形&#xD;&#xA;2．周长：2.4m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="142.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="010502001005" Mc="矩形柱" Xmtz="1．柱规格形状：矩形&#xD;&#xA;2．周长：2.4m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C35" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="160.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="010502001006" Mc="矩形柱" Xmtz="1．柱规格形状：矩形&#xD;&#xA;2．周长：2.4m以外&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C35" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="274.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="010502001007" Mc="矩形柱" Xmtz="1．柱规格形状：矩形&#xD;&#xA;2．周长：2.4m以外&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C40" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="669.35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="010501006002" Mc="混凝土包柱脚" Xmtz="1．部位：包柱脚部位&#xD;&#xA;2．混凝土强度等级：C40细石混凝土无收缩高强灌浆料" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="010501006003" Mc="混凝土填实" Xmtz="1．部位：杯口基础与钢柱相交处&#xD;&#xA;2．做法：钢柱定位校正后,，底面及侧面用C40细石混凝土填实" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="5.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="010502002001" Mc="构造柱" Xmtz="1．位置：构造柱&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="73.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="010503001001" Mc="基础梁" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="133.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="010503002001" Mc="矩形梁" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="53.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="010503004001" Mc="圈梁" Xmtz="1．部位：反坎、门槛、水平系圈梁、电梯圈梁、楼板防撞反坎等&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="107.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="010503005001" Mc="过梁" Xmtz="1．部位：门窗洞口过梁&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="010504001001" Mc="直形墙" Xmtz="1．墙规格：地下250mm以内&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35防水混凝土，抗渗等级为P10" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="13.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="010504001002" Mc="直形墙" Xmtz="1．墙规格：地下250mm以内&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30防水混凝土，抗渗等级为P10" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="6.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="50" Qdbm="WB010504003001" Mc="电梯井墙" Xmtz="1．墙规格：250mm以内&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35 防水混凝土，抗渗等级为P10" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="23.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="010505001001" Mc="有梁板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="4639.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="010505001002" Mc="有梁板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30防水混凝土，抗渗等级为P6" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1287.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="010505003001" Mc="平板" Xmtz="1．部位：桁架楼承板&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="34.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="010505003002" Mc="平板" Xmtz="1．部位：井道盖板&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="010505006001" Mc="栏板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="94.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="010505008001" Mc="雨篷板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以伸出外墙部分的水平投影面积计算" Dw="m2" Sl="4.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="010505007001" Mc="天沟、挑檐板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="32.19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="010506001001" Mc="直形楼梯" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="" Dw="m2" Sl="140.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="010507005001" Mc="扶手、压顶" Xmtz="1．部位：压顶&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="2.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="010507003001" Mc="地沟、电缆沟" Xmtz="1．部位：排水沟&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="11.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="010507001001" Mc="散水" Xmtz="1．基层处理：素土夯实&#xD;&#xA;2．混凝土强度等级：100mm厚C25混凝土随打随抹光，150厚卵石灌M2.5号混合砂浆砂浆&#xD;&#xA;3．从建筑边缘向外找坡5%,每隔6-10m设置一道伸缩缝。缝宽20mm,散水与外墙间设通缝,缝宽20mm,转角处设置45°缝,缝内填沥青胶泥。" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="312.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="010507001002" Mc="坡道" Xmtz="1．基层处理：素土夯实&#xD;&#xA;2．混凝土强度等级：300厚级配砂石稳定层，150厚C25混凝土(内配φ8@200单层双向)&#xD;&#xA;3．界面剂一道，25厚耐磨砂浆面层,表面划出横向纹道&#xD;&#xA;4．与室内地面间设缝,缝宽20mm,缝内填沥青砂浆" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="171.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="010507004001" Mc="台阶" Xmtz="1．素土夯实,压实系数不小于0.94&#xD;&#xA;2．混凝土强度等级：100厚C25混凝土(内配φ8@200单层双向)，300厚级配砂石稳定层&#xD;&#xA;3．20厚1:2水泥砂浆抹面，素水泥浆一道&#xD;&#xA;4．与室内地面间设缝,缝宽20mm,缝内填沥青砂浆" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="10.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="010507004002" Mc="台阶平台" Xmtz="1．素土夯实,压实系数不小于0.94&#xD;&#xA;2．混凝土强度等级：100厚C25混凝土(内配φ8@200单层双向)，300厚级配砂石稳定层&#xD;&#xA;3．20厚1:2水泥砂浆抹面，素水泥浆一道&#xD;&#xA;4．与室内地面间设缝,缝宽20mm,缝内填沥青砂浆" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="31.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="010508001001" Mc="后浇带" Xmtz="1．部位：基础梁&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35补偿收缩混凝土" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="010508001002" Mc="后浇带" Xmtz="1．部位：梁&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35补偿收缩混凝土" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="24.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="010508001003" Mc="后浇带" Xmtz="1．部位：板&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C35补偿收缩混凝土" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="56.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="010515001001" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HPB300级钢&#xD;&#xA;2．钢筋规格：Φ6&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="2.564" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="010515001002" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HPB300级钢&#xD;&#xA;2．钢筋规格：Φ8&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="8.120" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="70" Qdbm="010515001003" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ6&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="9.701" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="71" Qdbm="010515001004" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ8&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="342.795" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="010515001005" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ10&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="234.976" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="010515001006" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ12&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="39.195" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="010515001007" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ14&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="10.220" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="010515001008" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ16&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="16.764" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="010515001009" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ18&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="33.952" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="010515001010" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ20&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="44.103" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="010515001011" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ22&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="83.011" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="010515001012" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ25&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="107.129" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="010515001013" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ28&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="456.474" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="010515001014" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ32&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="18.908" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="010516002001" Mc="预埋铁" Xmtz="1．钢材种类：预埋铁件制作&#xD;&#xA;2．铁件尺寸：角钢、钢板等预埋件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="5.402" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="010516003001" Mc="钢筋连接" Xmtz="1．连接方式：电渣压力焊" Gcnr="" Jsgz="按实际数量计算" Dw="个" Sl="906" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="010516003002" Mc="钢筋连接" Xmtz="1．连接方式：直螺纹套筒连接&#xD;&#xA;2．规格：Φ16以上" Gcnr="" Jsgz="按实际数量计算" Dw="个" Sl="13710" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="WB010516004001" Mc="墙体拉结筋" Xmtz="1．钢筋种类：HRB300&#xD;&#xA;2．钢筋规格：Φ6" Gcnr="" Jsgz="按设计图示钢筋尺寸，以质量计算" Dw="t" Sl="5.423" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="WB010516005001" Mc="墙面钢板（丝）网" Xmtz="1．部位：两种不同基体交界处&#xA;2．钢筋网（钢丝网）种类、规格：不同材质交界处挂宽400mm的密纹钢丝网。钢丝网直径为0.9mm，钢丝网网孔尺寸为12.7mmX12.7mm" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="40.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="WB010516005002" Mc="墙面钢板（丝）网" Xmtz="1．钢筋种类、规格：后浇带处专用钢丝网隔断" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="165.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="WB010516005003" Mc="墙面钢板（丝）网" Xmtz="1．钢筋网（钢丝网）种类、规格：外墙面满铺&#xD;&#xA;2．耐碱玻纤网格布" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4491.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0106" Mc="金属结构工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="89" Qdbm="WB010603001001" Mc="钢柱" Xmtz="1．柱类型：连廊、集装箱装配区钢柱&#xA;2．钢柱材质：Q355B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．含依附于钢柱上的牛腿、女儿墙钢柱、连接板、加劲板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="50.843" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="010604001001" Mc="钢梁" Xmtz="1．梁类型：连廊、集装箱装配区钢梁&#xA;2．钢梁材质：Q355B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．含依附于钢梁上的连接板、加劲板等&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="" Dw="t" Sl="46.367" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="WB010603001002" Mc="钢柱" Xmtz="1．柱类型：集装箱装配区夹层钢柱&#xA;2．钢柱材质：Q235B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．含依附于钢柱上的牛腿、女儿墙钢柱、连接板、加劲板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="1.042" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="010604001002" Mc="钢梁" Xmtz="1．梁类型：集装箱装配区夹层钢梁&#xA;2．钢梁材质：Q235B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．含依附于钢梁上的连接板、加劲板等&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="" Dw="t" Sl="2.220" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="010606001001" Mc="钢支撑、钢拉条" Xmtz="1．类型：集装箱装配区钢支撑、系杆等&#xD;&#xA;2．钢材材质：Q235B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;5．含依附于钢支撑上的连接板、加劲板、节点板等&#xD;&#xA;6．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="20.873" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="010606002001" Mc="钢檩条" Xmtz="1．檩条类型：屋面檩条、墙面檩条、几字檩、门梁、门柱、窗梁、窗柱等&#xD;&#xA;2．钢材材质：Q355B镀锌钢材&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．含依附于梁、柱上的檩托、节点板、加劲肋、隔板、肋板、加强板、连接件等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="117.288" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="95" Qdbm="010606001002" Mc="钢拉条" Xmtz="1．类型：屋面钢拉条、斜拉条、撑杆、隅撑等&#xD;&#xA;2．钢材材质：Q235B镀锌钢材&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．含依附于钢拉条上的连接板、加劲板、节点板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="2.290" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="010606001003" Mc="钢拉条" Xmtz="1．类型：墙面钢拉条、斜拉条、撑杆等&#xD;&#xA;2．钢材材质：Q235B&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．含依附于钢拉条上的连接板、加劲板、节点板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="6.279" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="010606008001" Mc="钢梯" Xmtz="1．类型：屋面检修镀锌钢爬梯&#xA;2．防止人员随意攀登爬,护笼底部需要进行上锁设计,由专业厂家二次设计&#xD;&#xA;3．需满足规范GB4053.1—2009，做法可参15J401,D17页&#xD;&#xA;4．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="" Dw="t" Sl="0.545" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="010606008002" Mc="钢梯" Xmtz="1．参15J401-D7页WT3c-126&#xD;&#xA;2．除锈形式：抛丸除锈&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．所需预埋件等均包含在报价内&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.168" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="010606008003" Mc="钢爬梯（沉淀池）" Xmtz="1．参22S804 第191页&#xD;&#xA;2．除锈形式：抛丸除锈&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．所需预埋件等均包含在报价内&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.257" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="WB011405002001" Mc="金属构件油漆" Xmtz="1．油漆品种、刷漆遍数：环氧富锌(含锌量大于70%)底漆2遍&#xD;&#xA;2．所有非镀锌钢构件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="128.594" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="WB011405002002" Mc="金属构件油漆" Xmtz="1．油漆品种、刷漆遍数：环氧云铁中间涂料2遍&#xD;&#xA;2．所有非镀锌钢构件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="128.594" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="WB011405002003" Mc="金属构件油漆" Xmtz="1．油漆品种、刷漆遍数：脂肪族聚氨酯面漆3遍&#xD;&#xA;2．所有非镀锌钢构件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="128.594" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="010605001001" Mc="钢板楼板" Xmtz="1．部位：钢筋桁架楼层板&#xD;&#xA;2．楼承板型号：TD2-90&#xD;&#xA;3．楼板厚度：120mm&#xD;&#xA;4．含上弦钢筋、下弦钢筋、腹杆钢筋、底模钢板、侧边钢板包边等固定构件" Gcnr="" Jsgz="" Dw="m²" Sl="76.67" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="010605001002" Mc="钢板楼板" Xmtz="1．部位：钢筋桁架楼层板&#xD;&#xA;2．楼承板型号：TD5-100&#xD;&#xA;3．楼板厚度：130mm&#xD;&#xA;4．含上弦钢筋、下弦钢筋、腹杆钢筋、底模钢板、侧边钢板包边等固定构件" Gcnr="" Jsgz="" Dw="m²" Sl="188.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="010606011001" Mc="钢天沟" Xmtz="1．类型：3mm厚304不锈钢天沟&#xD;&#xA;2．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="4.759" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="WB010606016001" Mc="高强螺栓" Xmtz="1．强度：10.9级高强螺栓&#xD;&#xA;2．规格：M20" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="892" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="WB010606016002" Mc="高强螺栓" Xmtz="1．强度：10.9级高强螺栓&#xD;&#xA;2．规格：M22" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="168" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="108" Qdbm="WB010606016003" Mc="高强螺栓" Xmtz="1．强度：10.9级高强螺栓&#xD;&#xA;2．规格：M24" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="364" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="WB010606016004" Mc="高强螺栓" Xmtz="1．强度：10.9级高强螺栓&#xD;&#xA;2．规格：M27" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="WB010606016005" Mc="高强螺栓" Xmtz="1．强度：10.9级高强螺栓&#xD;&#xA;2．规格：M30" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="111" Qdbm="WB010606017001" Mc="栓钉" Xmtz="1．规格型号：Φ19栓钉&#xD;&#xA;2．焊接后长度为100mm" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1488" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="112" Qdbm="011407005001" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：钢柱、柱间支撑&#xA;2．耐火极限：3.0h&#xD;&#xA;3．非膨胀型防火涂料，防火涂料厚度不小于50mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="1122.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="113" Qdbm="011407005002" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：楼面钢梁&#xA;2．耐火极限：2.0h&#xD;&#xA;3．环氧类膨胀型防火涂料，防火涂料厚度≥5.0mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="378.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="114" Qdbm="011407005003" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：屋面梁、屋盖支撑、系杆等&#xA;2．耐火极限：1.5h&#xD;&#xA;3．膨胀型防火涂料，防火涂料厚度≥4.0mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="1068.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="115" Qdbm="010605002001" Mc="钢板墙板" Xmtz="1．部位：压型钢板复合保温外墙&#xD;&#xA;2．钢材品种、规格：0.6mm厚双面镀铝锌压型钢板外侧墙板,，镀铝锌量每面镀铝锌量≥180g/㎡，漆膜:正面HDP,厚度25um;背面为PE烤漆,厚度10um&#xD;&#xA;3．透气层：0.5mm防水透气膜 &#xD;&#xA;4．复合板夹芯材料种类、规格：100mm厚玻璃棉，容重≥16kg/m³&#xD;&#xA;5．含附加檩条压型彩钢板窗台板、压顶、包角、包边等构件费用" Gcnr="" Jsgz="按设计图示尺寸，以铺挂面积计算" Dw="m2" Sl="7211.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="116" Qdbm="WB010902005001" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层品种、规格、厚度：0.3mm厚聚脂膜隔汽层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="7211.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="117" Qdbm="010605002002" Mc="钢板墙板" Xmtz="1．部位：单层压型钢板复合保温泄爆外墙&#xD;&#xA;2．钢材品种、规格：0.6mm厚双面镀铝锌压型钢板外侧墙板,，镀铝锌量每面镀铝锌量≥180g/㎡，漆膜:正面HDP,厚度25um;背面为PE烤漆,厚度10um&#xD;&#xA;3．透气层：0.5mm防水透气膜 &#xD;&#xA;4．螺栓种类：泄爆螺栓和牵引绳&#xD;&#xA;5．复合板夹芯材料种类、规格：100mm厚玻璃棉，容重≥16kg/m³&#xD;&#xA;6．泄爆墙,质量≤60kg/m2参14J938-C9页-XQ2&#xD;&#xA;7．含附加檩条压型彩钢板窗台板、压顶、包角、包边等构件费用" Gcnr="" Jsgz="按设计图示尺寸，以铺挂面积计算" Dw="m2" Sl="36.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="118" Qdbm="010605002003" Mc="钢板墙板" Xmtz="1．部位：压型钢板内墙板&#xD;&#xA;2．钢材品种、规格：0.5厚双面镀铝锌压型钢板内侧墙板，镀铝锌量每面镀铝锌量≥150g/㎡，漆膜:PE烤漆,厚度20/5um&#xD;&#xA;3．含附加檩条压型彩钢板窗台板、包角、包边等构件费用" Gcnr="" Jsgz="按设计图示尺寸，以铺挂面积计算" Dw="m2" Sl="7175.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="119" Qdbm="WB011209016001" Mc="楼层防火带" Xmtz="1．部位：楼板与板墙交接处&#xD;&#xA;2．骨架材料种类、规格：200高防火岩棉防水透气膜包覆&#xD;&#xA;3．钢板厚度：1.5厚镀锌钢板承托板，防火胶封口，含彩钢收边件" Gcnr="" Jsgz="按设计图示尺寸以延长米计算" Dw="m" Sl="768.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="120" Qdbm="WB010605003001" Mc="钢结构雨棚" Xmtz="1．清单按水平投影面积计入&#xA;2．0.6厚镀锌压型钢板屋面上板，0.6厚镀锌压型钢板屋面下板&#xD;&#xA;3．含彩钢盖缝板、泛水板、彩板包边、板边处理、阴阳角、洞口收边、闭孔泡沫堵头、拉铆钉连接等" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="82.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="121" Qdbm="WB010605003002" Mc="钢板屋面板" Xmtz="1．部位：压型钢板复合保温屋面&#xD;&#xA;2．钢板厚度：0.6厚镀锌压型彩钢板&#xD;&#xA;3．复合板夹芯材料种类、规格：100mm环保玻璃棉保温层,防火A级,容重不小于16kg/m³" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1425.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="122" Qdbm="WB010902005002" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层品种、规格、厚度：复合YH38高强度聚丙烯贴面" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1425.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="123" Qdbm="010902001001" Mc="屋面卷材防水" Xmtz="1．卷材品种、规格、厚度：1.8mm厚热塑性聚烯烃(TPO)防水卷材" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1425.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="124" Qdbm="WB010516005004" Mc="钢板（丝）网" Xmtz="1．部位：钢板屋面&#xA;2．钢筋网（钢丝网）种类、规格：不锈钢丝网,钢丝直径1.2,网目为双向200x200" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1425.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0108" Mc="门窗工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="125" Qdbm="010804003001" Mc="成品钢质平开门" Xmtz="1．门名称：成品钢质平开门&#xA;2．门材质：钢质门门板不小于0.8mm冷轧镀锌钢板，门框1.5mm厚冷轧镀锌钢板（高强度铝蜂窝填充）&#xA;3．五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="" Dw="m2" Sl="58.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="126" Qdbm="010802003001" Mc="钢质防火门" Xmtz="1．门名称：成品钢质甲级防火门&#xD;&#xA;2．门材质：防火门门板不小于0.8mm冷轧镀锌钢板，门框1.5mm厚冷轧镀锌钢板（内填岩棉）&#xD;&#xA;3．观察窗：6厚铯钾玻璃&#xD;&#xA;4．五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、防火合页、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="81.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="127" Qdbm="010802003002" Mc="钢质防火门" Xmtz="1．门名称：成品钢质乙级防火门&#xD;&#xA;2．门材质：防火门门板不小于0.8mm冷轧镀锌钢板，门框1.5mm厚冷轧镀锌钢板（内填岩棉）&#xD;&#xA;3．观察窗：6厚铯钾玻璃&#xD;&#xA;4．五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、防火合页、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="36.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="128" Qdbm="010802003003" Mc="钢质防火门" Xmtz="1．门名称：成品钢质丙级防火门&#xD;&#xA;2．门材质：防火门门板不小于0.8mm冷轧镀锌钢板，门框1.5mm厚冷轧镀锌钢板（内填岩棉）&#xD;&#xA;3．五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、防火合页、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="8.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="129" Qdbm="010802001001" Mc="成品泄爆门" Xmtz="1．门名称、代号及洞口尺寸：XBM2023&#xD;&#xA;2．门材质：成品泄爆门（含配套门套）&#xD;&#xA;3．参图集14J938之B2~B5，泄爆门的根据标准图中要求由厂家在满足安全要求的前提下，自行核定；泄爆门材质为钢制&#xD;&#xA;4．五金品种、规格：含安装、配套所有五金配件等所有五金" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="4.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="130" Qdbm="010802001002" Mc="金属门" Xmtz="1．门名称、代号及洞口尺寸：铝合金玻璃门&#xD;&#xA;2．玻璃品种、厚度：6中透光Low-E+12空气+6透明防火钢化玻璃&#xD;&#xA;3．铝合金门框型材壁厚不小于2mm&#xD;&#xA;4．包含门套、防撞提示标志、锁具、门把手等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="12.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="131" Qdbm="010801001001" Mc="木质门" Xmtz="1．门代号及洞口尺寸：成品木门&#xD;&#xA;2．实木门框、模压木质门扇&#xD;&#xA;3．门下方设铝合金百叶&#xD;&#xA;4．五金品种、规格：包含门套、锁具、门把手等所有五金配件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="41.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="132" Qdbm="010803001001" Mc="快速卷帘门" Xmtz="1．门代号及洞口尺寸：快速卷帘门&#xD;&#xA;2．门材质：2.0厚不锈钢立柱，无缝滚筒及1.2厚冷板箱罩，不锈钢型材水平加强杆，多排式毛刷密封；1.5厚高强度化纤软质防水布(带PVC透明视窗)&#xD;&#xA;3．启闭速度:1.0m/s,耐燃性:离火5s自动熄灭&#xD;&#xA;4．雷达感应,高频电机与减速器整体装置,380V IP55,低噪音,带断电制动器、手动制动释放&#xD;&#xA;5．五金要求：含安装、打胶、配套所有五金配件" Gcnr="" Jsgz="按设计图纸安装高度乘以门的实际宽度，以面积计算" Dw="m2" Sl="32.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="133" Qdbm="010803001002" Mc="电动钢制卷帘门（带防风杆）" Xmtz="1．门代号及洞口尺寸：电动钢制卷帘门&#xD;&#xA;2．门材质：1.5mm厚镀锌钢框，帘片冷轧镀锌钢板,厚度不小于0.8mm&#xD;&#xA;3．卷帘门开启速度速度0.5M/S&#xD;&#xA;4．一层及平台层所有外立面卷帘门均设置，3m≤门宽≤4.7m，5厚80X100Q355镀锌矩形钢管，3m≤门宽≤4.7m，5厚80X100Q355镀锌矩形钢管，安全扣镀锌管φ30*3.54个，防风扣镀锌管120*120*3，吊装固定扣φ10钢筋锚入混凝土100&#xD;&#xA;5．五金要求：含安装、打胶、配套所有五金配件&#xD;&#xA;6．清单工程量为卷帘门洞口尺寸（包括卷帘箱高度），卷帘箱及上部封堵、导轨等所有配件，投标人自行综合考虑在报价内" Gcnr="" Jsgz="按设计图纸安装高度乘以门的实际宽度，以面积计算" Dw="m2" Sl="294.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="134" Qdbm="010803002001" Mc="手动+电动无机防火卷帘门" Xmtz="1．门代号及洞口尺寸：手动+电动无机防火卷帘门&#xD;&#xA;2．门材质：1.5mm厚镀锌钢框，帘片不燃性无机材料&#xD;&#xA;3．卷帘门开启速度速度0.5M/S,耐火隔热性≥4.0小时且耐火完成性≥4.0小时,专业厂家设计、制作、安装应符合《防火卷帘 第1部分:通用技术条件》GB 14102.1-2024内的相关要求&#xD;&#xA;4．五金要求：含安装、打胶、配套所有五金配件&#xD;&#xA;5．清单工程量为卷帘门洞口尺寸（包括卷帘箱高度），卷帘箱及上部封堵、导轨等所有配件，投标人自行综合考虑在报价内" Gcnr="" Jsgz="按设计图纸安装高度乘以门的实际宽度,以面积计算" Dw="m2" Sl="8.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="135" Qdbm="WB010803003001" Mc="金属卷闸门电动装置" Xmtz="1．启动装置品种、规格：电动钢制卷帘门" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="136" Qdbm="WB010803003002" Mc="防火卷帘门电动装置" Xmtz="1．启动装置品种、规格：电动防火卷帘门" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="137" Qdbm="010807001001" Mc="金属窗 " Xmtz="1．窗代号及洞口尺寸：80系列断热铝合金中空玻璃窗&#xD;&#xA;2．窗材质：铝合金外窗主型材主要受力部位基材截面最小实测壁厚不应小于1.8mm,内窗主型材最小实测壁厚小于1.4mm，隔热尼龙条,宽度≥24mm（表面粉末喷涂）&#xD;&#xA;3．玻璃品种、厚度：6透明+12空气+6透明钢化安全玻璃（卫生间采用磨砂玻璃，消防救援窗口玻璃应易于破碎）&#xD;&#xA;4．含五金配件、消防救援标识、可开启扇设置限位器、增加防脱落铰链或其他防脱措施由门窗厂家提供" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="459.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="138" Qdbm="WB010801008001" Mc="五金安装" Xmtz="1．手动开启装置" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="83.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="139" Qdbm="010807003001" Mc="成品铝合金防雨百页窗" Xmtz="1．窗名称：成品隔热铝合金防雨百页窗&#xA;2．窗材质：1.5mm厚铝合金百叶&#xD;&#xA;3．表面粉末喷涂，含防鼠防虫网" Gcnr="" Jsgz="" Dw="m2" Sl="72.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="140" Qdbm="010807003002" Mc="纱窗" Xmtz="1．窗材质：防虫纱窗" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="286.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="141" Qdbm="010808001001" Mc="防火卷帘门门套" Xmtz="1．面层材料品种、规格：12mm厚双层防火板面层，无机涂料面层(两底两面）&#xD;&#xA;2．50*100x3、50*100*3镀锌方管骨架，缝隙采用防火岩棉填塞&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以展开面积计算" Dw="m2" Sl="9.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0109" Mc="屋面及防水工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="142" Qdbm="010902003001" Mc="屋面刚性层" Xmtz="1．刚性层厚度：40厚C25配筋细石混凝土(掺减水剂,) &#xD;&#xA;2．钢筋规格、型号：双向配Φ6@150,每6米设缝,密封胶嵌缝" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6385.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="143" Qdbm="WB010902005003" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层做法：10厚低强度等级砂浆隔离层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6385.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="144" Qdbm="010902001002" Mc="屋面卷材防水" Xmtz="1．卷材品种、规格、厚度：1.5mm厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6600.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="145" Qdbm="WB010902005004" Mc="屋面找平层 " Xmtz="1．找平层厚度、砂浆配合比：20厚1:3水泥砂浆找平（掺入聚丙烯）" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6385.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="146" Qdbm="011001001001" Mc="保温隔热屋面" Xmtz="1．保温隔热材料品种、规格、厚度：70厚高密度挤塑聚苯板(B1级)" Gcnr="" Jsgz="1.按设计图示尺寸，以面积计算2.按设计图示尺寸，以体积计算" Dw="m2" Sl="6385.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="147" Qdbm="010902002001" Mc="屋面涂膜防水" Xmtz="1．防水膜品种：2厚聚合物水泥基防水涂料一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6600.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="148" Qdbm="010902001003" Mc="屋面卷材防水" Xmtz="1．卷材品种、规格、厚度：1.5mm厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="50.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="149" Qdbm="WB010902005005" Mc="屋面找平层 " Xmtz="1．找平层厚度、砂浆配合比：20厚1:3水泥砂浆找平（掺入聚丙烯）" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="50.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="150" Qdbm="011001001002" Mc="保温隔热屋面" Xmtz="1．保温隔热材料品种、规格、厚度：70厚高密度挤塑聚苯板(B1级)" Gcnr="" Jsgz="1.按设计图示尺寸，以面积计算2.按设计图示尺寸，以体积计算" Dw="m2" Sl="50.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="151" Qdbm="010902002002" Mc="屋面涂膜防水" Xmtz="1．防水膜品种：2厚聚合物水泥基防水涂料一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="50.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="152" Qdbm="011201001001" Mc="墙面一般抹灰" Xmtz="1．部位：外墙面&#xD;&#xA;2．底层厚度、砂浆配合比：5mm厚聚合物水泥防水砂浆" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4491.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="153" Qdbm="010903002001" Mc="墙面涂膜防水" Xmtz="1．部位：外墙面&#xD;&#xA;2．涂膜厚度、遍数：2mm厚聚合物水泥防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4491.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="154" Qdbm="010904002002" Mc="楼（地）面涂膜防水" Xmtz="1．部位：卫生间楼地面&#xD;&#xA;2．涂膜厚度、遍数：1.5mm厚聚氨酯防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="224.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="155" Qdbm="010904002003" Mc="楼（地）面涂膜防水" Xmtz="1．部位：卫生间楼地面&#xD;&#xA;2．涂膜厚度、遍数：2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="224.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="156" Qdbm="010903002002" Mc="墙面涂膜防水" Xmtz="1．部位：卫生间墙面&#xD;&#xA;2．涂膜厚度、遍数：1.5厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="995.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="157" Qdbm="010903002003" Mc="天棚涂膜防水" Xmtz="1．部位：卫生间天棚&#xD;&#xA;2．涂膜厚度、遍数：1.2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="293.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="158" Qdbm="010904002004" Mc="楼（地）面涂膜防水" Xmtz="1．部位：用于报警阀间等无腐蚀性普通室内排水沟&#xD;&#xA;2．涂膜厚度、遍数：1.5厚水性聚合物沥青类防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="8.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="159" Qdbm="010904003001" Mc="楼（地）面砂浆防水（防潮）" Xmtz="1．部位：用于报警阀间等无腐蚀性普通室内排水沟&#xD;&#xA;2．防水层做法：1:2聚合物防水砂浆0.5%纵向找坡,最薄处20厚" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="8.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="160" Qdbm="010904002005" Mc="楼（地）面涂膜防水" Xmtz="1．部位：雨棚&#xD;&#xA;2．涂膜厚度、遍数：2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="5.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="161" Qdbm="010904003002" Mc="楼（地）面砂浆防水（防潮）" Xmtz="1．部位：雨棚&#xD;&#xA;2．防水层做法：20厚1:2.5防水砂浆" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="5.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="162" Qdbm="011101006001" Mc="水泥砂浆楼地面找平层 " Xmtz="1．部位：电梯基坑、沉淀池、提升基坑、漏液收集坑、电缆井等底板&#xD;&#xA;2．找平层厚度、砂浆配合比：20厚DS M15砂浆(1:3水泥砂浆)找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="88.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="163" Qdbm="010904001001" Mc="楼（地）面卷材防水" Xmtz="1．部位：电梯基坑、沉淀池、提升基坑、漏液收集坑、电缆井等底板&#xD;&#xA;2．卷材品种、规格、厚度：1.5厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="88.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="164" Qdbm="WB011101007001" Mc="细石混凝土找平层 " Xmtz="1．部位：电梯基坑、沉淀池、提升基坑、漏液收集坑、电缆井等底板&#xD;&#xA;2．找平层厚度、混凝土强度等级：50厚C20细石砼保护层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="88.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="165" Qdbm="010903003001" Mc="墙面砂浆防水（防潮）" Xmtz="1．部位：电梯基坑、沉淀池、提升基坑、漏液收集坑、电缆井等侧壁&#xD;&#xA;2．防水层做法：20厚DS M15砂浆(1:3水泥砂浆)找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="194.57" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="166" Qdbm="010903001001" Mc="墙面卷材防水" Xmtz="1．部位：电梯基坑、沉淀池、提升基坑、漏液收集坑、电缆井等侧壁&#xD;&#xA;2．卷材品种、规格、厚度：1.5厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="194.57" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="167" Qdbm="010903005001" Mc="墙面防水保护层" Xmtz="1．部位：电梯基坑、沉淀池、提升基坑、漏液收集坑、电缆井等侧壁&#xD;&#xA;2．保护层品种、规格、厚度：30厚挤塑聚苯板保护层,用建筑胶粘贴&#xD;&#xA;3．DP M15砂浆局部找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="194.57" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="168" Qdbm="010904004001" Mc="楼（地）面变形缝" Xmtz="1．嵌缝材料种类：硬质岩棉填缝,厚度200,外面弹性防火材料封堵&#xD;&#xA;2．止水带材料种类：1.5厚三元乙丙防水卷材&#xD;&#xA;3．盖缝材料：6厚不锈钢板，角钢L70x45x4，PU橡胶" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="170.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="169" Qdbm="010903004001" Mc="外墙面变形缝" Xmtz="1．嵌缝材料种类：内填岩棉&#xD;&#xA;2．止水带材料种类：橡胶止水带&#xD;&#xA;3．盖缝材料：0.6厚镀铝锌彩钢板" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="72.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="170" Qdbm="010904004002" Mc="顶棚变形缝" Xmtz="1．盖缝材料：1厚铝合金盖板&#xD;&#xA;2．防护材料种类：1.5厚镀锌钢板承托板，膨胀螺栓，弹性胶条，铝锚夹" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="160.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="171" Qdbm="ZB010902008001" Mc="屋面变形缝" Xmtz="1．嵌缝材料种类：内填岩棉，聚乙烯泡沬塑料棒&#xD;&#xA;2．盖缝材料：1厚铝合金盖板，1厚铝合金盖板" Gcnr="" Jsgz="按设计图示以长度计算。" Dw="m" Sl="50.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="172" Qdbm="010904004003" Mc="楼（地）面变形缝" Xmtz="1．部位：楼梯滑动支座&#xD;&#xA;2．嵌缝材料种类：缝宽50mm聚苯板填充、钢板之间满铺石墨粉" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="36.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0110" Mc="保温、隔热、防腐工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="173" Qdbm="011001003001" Mc="保温隔热墙面" Xmtz="1．保温隔热部位：外墙面&#xD;&#xA;2．保温隔热材料品种、规格及厚度：50厚岩棉板&#xD;&#xA;3．增强网及抗裂防水砂浆种类：5厚聚合物抗裂砂浆，热镀锌钢网丝&#xD;&#xA;4．锚栓固定（锚栓数量不应小于 6 个/m2。在墙面阴、阳角等部位应适当增加锚栓数量）&#xD;&#xA;5．岩棉板外保温系统参图集10J121第附录3-1~附录3-9页执行" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2956.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0111" Mc="楼地面装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="174" Qdbm="WB010101007001" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="7300.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="175" Qdbm="010404001002" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="2190.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="176" Qdbm="010404001003" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="730.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="177" Qdbm="WB010902005006" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层做法：0.5厚双层PE膜" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="7300.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="178" Qdbm="011101003001" Mc="混凝土楼地面 " Xmtz="1．面层厚度、混凝土强度等级：200厚C30钢筋混凝土抹平(内配φ10@150双层双向钢筋)" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="7300.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="179" Qdbm="WB010101007002" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="95.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="180" Qdbm="010404001004" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="28.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="181" Qdbm="010404001005" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="9.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="182" Qdbm="WB011101007002" Mc="细石混凝土找平层 " Xmtz="1．找平层厚度、混凝土强度等级：最薄处30厚C20细石混凝土找坡层,向地漏找1%坡,随打随抹平。地漏四周及管根部用DS M15砂浆抹小八角字&#xD;&#xA;2．界面剂一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="95.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="183" Qdbm="011102003001" Mc="块料楼地面" Xmtz="1．面层材料品种、规格、颜色：5~10mm厚600x600mm防滑地砖，DTG砂浆擦缝&#xD;&#xA;2．结合层厚度、砂浆配合比或粘接剂种类：20厚1:3干硬性水泥砂浆结合层,表面撒水泥粉&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="95.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="184" Qdbm="WB011101007003" Mc="细石混凝土找平层 " Xmtz="1．找平层厚度、混凝土强度等级：最薄处30厚C20细石混凝土找坡层,向地漏找1%坡,随打随抹平。地漏四周及管根部用DS M15砂浆抹小八角字&#xD;&#xA;2．界面剂一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="128.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="185" Qdbm="011102003002" Mc="块料楼地面" Xmtz="1．面层材料品种、规格、颜色：5~10mm厚600x600mm防滑地砖，DTG砂浆擦缝&#xD;&#xA;2．结合层厚度、砂浆配合比或粘接剂种类：20厚1:3干硬性水泥砂浆结合层,表面撒水泥粉&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="128.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0112" Mc="墙、柱面装饰与隔断、幕墙工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="186" Qdbm="011201001002" Mc="墙面一般抹灰" Xmtz="1．部位：砖胎膜&#xD;&#xA;2．底层厚度、砂浆配合比：20厚1:2.5水泥砂浆" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="248.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="187" Qdbm="011201001003" Mc="墙面一般抹灰" Xmtz="1．部位：外墙面1&#xD;&#xA;2．底层厚度、砂浆配合比：10厚1:3水泥砂浆找平(加5%防水剂)&#xD;&#xA;3．专用砂浆或界面剂一道甩毛&#xD;&#xA;4．水泥砂浆中加入杜拉纤维,增强抗裂性能" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4491.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="188" Qdbm="011201001004" Mc="墙面一般抹灰" Xmtz="1．部位：内墙面3&#xD;&#xA;2．挂金属网,8厚DP M20(1:2.5水泥砂浆)压实抹平&#xD;&#xA;3．底层厚度、砂浆配合比：6厚DP M5砂浆(1:1:6水泥石灰膏砂浆)打底扫毛或划出纹道 &#xD;&#xA;4．界面剂一道&#xD;&#xA;5．用修补砂浆局部修补墙面,DP砂浆勾实接缝并拉毛" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1009.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="189" Qdbm="011204003001" Mc="块料墙面" Xmtz="1．部位：卫生间墙面&#xD;&#xA;2．面层材料品种、规格、品牌、颜色：10厚300*600陶瓷墙砖&#xD;&#xA;3．结合层材料种类：5厚DTA砂浆&#xD;&#xA;4．缝宽、嵌缝材料种类：白水泥擦缝 " Gcnr="" Jsgz="按设计图示尺寸，以镶贴表面积计算" Dw="m2" Sl="1009.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="190" Qdbm="WB011207002001" Mc="轻钢龙骨隔墙" Xmtz="1．龙骨材料种类、规格、中距：75系列轻钢龙骨纤维增强硅酸钙墙&#xD;&#xA;2．8厚防火硅酸钙板+C75轻钢龙骨,内填75厚岩棉(容重≥100kg/m3)+8厚防火硅酸钙板&#xD;&#xA;3．应通过消防测试,耐火极限不小于2.00h。墙体做法参07J905-1《防火墙建筑构造(一)》第11页墙12&#xD;&#xA;4．隔墙高度5~6米参图集13J502-1 A13，14页，控制龙骨壁厚1.0mm、龙骨间距300mm、变形量L/240,压强值240Pa。8米高隔墙可4米一道增加75x50x1.0方钢加强，厂家深化图纸后设计确认后方可施工，加强构造等相关费用已包含在内，投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="按设计图示尺寸，以展开面积计算" Dw="m2" Sl="2795.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="191" Qdbm="WB011207002002" Mc="成品抗爆板抗爆墙" Xmtz="1．成品抗爆板抗爆墙&#xD;&#xA;2．构造做法参14J938-C2-C6页，选用KBQ2构造做法&#xD;&#xA;3．需专业厂家深化设计确认，投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="按设计图示尺寸，以展开面积计算" Dw="m2" Sl="115.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0113" Mc="天棚工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="192" Qdbm="011301001001" Mc="天棚清理" Xmtz="1．板底原浆抹平，表面清扫干净" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="37125.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="193" Qdbm="011301001002" Mc="天棚抹灰" Xmtz="1．部位：混凝土雨棚&#xD;&#xA;2．抹灰厚度、材料种类：7厚水泥纸筋石灰砂浆打底，5厚水泥细纸筋石灰粉面" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="4.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="194" Qdbm="WB011302005001" Mc="铝合金方板扣板吊顶" Xmtz="1．部位：吊顶2&#xD;&#xA;2．面层材料品种、规格：0.8mm铝合金方板600*600mm&#xD;&#xA;3．龙骨：与安装型式配套的专用上层主龙骨,间距≤1200用吊件与钢筋吊杆联结后找平 ，与铝合金方板配套的专用下层副龙骨联结,间距≤600 &#xD;&#xA;4．吊顶形式、吊杆规格、高度：Φ6钢筋吊杆,双向中距≤1200,吊杆上部与预留钢筋吊环固定&#xD;&#xA;5．板内预留Φ8钢筋吊环双向中距≤1200;" Gcnr="" Jsgz="按设计图示尺寸以展开面积计算" Dw="m2" Sl="224.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="195" Qdbm="WB011302005002" Mc="抗暴吊顶" Xmtz="1．部位：电解液暂存间&#xD;&#xA;2．面层材料品种、规格：2400*1200*9.5厚纤维水泥复合钢板&#xD;&#xA;3．配套槽钢抗爆龙骨、专用高强吊杆、化学锚栓固定，防火密封接缝，含制作安装、辅材等&#xD;&#xA;4．参图集14J938 E2 1做法，需专业厂家深化设计确认，投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="按设计图示尺寸以展开面积计算" Dw="m2" Sl="21.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0114" Mc="油漆、涂料、裱糊工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="196" Qdbm="WB011406001001" Mc="外墙涂料" Xmtz="1．部位：外墙（含栏板、节点及外立面水管等）&#xD;&#xA;2．基层类型：外墙耐水腻子2道, 打磨平整&#xD;&#xA;3．油漆品种、刷漆遍数：外墙涂料饰面（一底两面，罩面漆一遍）" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4491.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0115" Mc="其他装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="197" Qdbm="011503001001" Mc="楼梯栏杆" Xmtz="1．部位：楼梯栏杆&#xD;&#xA;2．高度：900mm&#xD;&#xA;3．做法：φ51*3不锈钢管立柱，φ63*1.5不锈钢管扶手，φ25*1.0不锈钢管立杆，φ38*1.0不锈钢管横杆&#xD;&#xA;4．201不锈钢法兰，预埋件见22J403-1  M3/5-19" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="88.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="198" Qdbm="011503001002" Mc="楼梯护窗栏杆" Xmtz="1．部位：楼梯护窗栏杆&#xD;&#xA;2．高度：700mm&#xD;&#xA;3．做法：φ51*3不锈钢管立柱，φ63*1.5不锈钢管扶手，φ25*1.0不锈钢管立杆，φ38*1.0不锈钢管横杆&#xD;&#xA;4．201不锈钢法兰，预埋件见22J403-1  M3/5-19" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="2.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="199" Qdbm="011503001003" Mc="楼梯护窗栏杆" Xmtz="1．部位：楼梯护窗栏杆&#xD;&#xA;2．高度：1004mm&#xD;&#xA;3．做法：φ51*3不锈钢管立柱，φ63*1.5不锈钢管扶手，φ25*1.0不锈钢管立杆，φ38*1.0不锈钢管横杆&#xD;&#xA;4．201不锈钢法兰，预埋件见22J403-1  M3/5-19" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="3.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="200" Qdbm="011503001004" Mc="楼梯护窗、平台栏杆" Xmtz="1．部位：楼梯护窗、平台栏杆&#xD;&#xA;2．高度：1100mm&#xD;&#xA;3．做法：φ51*3不锈钢管立柱，φ63*1.5不锈钢管扶手，φ25*1.0不锈钢管立杆，φ38*1.0不锈钢管横杆&#xD;&#xA;4．201不锈钢法兰，预埋件见22J403-1  M3/5-19" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="12.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="201" Qdbm="011503001005" Mc="活动栏杆" Xmtz="1．部位：活动栏杆&#xD;&#xA;2．高度：1100mm&#xD;&#xA;3．扶手材料种类、规格、品牌：φ50x2.5不锈钢管&#xD;&#xA;4．栏杆材料种类、规格、品牌：φ25x1.5不锈钢管&#xD;&#xA;5．固定配件种类：预埋套管φ60*2.5不锈钢焊接预埋铁件-200*100*6" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="10.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="202" Qdbm="011503001006" Mc="可拆卸式不锈钢防护栏杆" Xmtz="1．部位：吊装口卷帘门&#xD;&#xA;2．高度：1100mm&#xD;&#xA;3．扶手材料种类、规格、品牌：φ50x1.5不锈钢管&#xD;&#xA;4．栏杆材料种类、规格、品牌：φ50x1.5不锈钢管立柱，φ30*1.5不锈钢管立杆&#xD;&#xA;5．固定配件种类：不锈钢防护栏套管φ80*2.0" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="38.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="203" Qdbm="011503001007" Mc="吊装口防护栏" Xmtz="1．部位：吊装口卷帘门上口100mm&#xD;&#xA;2．扶手材料种类、规格、品牌：DN60*3防撞栏，黑黄色警示漆&#xD;&#xA;" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="28.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="204" Qdbm="040205017001" Mc="防撞柱" Xmtz="1．部位：室内防撞柱&#xD;&#xA;2．高度：高出地面1200mm&#xD;&#xA;3．规格、型号：φ150*3钢管，外刷黄黑漆（两遍）&#xD;&#xA;4．柱脚C25砼浇筑，预埋300*300*8钢板，M16*150膨胀螺栓固定" Gcnr="" Jsgz="" Dw="个" Sl="42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="205" Qdbm="040205017002" Mc="防撞柱" Xmtz="1．部位：室外防撞柱&#xD;&#xA;2．高度：高出地面1200mm&#xD;&#xA;3．规格、型号：φ150*3钢管，外刷黄黑漆（两遍）&#xD;&#xA;4．柱脚C25砼浇筑，预埋400*400*8钢板，φ12钢筋焊接固定" Gcnr="" Jsgz="" Dw="个" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="206" Qdbm="011503001008" Mc="防撞带" Xmtz="1．部位：室内防撞带&#xD;&#xA;2．高度：300mm&#xD;&#xA;3．规格、型号：防撞钢管φ50*3，表面刷黄黑相间警示漆&#xD;&#xA;4．8厚钢板，M16*150螺栓固定表面刷黄色漆" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="6.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="207" Qdbm="011503001009" Mc="防撞带" Xmtz="1．部位：室外防撞带&#xD;&#xA;2．高度：300mm&#xD;&#xA;3．规格、型号：防撞钢管φ100*3，表面刷黄黑相间警示漆&#xD;&#xA;4．8厚200*200、400*200镀锌钢板，M16*150螺栓固定表面刷黄色漆" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="101.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="208" Qdbm="ZB010101001001" Mc="排水沟盖板" Xmtz="1．材料种类：50mm厚不锈钢格栅盖板&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m2" Sl="17.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="209" Qdbm="ZB010101001002" Mc="排水沟盖板" Xmtz="1．材料种类：50mm厚成品镀锌花纹钢板盖板&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m2" Sl="2.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="210" Qdbm="ZB010101001003" Mc="沉淀池盖板" Xmtz="1．材料种类：1.2厚不锈钢盖板&#xD;&#xA;2．平时上锁管理/50热浸镀锌钢方通" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m2" Sl="2.63" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="211" Qdbm="ZB010101001004" Mc="线性截水槽" Xmtz="1．部位：吊装口&#xD;&#xA;2．规格、材质：1厚304#不锈钢u型槽" Gcnr="" Jsgz="" Dw="m" Sl="27.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="212" Qdbm="ZB010101001005" Mc="排水沟内衬板" Xmtz="1．部位：溶剂房、溶液房、清洗房、电解液存放间等有腐蚀性液体房排水沟&#xD;&#xA;2．沟三面内衬0.8mm不锈钢&#xD;&#xA;3．内衬不锈钢使用螺栓或焊接进行固定,对焊接接头进行清理、打磨,确保其表面光亮洁净。然后涂抹焊接胶。" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m2" Sl="31.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="213" Qdbm="WB011209008001" Mc="铝板压顶" Xmtz="1．部位：屋面女儿墙&#xD;&#xA;2．金属板材品种、规格、颜色：3mm厚铝板&#xD;&#xA;3．嵌缝材料:泡沫棒、硅酮耐候胶" Gcnr="" Jsgz="按设计图示尺寸，以展开面积计算" Dw="m2" Sl="281.63" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="214" Qdbm="040205019001" Mc="成品塑胶缓冲垫" Xmtz="1．部位：吊装口&#xD;&#xA;2．材料品种：成品塑胶缓冲垫,凸出外墙50&#xD;&#xA;3．规格、型号：350宽塑胶缓冲垫（可用道路减速带制作）&#xD;&#xA;4．1.0mm厚铝板(成品)泛水件密封胶封严水泥钉或射钉@500镀锌垫片20x20x0.7" Gcnr="" Jsgz="按设计图示以长度计算" Dw="m" Sl="30.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="215" Qdbm="ZB010101001006" Mc="挡鼠板" Xmtz="1．名称：挡鼠板&#xD;&#xA;2．12厚防火木板,h=600mm，卡槽(6厚扁钢)高600mm,预埋件参06J403-1 M2/161" Gcnr="" Jsgz="" Dw="m2" Sl="4.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="216" Qdbm="011505001001" Mc="大便蹲位" Xmtz="1．部位：大便蹲位&#xD;&#xA;2．做法参16J914-1页XT18节点1" Gcnr="" Jsgz="按设计图示尺寸，以台面展开面积计算，不扣除孔洞、挖弯、削角所占面积" Dw="m2" Sl="63.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="217" Qdbm="011210005001" Mc="成品隔断" Xmtz="1．部位：卫生间隔断、小便斗隔断&#xD;&#xA;2．隔断材料品种、规格、颜色：32mm厚复合树脂板隔断&#xD;&#xA;3．配件品种、规格：含合页、配套显示门锁&#xD;&#xA;4．参16J914-1页XT9" Gcnr="" Jsgz="按设计图示框外围尺寸，以面积计算" Dw="m2" Sl="287.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="218" Qdbm="011505001002" Mc="洗漱台" Xmtz="1．柜体规格：20mm人造大理石台面台面&#xD;&#xA;2．五金种类、规格：包含五金等&#xD;&#xA;3．参16J914-1页XT12相关做法" Gcnr="" Jsgz="按设计图示尺寸，以台面展开面积计算，不扣除孔洞、挖弯、削角所占面积" Dw="m2" Sl="5.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="219" Qdbm="011505010001" Mc="镜面玻璃(卫生间）" Xmtz="1．镜面玻璃品种、规格：5mm镀铝膜银镜面镜&#xD;&#xA;2．高1200mm，镜底距地1200mm,黑色拉丝不锈钢窄边框，安装做法参16J914-1页3/XT25" Gcnr="" Jsgz="" Dw="m2" Sl="10.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="220" Qdbm="011505008001" Mc="卫生纸盒" Xmtz="1．成品不锈钢卫生纸盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="221" Qdbm="ZB010101001007" Mc="溢流口" Xmtz="1．名称：溢水口" Gcnr="" Jsgz="" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="222" Qdbm="ZB010101001008" Mc="簸箕" Xmtz="1．规格、材质：500x500x40mmC20细石混凝土板配6@100X100" Gcnr="" Jsgz="" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="223" Qdbm="ZB010101001009" Mc="电梯召唤盒预留洞" Xmtz="1．电梯召唤盒预留洞" Gcnr="" Jsgz="" Dw="个" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="224" Qdbm="ZB010101001010" Mc="电梯吊钩" Xmtz="1．电梯吊钩" Gcnr="" Jsgz="" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="225" Qdbm="ZB010101001011" Mc="屋面出入口" Xmtz="1．部位：屋面出入口&#xD;&#xA;2．C25混凝土踏步&#xD;&#xA;3．20mm厚1:2防水水泥砂浆粉刷" Gcnr="" Jsgz="" Dw="m2" Sl="1.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="226" Qdbm="ZB010101001012" Mc="电梯口包边" Xmtz="1．部位：电梯口包边&#xD;&#xA;2．10厚光面钢板,面层包1.4不锈钢板&#xD;&#xA;3．6#槽钢骨架@300，膨胀螺丝固定" Gcnr="" Jsgz="" Dw="m2" Sl="12.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="227" Qdbm="ZB010101001013" Mc="防火封堵" Xmtz="1．名称：墙体防火封堵节点一&#xD;&#xA;2．部位：配电房、消控室、楼梯间、弱电间、送排风机房等有防火需求设备用房间&#xD;&#xA;3．材料种类：9厚纤维增强硅酸盐板75厚岩棉9厚纤维增强硅酸盐板&#xD;&#xA;4．附加龙骨，防火岩棉封填密实，50X50镀锌钢板角件，密封膏" Gcnr="" Jsgz="" Dw="m2" Sl="490.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="228" Qdbm="ZB010101001014" Mc="防火封堵" Xmtz="1．名称：墙体防火封堵节点二&#xD;&#xA;2．部位：配电房、消控室、楼梯间、弱电间、送排风机房等有防火需求设备用房间&#xD;&#xA;3．材料种类：9厚纤维增强硅酸盐板75厚岩棉9厚纤维增强硅酸盐板&#xD;&#xA;4．附加龙骨，防火岩棉封填密实，金属盖缝板，密封膏" Gcnr="" Jsgz="" Dw="m2" Sl="20.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="229" Qdbm="WB010902006001" Mc="屋面排气管" Xmtz="1．排气管品种、规格:中50镀锌钢管排期管23页&#xD;&#xA;2．4厚钢板环与钢管焊接&#xD;&#xA;3．参12J201第A21" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="355" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0117" Mc="措施项目" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="230" Qdbm="WB011701010001" Mc="单层轻钢厂房脚手架" Xmtz="1．搭设部位：部位：梁柱、屋面板等水平结构&#xD;&#xA;2．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="1.柱梁、屋面瓦等水平结构安装按厂房水平投影面积计算2.墙板、门窗、雨篷等竖向结构按厂房垂直投影面积计算" Dw="m2" Sl="1425.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="231" Qdbm="WB011701010002" Mc="单层轻钢厂房脚手架" Xmtz="1．搭设部位：墙板、门窗、雨篷等竖向结构&#xD;&#xA;2．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="1.柱梁、屋面瓦等水平结构安装按厂房水平投影面积计算2.墙板、门窗、雨篷等竖向结构按厂房垂直投影面积计算" Dw="m2" Sl="7211.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="232" Qdbm="011701002001" Mc="外脚手架" Xmtz="1．搭设方式：外脚手架（含电梯井）&#xA;2．脚手架材质：钢管脚手架&#xD;&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="8753.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="233" Qdbm="011701003001" Mc="里脚手架" Xmtz="1．搭设方式：内墙砌筑脚手架&#xA;2．脚手架材质：钢管脚手架&#xD;&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="3287.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="234" Qdbm="011701006001" Mc="装饰满堂脚手架" Xmtz="1．搭设方式：装饰满堂脚手架&#xA;2．脚手架材质：钢管脚手架&#xD;&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="21.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="235" Qdbm="011702001001" Mc="基础垫层-模板" Xmtz="1．基础类型：基础垫层&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="324.32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="236" Qdbm="011702001002" Mc="基础-模板" Xmtz="1．基础类型：桩承台基础&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1393.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="237" Qdbm="011702001003" Mc="基础-模板" Xmtz="1．基础类型：筏板基础&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="60.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="238" Qdbm="011702001004" Mc="设备基础" Xmtz="1．基础类型：设备基础&#xD;&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="35.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="239" Qdbm="011702002001" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：1.6m以内&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="648.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="240" Qdbm="011702002002" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：2.4m以内&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1821.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="241" Qdbm="011702002003" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：2.4m以外&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="4295.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="242" Qdbm="011702003001" Mc="构造柱-模板" Xmtz="1．构造柱模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="824.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="243" Qdbm="011702005001" Mc="基础梁" Xmtz="1．基础梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="792.87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="244" Qdbm="011702006001" Mc="矩形梁" Xmtz="1．矩形梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="260.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="245" Qdbm="011702008001" Mc="圈梁-模板" Xmtz="1．圈梁、反坎等模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1236.91" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="246" Qdbm="011702009001" Mc="过梁-模板" Xmtz="1．过梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="31.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="247" Qdbm="011702011001" Mc="直形墙-模板" Xmtz="1．地下直行墙等模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="126.67" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="248" Qdbm="011702013001" Mc="短肢剪力墙、电梯井壁" Xmtz="1．电梯井墙等模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="72.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="249" Qdbm="011702014001" Mc="有梁板" Xmtz="1．有梁板模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="40053.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="250" Qdbm="011702016001" Mc="平板" Xmtz="1．平板模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="4.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="251" Qdbm="011702021001" Mc="栏板" Xmtz="1．栏板模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1202.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="252" Qdbm="011702022001" Mc="天沟、挑檐" Xmtz="1．天沟、挑檐模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="478.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="253" Qdbm="011702023001" Mc="雨篷、悬挑板、阳台板" Xmtz="1．雨棚模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按设计图示尺寸，以外挑部分水平投影面积计算" Dw="m2" Sl="9.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="254" Qdbm="011702024001" Mc="楼梯" Xmtz="1．楼梯模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按楼梯（包括休息平台、水平梁、斜梁和楼层板的连接梁）的水平投影面积计算" Dw="m2" Sl="140.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="255" Qdbm="011702026001" Mc="电缆沟、地沟" Xmtz="1．排水沟等板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="46.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="256" Qdbm="WB011702039001" Mc="压顶-模板" Xmtz="1．压顶模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="36.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="257" Qdbm="WB011702044001" Mc="后浇混凝土-模板" Xmtz="1．后浇带基础梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇砼接触面积计算" Dw="m2" Sl="8.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="258" Qdbm="WB011702044002" Mc="后浇混凝土-模板" Xmtz="1．后浇带梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇砼接触面积计算" Dw="m2" Sl="214.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="259" Qdbm="WB011702044003" Mc="后浇混凝土-模板" Xmtz="1．后浇带板模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇砼接触面积计算" Dw="m2" Sl="362.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="260" Qdbm="WB011702030001" Mc="柱支模超高" Xmtz="1．柱支模超高&#xD;&#xA;2．模板及支架的制作、安装、拆除、整理堆放、场内外运输、清理模板粘结物、杂物、刷隔离剂等一切费用，投标人综合考虑自行报价，中标后不予调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="5115.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="261" Qdbm="WB011702031001" Mc="梁支模超高" Xmtz="1．梁支模超高&#xD;&#xA;2．模板及支架的制作、安装、拆除、整理堆放、场内外运输、清理模板粘结物、杂物、刷隔离剂等一切费用，投标人综合考虑自行报价，中标后不予调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="856.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="262" Qdbm="WB011702033001" Mc="板支模超高" Xmtz="1．板支模超高&#xD;&#xA;2．模板及支架的制作、安装、拆除、整理堆放、场内外运输、清理模板粘结物、杂物、刷隔离剂等一切费用，投标人综合考虑自行报价，中标后不予调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="87170.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="263" Qdbm="WB011702032001" Mc="高大支模增加费" Xmtz="1．有梁板高大模板增加费&#xD;&#xA;2．按水平投影面计算&#xD;&#xA;3．包括支撑硬化、高支模设计、制定并通过专项方案论证、按照方案施工、安全监测等所有费用，投标人自行考虑投标报价，结算是不予调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="7694.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="264" Qdbm="011703001001" Mc="建筑垂直运输" Xmtz="1．层数：多层厂房&#xA;2．建筑物建筑类型及结构形式：框架结构&#xA;3．建筑物檐口高度、层数：23.55m&#xD;&#xA;" Gcnr="" Jsgz="1.建筑物地下室部分垂直运输按设计室内地坪(±0.00)以下的建筑面积，以面积计算2.建筑物上部建筑部分垂直运输按室内地坪(±0.00)以上的建筑面积总和，以面积计算" Dw="m2" Sl="27397.32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="265" Qdbm="011704001001" Mc="建筑超高施工增加" Xmtz="1．建筑物建筑类型及结构形式：框架+钢结构&#xD;&#xA;2．建筑物檐口高度、层数：23.6m、4层" Gcnr="" Jsgz="按建筑面积计算" Dw="m2" Sl="3332.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="266" Qdbm="011705001001" Mc="大型机械设备进出场及安拆" Xmtz="1．机械设备名称：打桩机、挖掘机、起重机、施工电梯、预拌砂浆罐式搅拌机等机械含基础等、投标人自行根据施工方案考虑、综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按使用机械设备的数量计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="00002" Dwgcmc="厂房三（安装）" Zylb="1" Jzmj="27397.32" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B9767C6F3B122686496A" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="1.1" Mc="配电箱、柜" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="030404017001" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="030404017002" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-102&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="030404017003" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-103&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="030404017004" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-104&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="5" Qdbm="030404017005" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-201&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="030404017006" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-301&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="030404017007" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MP-F3-401&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="030404017008" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EAP-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="030404017009" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EAP-F3-201&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="030404017010" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EMCC-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="030404017011" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EMCC-F3-R01&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="030404017012" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MCC-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="030404017013" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MCC-F3-102&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="030404017014" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MCC-F3-201&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="030404017015" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MCC-F3-301&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="030404017016" Mc="配电箱" Xmtz="1、名称：厂房三配电箱MCC-F3-401&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="030404017017" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AT-F3-401&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="18" Qdbm="030404017018" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AT-F3-402&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="030404017019" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AT-F3-403&#xD;&#xA;2、型号：箱体参考尺寸:800Wx1000Hx250D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="030404017020" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="030404017021" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-102&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="030404017022" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-201&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="030404017023" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-202&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="030404017024" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-301&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="030404017025" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-302&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="030404017026" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-401&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="030404017027" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AL-F3-402&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="030404017028" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AR-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="030404017029" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AR-F3-102&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="030404017030" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AR-F3-201&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="030404017031" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AR-F3-301&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="030404017032" Mc="配电箱" Xmtz="1、名称：厂房三配电箱AR-F3-401&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="030404017033" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EAL-F3-101&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="030404017034" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EAL-F3-201&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="030404017035" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EAL-F3-301&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="030404017036" Mc="配电箱" Xmtz="1、名称：厂房三配电箱EAL-F3-401&#xD;&#xA;2、型号：箱体参考尺寸:500Wx600Hx200D，具体尺寸以盘柜厂深化为准&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="37" Qdbm="WB030904012001" Mc="A型应急照明集中电源" Xmtz="1、名称：厂房三应急照明集中电源EAL-F3-101A&#xD;&#xA;2、规格：非标 &#xD;&#xA;3、安装方式：壁挂&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="WB030904012002" Mc="A型应急照明集中电源" Xmtz="1、名称：厂房三应急照明集中电源EAL-F3-102A&#xD;&#xA;2、规格：非标 &#xD;&#xA;3、安装方式：壁挂&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="WB030904012003" Mc="A型应急照明集中电源" Xmtz="1、名称：厂房三应急照明集中电源EAL-F3-201A&#xD;&#xA;2、规格：非标 &#xD;&#xA;3、安装方式：壁挂&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="WB030904012004" Mc="A型应急照明集中电源" Xmtz="1、名称：厂房三应急照明集中电源EAL-F3-301A&#xD;&#xA;2、规格：非标 &#xD;&#xA;3、安装方式：壁挂&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="WB030904012005" Mc="A型应急照明集中电源" Xmtz="1、名称：厂房三应急照明集中电源EAL-F3-401A&#xD;&#xA;2、规格：非标 &#xD;&#xA;3、安装方式：壁挂&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="030404017037" Mc="配电箱" Xmtz="1．名称：防火卷帘控制箱（设备自带，仅计安装费）&#xD;&#xA;2．安装方式：明装&#xD;&#xA;3．成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="030404017038" Mc="配电箱" Xmtz="1．名称：防爆卷帘门控制箱（设备自带，仅计安装费）&#xD;&#xA;2．安装方式：明装&#xD;&#xA;3．成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="030404017039" Mc="配电箱" Xmtz="1、名称：沉淀池水泵控制箱（设备自带，仅计安装费）&#xD;&#xA;2、安装方式：明装&#xD;&#xA;3、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="030404017040" Mc="配电箱" Xmtz="1、名称：消防空压机控制箱（设备自带，仅计安装费）&#xD;&#xA;2、安装方式：明装&#xD;&#xA;3、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="030404017041" Mc="配电箱" Xmtz="1、名称：稳压泵控制箱（设备自带，仅计安装费）&#xD;&#xA;2、安装方式：明装&#xD;&#xA;3、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="030404017042" Mc="配电箱" Xmtz="1、名称：电梯控制箱（设备自带，仅计安装费）&#xD;&#xA;2、安装方式：明装&#xD;&#xA;3、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="030414002001" Mc="送配电装置系统" Xmtz="1、名称：送配电装置系统调试&#xD;&#xA;2、电压等级（KV)：1KV以下&#xD;&#xA;" Gcnr="" Jsgz="按设计图示系统计算" Dw="系统" Sl="14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="030414004001" Mc="自动投入装置" Xmtz="1、名称：自动切换电源系统调试&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="系统（台、套）" Sl="8.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.2" Mc="照明灯具、开关插座" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="50" Qdbm="030412005001" Mc="荧光灯" Xmtz="1、名称：LED单管壁灯&#xD;&#xA;2、规格：1x18W LED 光通量1890lm&#xD;&#xA;3、安装形式：壁装，距地2.6m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="030412005002" Mc="荧光灯" Xmtz="1、名称：LED双管壁灯&#xD;&#xA;2、规格：2X18W LED 光通量3780LM&#xD;&#xA;3、安装形式：壁装，距地2.6m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="030412001001" Mc="普通灯具" Xmtz="1、名称：LED单管灯&#xD;&#xA;2、规格：1x18W LED 光通量1890lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="030412001002" Mc="普通灯具" Xmtz="1、名称：LED单管灯&#xD;&#xA;2、规格：1x18W LED 光通量1890lm&#xD;&#xA;3、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="109" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="030412001003" Mc="普通灯具" Xmtz="1、名称：LED双管灯&#xD;&#xA;2、规格：2x18W LED 光通量3780lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="030412002001" Mc="工厂灯" Xmtz="1、名称：防爆LED双管灯&#xD;&#xA;2、规格：2x18W LED 光通量3780lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="030412001004" Mc="普通灯具" Xmtz="1、名称：三防LED双管灯&#xD;&#xA;2、规格：2x18W LED 光通量3780lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="030412004001" Mc="装饰灯" Xmtz="1、名称：100*50金属线槽灯&#xD;&#xA;2、规格：2x18W LED 光通量3780lm&#xD;&#xA;3、安装方式：吊装&#xD;&#xA;4、含金属线槽、开孔、接地、附件安装、修理、基础等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="030412001005" Mc="普通灯具" Xmtz="1、名称：防水防尘灯&#xD;&#xA;2、规格：1x11W LED 光通量1155lm，防护等级：IP54&#xD;&#xA;3、安装方式：吸顶" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="030412005003" Mc="荧光灯" Xmtz="1、名称：节能LED灯（附带红外线光控带延时开关）&#xD;&#xA;2、规格：1x14W,LED 光通量1470lm&#xD;&#xA;3、安装形式：吸顶" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="030412001006" Mc="普通灯具" Xmtz="1、名称：电梯井道灯具&#xD;&#xA;2、型号：防水、防尘、带防护罩灯具，内设13W LED灯&#xD;&#xA;3、安装形式：壁装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="WB030904013001" Mc="智能照明灯/指示灯" Xmtz="1、名称：安全疏散方向标志灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：壁装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="300" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="WB030904013002" Mc="智能照明灯/指示灯" Xmtz="1、名称：安全疏散方向标志灯（大型）&#xD;&#xA;2、规格：DC36V,1X1W,LED&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="44" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="WB030904013003" Mc="智能照明灯/指示灯" Xmtz="1、名称：防爆安全疏散方向标志灯（大型）&#xD;&#xA;2、规格：DC36V,1X1W,LED&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="WB030904013004" Mc="智能照明灯/指示灯" Xmtz="1、名称：安全出口标志灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：门框上沿0.1m明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="WB030904013005" Mc="智能照明灯/指示灯" Xmtz="1、名称：防爆安全出口标志灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：门框上沿0.1m明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="WB030904013006" Mc="智能照明灯/指示灯" Xmtz="1、名称：楼层指示指示灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="WB030904013007" Mc="智能照明灯/指示灯" Xmtz="1、名称：疏散出口指示灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：门框上沿0.1m明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="WB030904013008" Mc="智能照明灯/指示灯" Xmtz="1、名称：消防应急照明灯&#xD;&#xA;2、规格：DC36V,1*6W,LED 光通量720lm&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="311" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="WB030904013009" Mc="智能照明灯/指示灯" Xmtz="1、名称：消防应急照明灯（IP67）&#xD;&#xA;2、规格：DC36V,1*6W,LED 光通量720lm&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="70" Qdbm="WB030904013010" Mc="智能照明灯/指示灯" Xmtz="1、名称：消防应急照明灯（9W）&#xD;&#xA;2、规格：DC36V,1X9W,LED 光通量1080LM&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="71" Qdbm="WB030904013011" Mc="智能照明灯/指示灯" Xmtz="1、名称：防爆消防应急照明灯&#xD;&#xA;2、规格：DC36V,1X9W,LED 光通量1080LM&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="030404034001" Mc="照明开关" Xmtz="1、名称：单联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="030404034002" Mc="照明开关" Xmtz="1、名称：双联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="030404034003" Mc="照明开关" Xmtz="1、名称：三联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="030404034004" Mc="照明开关" Xmtz="1、名称：单联双控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="030404034005" Mc="照明开关" Xmtz="1、名称：密闭防水三联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="030404034006" Mc="照明开关" Xmtz="1、名称：密闭防水双联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="030404034007" Mc="照明开关" Xmtz="1、名称：防爆单联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="030404034008" Mc="照明开关" Xmtz="1、名称：卫生间洗手池、小便池感应开关电源" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="030404031001" Mc="小电器" Xmtz="1、名称：控制按钮盒（两个按钮，1个检修按钮）&#xD;&#xA;2、安装方式：距地1.5明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（套、台）" Sl="19.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="030404031002" Mc="小电器" Xmtz="1、名称：防爆控制按钮盒(3个按钮,1个检修旋钮)&#xD;&#xA;2、安装方式：距地1.5明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（套、台）" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="030404031003" Mc="小电器" Xmtz="1、名称：防爆强启按钮盒(1个旋钮)&#xD;&#xA;2、安装方式：距地1.5明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（套、台）" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="030404035001" Mc="插座" Xmtz="1、名称：单相二、三眼插座&#xD;&#xA;2、规格：AC250V,10A，安全型&#xD;&#xA;3、安装方式：距地0.3m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="131" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="030404035002" Mc="插座" Xmtz="1、名称：单相二、三眼插座（密闭型）&#xD;&#xA;2、规格：AC250V,10A，安全型&#xD;&#xA;3、安装方式：距地0.3m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="030404035003" Mc="插座" Xmtz="1、名称：烘手器插座&#xD;&#xA;2、规格：AC250V,16A，安全型&#xD;&#xA;3、安装方式：距地1.5m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="030411006001" Mc="接线盒" Xmtz="1、名称：开关盒（插座盒）&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="260" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="030411006002" Mc="接线盒" Xmtz="1、名称：接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="972" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="030411006003" Mc="接线盒" Xmtz="1、名称：防爆接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.3" Mc="桥架、配管" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="89" Qdbm="030411003001" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：800*200&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="80.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="030411003002" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：800*150&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="112.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="030411003003" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：600*200&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="75.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="030411003004" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：600*150&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="245.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="030411003005" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：500*200&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="7.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="030411003006" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：400*200&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="238.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="95" Qdbm="030411003007" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：400*150&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="568.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="030411003008" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：200*100&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="76.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="030411003009" Mc="桥架" Xmtz="1、名称：电缆桥架&#xD;&#xA;2、规格：150*75&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="4.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="030413001001" Mc="铁构件" Xmtz="1、材质：型钢、角钢&#xD;&#xA;2、名称：桥架支撑架&#xD;&#xA;3、制作、安装" Gcnr="" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="2.399" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="030408008001" Mc="防火堵洞" Xmtz="1、名称：桥架、电缆等防火堵洞&#xD;&#xA;2、备注：包含本系统所有防火堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="13.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="030411001001" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN125&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="51.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="030411001002" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN100&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="50.64" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="030411001003" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="132.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="030411001004" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN40&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="109.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="030411001005" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN32&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="123.73" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="030411001006" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="1047.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="030411001007" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="1362.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="030411001008" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN32&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="12.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="108" Qdbm="030411001009" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="21.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="030411001010" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="37.59" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="030411001011" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="2619.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="111" Qdbm="030411001012" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="11496.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="112" Qdbm="030411001013" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="92.36" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="113" Qdbm="030411001014" Mc="配管" Xmtz="1、名称：金属软管&#xD;&#xA;2、规格：20#&#xD;&#xA;3、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="338.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="114" Qdbm="030413001002" Mc="铁构件" Xmtz="1、名称：线管吊装支架&#xD;&#xA;2、材质：型钢" Gcnr="" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="0.106" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="115" Qdbm="031002003001" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="116" Qdbm="031002003002" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN50&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.4" Mc="电缆、电线" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="117" Qdbm="030408001001" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-4*150+1*70&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="66.57" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="118" Qdbm="030408001002" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-4*95+1*50&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="105.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="119" Qdbm="030408001003" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-3*95+2*50&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="123.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="120" Qdbm="030408001004" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-4*16+1*16&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="74.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="121" Qdbm="030408001005" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-4*6+1*6&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="308.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="122" Qdbm="030408001006" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*150+2*70&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="55.14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="123" Qdbm="030408001007" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*70+1*35&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="123.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="124" Qdbm="030408001008" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*70+2*35&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="29.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="125" Qdbm="030408001009" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZBN-YJV-7*95&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="9.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="126" Qdbm="030408001010" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*25+1*16&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="468.38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="127" Qdbm="030408001011" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*16+1*16&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="183.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="128" Qdbm="030408001012" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*16+2*16&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="12.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="129" Qdbm="030408001013" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*10+1*10&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="413.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="130" Qdbm="030408001014" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*10+1*10&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="413.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="131" Qdbm="030408001015" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*10+2*10&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="115.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="132" Qdbm="030408001016" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*6+1*6&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="359.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="133" Qdbm="030408001017" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*6+2*6&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="387.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="134" Qdbm="030408001018" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZBN-YJV-5*4&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="63.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="135" Qdbm="030408001019" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZBN-YJV-5*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="56.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="136" Qdbm="030408001020" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*2.5+2*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="1029.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="137" Qdbm="030408001021" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*2.5+1*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="1835.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="138" Qdbm="030408001022" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZBN-YJV-3*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="519.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="139" Qdbm="030408002001" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-14*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="8.87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="140" Qdbm="030408002002" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-4*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="471.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="141" Qdbm="030408002003" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-2*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="12.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="142" Qdbm="030408002004" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZB-KVV-6*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="1233.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="143" Qdbm="030408002005" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZB-KVV-2*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="74.44" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="144" Qdbm="030408007001" Mc="控制电缆头" Xmtz="1、名称：控制电缆头&#xD;&#xA;2、规格型号：≤14芯&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="145" Qdbm="030408007002" Mc="控制电缆头" Xmtz="1、名称：控制电缆头&#xD;&#xA;2、规格型号：≤6芯&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="146" Qdbm="030408006001" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：10mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="160" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="147" Qdbm="030408006002" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：16mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="148" Qdbm="030408006003" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：35mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="149" Qdbm="030408006004" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：70mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="150" Qdbm="030408006005" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：120mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="151" Qdbm="030408006006" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：240mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="152" Qdbm="030411004001" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZB-BV2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="14587.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="153" Qdbm="030411004002" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-BV2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="844.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="154" Qdbm="030411004003" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZB-BV4&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="7973.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="155" Qdbm="030411004004" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-B2-RVS-2X2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="7666.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.5" Mc="防雷接地" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="156" Qdbm="030409005001" Mc="避雷网" Xmtz="1、名称：避雷网&#xD;&#xA;2、材质：Φ12热镀锌圆钢&#xD;&#xA;3、安装形式：明敷 " Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="1785.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="157" Qdbm="030409005002" Mc="避雷网" Xmtz="1、名称：避雷网&#xD;&#xA;2、材质：25*4热镀锌扁钢&#xD;&#xA;3、安装形式：明敷 " Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="119.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="158" Qdbm="030409003001" Mc="避雷引下线" Xmtz="1、名称：引下线&#xD;&#xA;2、安装形式：利用钢柱或柱内两根≥中16的主筋上端与屋面接闪器相连，下端与基础接地装置可靠焊接。" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="1083.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="159" Qdbm="WB030409002001" Mc="柱主筋与圈梁钢筋焊接" Xmtz="1、名称：柱主筋与圈梁钢筋焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="52.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="160" Qdbm="030409002001" Mc="接地母线" Xmtz="1、名称：接地母线&#xD;&#xA;2、材质：热镀锌扁钢&#xD;&#xA;3、规格：-25*4" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="561.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="161" Qdbm="030409002002" Mc="接地母线" Xmtz="1、名称：接地母线&#xD;&#xA;2、材质：热镀锌扁钢&#xD;&#xA;3、规格：-40*4" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="130.91" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="162" Qdbm="030409002003" Mc="接地母线" Xmtz="1、名称：接地母线&#xD;&#xA;2、材质：热镀铜扁钢&#xD;&#xA;3、规格：-40*4" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="1442.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="163" Qdbm="030409004001" Mc="基础梁接地线" Xmtz="1、名称：接地网&#xD;&#xA;2、安装形式：利用基础梁内两根&gt;16主钢筋(无钢筋处采用-40*4热镀铜扁钢)组成接地网&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="501.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="164" Qdbm="030409008001" Mc="等电位端子箱、测试板" Xmtz="1、名称：总等电位箱MEB&#xD;&#xA;2、材质：金属" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="165" Qdbm="030409008002" Mc="等电位端子箱、测试板" Xmtz="1、名称：局部等电位箱LEB&#xD;&#xA;2、材质：金属" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="166" Qdbm="030409008003" Mc="等电位端子箱、测试板" Xmtz="1、名称：辅助等电位箱SEB&#xD;&#xA;2、材质：金属" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="167" Qdbm="030409008004" Mc="等电位端子箱、测试板" Xmtz="1、名称：接地箱&#xD;&#xA;2、安装：安装于地面上0.3m或天花上0.3m" Gcnr="1、采购、安装" Jsgz="按设计图示数量计算" Dw="个" Sl="78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="168" Qdbm="WB030409003001" Mc="接地跨接线" Xmtz="1、名称：临时接地接线柱" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="6.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="169" Qdbm="030409001001" Mc="接地极" Xmtz="1、名称：预埋接地钢板&#xD;&#xA;2、规格、材质：100*100*8" Gcnr="" Jsgz="按设计图示数量计算" Dw="块" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="170" Qdbm="030411001015" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：PC&#xD;&#xA;3、规格：40&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="26.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="171" Qdbm="030411004005" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：穿管敷设&#xD;&#xA;3、规格：BVR-1*35&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="26.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="172" Qdbm="030414011001" Mc="接地装置" Xmtz="1、名称：接地系统测试" Gcnr="" Jsgz="1．以系统计量，按设计图示系统计算2．以组计量，按设计图示数量计算。" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.1" Mc="给水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="173" Qdbm="031001007001" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN80&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="122.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="174" Qdbm="031001007002" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN65&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="75.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="175" Qdbm="031001007003" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN50&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="100.29" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="176" Qdbm="031001007004" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN40&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="6.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="177" Qdbm="031001007005" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN32&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="8.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="178" Qdbm="031001007006" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN25&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="49.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="179" Qdbm="031001007007" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN20&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="7.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="180" Qdbm="031001006001" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 DN15&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="54.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="181" Qdbm="031001006002" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De20&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="270.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="182" Qdbm="031001006003" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De25&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="26.73" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="183" Qdbm="031001006004" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De32&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="11.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="184" Qdbm="031001006005" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De40&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="14.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="185" Qdbm="031001006006" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De50&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="28.22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="186" Qdbm="031003003001" Mc="焊接法兰阀门" Xmtz="1、类型：闸阀 DN80&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="187" Qdbm="031003003002" Mc="焊接法兰阀门" Xmtz="1、类型：闸阀 DN65&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="188" Qdbm="031003001001" Mc="螺纹阀门" Xmtz="1、类型：闸阀 DN50&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="189" Qdbm="031003001002" Mc="螺纹阀门" Xmtz="1、类型：球阀 DN50&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="190" Qdbm="031003001003" Mc="螺纹阀门" Xmtz="1、类型：球阀 DN40&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="191" Qdbm="031003001004" Mc="螺纹阀门" Xmtz="1、类型：球阀 DN32&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="192" Qdbm="031003001005" Mc="螺纹阀门" Xmtz="1、类型：球阀 DN25&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="193" Qdbm="031003001006" Mc="螺纹阀门" Xmtz="1、类型：减压阀 DN40&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="194" Qdbm="031003001007" Mc="螺纹阀门" Xmtz="1、类型：不锈钢自动排气阀 DN20&#xD;&#xA;2、连接形式：丝扣连接&#xD;&#xA;3、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="195" Qdbm="031003001008" Mc="螺纹阀门" Xmtz="1、类型：压力型真空破坏器&#xD;&#xA;2、规格：DN25&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="196" Qdbm="031003013001" Mc="水表" Xmtz="1、名称：远传水表 DN80&#xD;&#xA;2、连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="197" Qdbm="031003013002" Mc="水表" Xmtz="1、名称：远传水表 DN65&#xD;&#xA;2、连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="198" Qdbm="031003013003" Mc="水表" Xmtz="1、名称：远传水表 DN50&#xD;&#xA;2、连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="199" Qdbm="031003013004" Mc="水表" Xmtz="1、名称：远传水表 DN40&#xD;&#xA;2、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="200" Qdbm="031003013005" Mc="水表" Xmtz="1、名称：远传水表 DN32&#xD;&#xA;2、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="201" Qdbm="031003013006" Mc="水表" Xmtz="1、名称：远传水表 DN25&#xD;&#xA;2、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="202" Qdbm="031003003003" Mc="焊接法兰阀门" Xmtz="1、类型：Y型过滤器 DN50&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="203" Qdbm="031003003004" Mc="焊接法兰阀门" Xmtz="1、类型：低阻力倒流防止器 DN50&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="204" Qdbm="ZB040502011001" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN80&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="205" Qdbm="ZB040502011002" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN65&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="206" Qdbm="ZB040502011003" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN32&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="207" Qdbm="ZB040502011004" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN25&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="208" Qdbm="031002003003" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN80&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="209" Qdbm="031002003004" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="210" Qdbm="031002003005" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN32&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="211" Qdbm="031002003006" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN25&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="212" Qdbm="031002003007" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN65" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="213" Qdbm="031002001001" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="2471.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="214" Qdbm="031201003001" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后防锈漆二道,再刷灰色调和漆二道。" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="2471.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="215" Qdbm="031201001001" Mc="管道刷油" Xmtz="1、油漆品种：银粉漆&#xD;&#xA;2、涂刷遍数、漆膜厚度：2道" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="73.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="216" Qdbm="031208002001" Mc="管道绝热" Xmtz="1、名称：吊顶内架空充水给水管道防结露&#xD;&#xA;2、绝热材料品种：橡塑管壳&#xD;&#xA;3、绝热厚度：保温厚度20mm&#xD;&#xA;" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="1.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="217" Qdbm="031208002002" Mc="管道绝热" Xmtz="1、名称：室外明露给水管道(生活、消防)防冻保温&#xD;&#xA;2、绝热材料品种：橡塑管壳&#xD;&#xA;3、绝热厚度：30mm" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="0.14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="218" Qdbm="031208007001" Mc="防潮层、保护层" Xmtz="1、名称：室外明露给水管道(生活、消防)防冻保温&#xD;&#xA;2、保护层：外包0.5mm厚铝箔保护" Gcnr="" Jsgz="1.以立方米计算，按图示表面积加绝热层厚度及调整系数计算2.以千克计量，按图示金属结构质量计算" Dw="m2" Sl="6.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="219" Qdbm="WB031002009001" Mc="凿槽、刨沟" Xmtz="1、名称：管道剔堵沟槽&#xD;&#xA;2、墙体类型：砖墙&#xD;&#xA;3、尺寸：70*70以内" Gcnr="" Jsgz="按设计图示长度计算" Dw="m" Sl="220.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.2" Mc="排水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="220" Qdbm="031001006007" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De160&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="3.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="221" Qdbm="031001006008" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De110&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="378.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="222" Qdbm="031001006009" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De75&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="71.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="223" Qdbm="031001006010" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De50&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="168.87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="224" Qdbm="031001006011" Mc="塑料管" Xmtz="1、名称：耐热排水塑料管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De110&#xD;&#xA;5、连接形式：沟槽式卡箍连接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="29.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="225" Qdbm="WB031002001001" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN100" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="157" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="226" Qdbm="WB031002001002" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN75" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="227" Qdbm="WB031002001003" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN50" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="141" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="228" Qdbm="031002001002" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="125.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="229" Qdbm="031201003002" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后防锈漆二道,再刷灰色调和漆二道。" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="125.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="230" Qdbm="031004014001" Mc="给、排水附（配）件" Xmtz="1、名称：不锈钢防臭式地漏&#xD;&#xA;2、型号、规格：DN50" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="25.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="231" Qdbm="031004014002" Mc="给、排水附（配）件" Xmtz="1、名称：不锈钢大流量地漏&#xD;&#xA;2、型号、规格：DN100" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="9.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="232" Qdbm="031004014003" Mc="给、排水附（配）件" Xmtz="1、名称：不锈钢大流量地漏&#xD;&#xA;2、型号、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="233" Qdbm="031004014004" Mc="给、排水附（配）件" Xmtz="1、名称：清扫口&#xD;&#xA;2、材质：铜质&#xD;&#xA;3、型号、规格：DN100&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="9.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="234" Qdbm="031004006001" Mc="大便器" Xmtz="1、名称：低水箱蹲便器&#xD;&#xA;2、材质：陶瓷&#xD;&#xA;3、组装形式：成套&#xD;&#xA;4、附件名称、数量：含给排水附件&#xD;&#xA;5、参考图集09S304/83" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="235" Qdbm="031004003001" Mc="洗脸盆" Xmtz="1、名称：台式洗手盆&#xD;&#xA;2、材质：陶瓷&#xD;&#xA;3、组装形式：成套&#xD;&#xA;4、附件名称、数量：含给排水附件&#xD;&#xA;5、参考图集09S304/39（53）" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="236" Qdbm="031004007001" Mc="小便器" Xmtz="1、名称：感应式落地式小便器&#xD;&#xA;2、材质：陶瓷&#xD;&#xA;3、组装形式：成套&#xD;&#xA;4、附件名称、数量：含给排水附件&#xD;&#xA;5、参考图集09S304/109" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="237" Qdbm="031004008001" Mc="通气帽" Xmtz="1、材质：通气帽&#xD;&#xA;2、规格、类型：DN100&#xD;&#xA;3、附件名称、数量：含安装附件等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="238" Qdbm="031002003008" Mc="套管制作与安装" Xmtz="1、名称：阻火圈&#xD;&#xA;2、规格：DN100" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="239" Qdbm="031002003009" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="240" Qdbm="031002003010" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="241" Qdbm="031002003011" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.3" Mc="雨水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="242" Qdbm="031001006012" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De200&#xD;&#xA;4、连接形式：承插电热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="51.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="243" Qdbm="031001006013" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De160&#xD;&#xA;4、连接形式：承插电热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="756.50" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="244" Qdbm="031001006014" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De110&#xD;&#xA;4、连接形式：承插电热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="175.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="245" Qdbm="031001006015" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De75（防紫外线型）&#xD;&#xA;4、连接形式：承插电热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="175.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="246" Qdbm="WB031002001004" Mc="成品管卡安装" Xmtz="1．名称：成品管卡&#xD;&#xA;2．型号、规格：DN200" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="247" Qdbm="WB031002001005" Mc="成品管卡安装" Xmtz="1．名称：成品管卡&#xD;&#xA;2．型号、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="378" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="248" Qdbm="WB031002001006" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN100" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="249" Qdbm="WB031002001007" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN75" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="250" Qdbm="031004014005" Mc="给、排水附（配）件" Xmtz="1、型号、规格：87型雨水斗DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="251" Qdbm="031004014006" Mc="给、排水附（配）件" Xmtz="1、型号、规格：侧排雨水斗DN75" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="252" Qdbm="031002003012" Mc="溢流口" Xmtz="1、名称：溢流口&#xD;&#xA;2、规格：φ200PVC" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="253" Qdbm="031002003013" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="254" Qdbm="031002003014" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="255" Qdbm="031002003015" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN200&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="256" Qdbm="031002003016" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN75&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="257" Qdbm="031002003017" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="258" Qdbm="031002003018" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="259" Qdbm="031201001002" Mc="管道刷油" Xmtz="1、油漆品种：调和漆&#xD;&#xA;2、涂刷遍数、漆膜厚度：2道" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="400.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.4" Mc="负极清洗间废液排水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="260" Qdbm="030109001001" Mc="离心泵" Xmtz="1、名称：耐腐蚀卧式自吸泵&#xD;&#xA;2、设备参数：Q:15m3/h,H:38m,N:4.0kW" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="261" Qdbm="031001003001" Mc="不锈钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：压力废水&#xD;&#xA;3、规格、压力等级：SUS304不锈钢 DN100&#xD;&#xA;4、连接形式：卡压连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="85.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="262" Qdbm="031001003002" Mc="不锈钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：压力废水&#xD;&#xA;3、规格、压力等级：SUS304不锈钢 DN65&#xD;&#xA;4、连接形式：卡压连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="14.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="263" Qdbm="031001002001" Mc="钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：压力废水&#xD;&#xA;3、规格、压力等级：内外壁热浸镀锌钢管 DN100&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="85.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="264" Qdbm="031001002002" Mc="钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：压力废水&#xD;&#xA;3、规格、压力等级：内外壁热浸镀锌钢管 DN65&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="7.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="265" Qdbm="031003003005" Mc="焊接法兰阀门" Xmtz="1、类型：不锈钢法兰蝶阀&#xD;&#xA;2、规格、压力等级：DN65&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="266" Qdbm="031003003006" Mc="焊接法兰阀门" Xmtz="1、类型：不锈钢止回阀&#xD;&#xA;2、规格、压力等级：DN65&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="267" Qdbm="031003003007" Mc="焊接法兰阀门" Xmtz="1、类型：不锈钢止回阀&#xD;&#xA;2、规格、压力等级：DN65&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="268" Qdbm="031003010001" Mc="软接头（软管）" Xmtz="1、类型：可曲挠橡胶接头&#xD;&#xA;2、规格、压力等级：DN65&#xD;&#xA;3、连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="269" Qdbm="030601002001" Mc="压力仪表" Xmtz="1、名称：压力表&#xA;2、型号：满足设计要求&#xD;&#xA;3、压力等级：0~1.0MPa&#xA;4、备注：自带弯管及检修阀" Gcnr="" Jsgz="" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="270" Qdbm="ZB040502011005" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="271" Qdbm="030804001001" Mc="吸水喇叭口" Xmtz="1、名称：吸水喇叭口&#xD;&#xA;2、规格：DN65&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、含支架" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="272" Qdbm="030804001002" Mc="吸水喇叭口" Xmtz="1、名称：吸水喇叭口&#xD;&#xA;2、规格：DN65&#xD;&#xA;3、材质：SUS304不锈钢&#xD;&#xA;4、含支架" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="273" Qdbm="WB031002006001" Mc="预留孔洞" Xmtz="1、名称：预留孔洞&#xD;&#xA;2、规格：φ150&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="274" Qdbm="031201001003" Mc="管道刷油" Xmtz="1、油漆品种：调和漆&#xD;&#xA;2、涂刷遍数、漆膜厚度：2道" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="61.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.1" Mc="消火栓系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="275" Qdbm="030901001001" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="5.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="276" Qdbm="030901002001" Mc="消火栓钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸镀锌钢管&#xD;&#xA;3、规格：DN65&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="303.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="277" Qdbm="030901001002" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN100&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="738.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="278" Qdbm="030901002002" Mc="消火栓钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸镀锌钢管&#xD;&#xA;3、规格：DN150&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="773.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="279" Qdbm="031002001003" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="1650.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="280" Qdbm="031201003003" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后刷防锈漆二道,再刷灰色调和漆二道" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="1650.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="281" Qdbm="031201001004" Mc="管道刷油" Xmtz="1、名称：消火栓管道刷油&#xD;&#xA;2、油漆品种：除锈后刷红色调和漆二道。" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="702.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="282" Qdbm="031003001009" Mc="螺纹阀门" Xmtz="1、类型：不锈钢自动排气阀 DN25&#xD;&#xA;2、连接形式：丝扣连接&#xD;&#xA;3、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="283" Qdbm="031003003008" Mc="焊接法兰阀门" Xmtz="1、类型：闸阀&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="284" Qdbm="031003003009" Mc="焊接法兰阀门" Xmtz="1、类型：涡轮型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="285" Qdbm="031003003010" Mc="焊接法兰阀门" Xmtz="1、类型：涡轮型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="286" Qdbm="031003003011" Mc="焊接法兰阀门" Xmtz="1、类型：把手型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN65&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="287" Qdbm="ZB040502011006" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="288" Qdbm="ZB040502011007" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="289" Qdbm="030901010001" Mc="室内消火栓" Xmtz="1、名称：SNZW65-III型减压稳压消火栓&#xD;&#xA;2、箱内配置：采用甲型单栓带灭火器箱组合式消防柜,单栓箱内设有中Φ65消火栓1只Φ65x19水枪1只、Φ65x25m长衬胶水带1根。在每个消火栓处设置一个消火栓的按钮,作为发出报警信号的开关。箱体材质采用铝合金-钢制,箱内设有:室内减压稳压消火栓,出水口压力为0.35Mpa,选用消火栓栓口与墙面成90°角且箱体厚度为240mm的消防箱。暗装在防火上消火栓箱,箱体背面砌体应满足耐火极限不小于3小时;暗装在其他墙体上的箱体，其背面应保留100mm厚以上同材质的砌体;否则应在箱体背面采用不低于该墙体耐火极限(参《民用建筑构件防火设计用料表》)的防火板封堵。采用减压稳压型消火栓。消火栓箱门不应被装饰物遮掩,消火栓箱门四周的装修材料颜色应与消火栓箱门的颜色有明显区别或在消火栓箱门表面设置发光标志。&#xD;&#xA;3、含软包防撞处理、灭火器" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="290" Qdbm="030901010002" Mc="室内消火栓" Xmtz="1、名称：室内消火栓&#xD;&#xA;2、箱内配置：采用甲型单栓带灭火器箱组合式消防柜,单栓箱内设有中Φ65消火栓1只Φ65x19水枪1只、Φ65x25m长衬胶水带1根。在每个消火栓处设置一个消火栓的按钮,作为发出报警信号的开关。箱体材质采用铝合金-钢制，消火栓箱门四周的装修材料颜色应与消火栓箱门的颜色有明显区别或在消火栓箱门表面设置发光标志。&#xD;&#xA;3、含软包防撞处理、灭火器" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="291" Qdbm="030901010003" Mc="室内消火栓" Xmtz="1、名称：屋顶试验消火栓&#xD;&#xA;2、箱内配置：采用甲型单栓带灭火器箱组合式消防柜,单栓箱内设有中Φ65消火栓1只Φ65x19水枪1只、Φ65x25m长衬胶水带1根。在每个消火栓处设置一个消火栓的按钮,作为发出报警信号的开关。箱体材质采用铝合金-钢制,箱内设有:室内减压稳压消火栓,出水口压力为0.35Mpa,选用消火栓栓口与墙面成90°角且箱体厚度为240mm的消防箱。暗装在防火上消火栓箱,箱体背面砌体应满足耐火极限不小于3小时;暗装在其他墙体上的箱体，其背面应保留100mm厚以上同材质的砌体;否则应在箱体背面采用不低于该墙体耐火极限(参《民用建筑构件防火设计用料表》)的防火板封堵。采用减压稳压型消火栓。消火栓箱门不应被装饰物遮掩,消火栓箱门四周的装修材料颜色应与消火栓箱门的颜色有明显区别或在消火栓箱门表面设置发光标志。&#xD;&#xA;3、含软包防撞处理、灭火器" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="292" Qdbm="030901013001" Mc="灭火器箱" Xmtz="1、名称：灭火器箱&#xA;2、规格、型号：可放置两具灭火器" Gcnr="" Jsgz="" Dw="套" Sl="48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="293" Qdbm="030901013002" Mc="灭火器" Xmtz="1、名称：磷酸铵盐干粉灭火器&#xA;2、规格、型号：MF/ABC4" Gcnr="" Jsgz="" Dw="具" Sl="96.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="294" Qdbm="030901013003" Mc="灭火器" Xmtz="1、名称：磷酸铵盐推车灭火器&#xA;2、规格、型号：MFT/ABC20" Gcnr="" Jsgz="" Dw="具" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="295" Qdbm="030901013004" Mc="灭火器" Xmtz="1、名称：泡沫推车灭火器 &#xA;2、规格、型号：MPT20" Gcnr="" Jsgz="" Dw="具" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="296" Qdbm="030901013005" Mc="灭火器" Xmtz="1、名称：超细干粉自动灭火装置/悬挂式&#xA;2、规格、型号：15KG" Gcnr="" Jsgz="按设计图示数量计算" Dw="具" Sl="19.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="297" Qdbm="030902009001" Mc="无管网气体灭火装置" Xmtz="1、名称：柜式(无管网)预制七氟丙烷灭火装置&#xA;2、规格、型号：GQQ150*2/2.5&#xD;&#xA;3、含药剂，每瓶药剂量139Kg" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="298" Qdbm="031003011001" Mc="沟槽管堵" Xmtz="1、名称：沟槽管堵&#xD;&#xA;2、规格、型号：DN65" Gcnr="" Jsgz="按设计图示数量计算" Dw="片" Sl="12.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="299" Qdbm="031002003019" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="300" Qdbm="031002003020" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="301" Qdbm="031002003021" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="302" Qdbm="031002003022" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="303" Qdbm="031002003023" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="304" Qdbm="031002003024" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="305" Qdbm="030905002001" Mc="水灭火系统控制装置调试" Xmtz="1、名称：消火栓系统调试" Gcnr="" Jsgz="按控制装置的点数计算" Dw="点" Sl="92.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.2" Mc="喷淋系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="306" Qdbm="030901001003" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="3179.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="307" Qdbm="030901001004" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN32&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="1605.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="308" Qdbm="030901001005" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN40&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="1312.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="309" Qdbm="030901001006" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="2775.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="310" Qdbm="030901001007" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN65&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="318.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="311" Qdbm="030901001008" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN80&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="301.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="312" Qdbm="030901001009" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN100&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="135.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="313" Qdbm="030901001010" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN150&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="860.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="314" Qdbm="030901001011" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN200&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="124.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="315" Qdbm="031002001004" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="8079.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="316" Qdbm="031201003004" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后刷防锈漆二道,再刷灰色调和漆二道" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="8079.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="317" Qdbm="031201001005" Mc="管道刷油" Xmtz="1、名称：自动喷洒管管道刷油&#xD;&#xA;2、油漆品种：除锈后刷红色调和漆二道。" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="1991.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="318" Qdbm="031208002003" Mc="管道绝热" Xmtz="1、名称：室外明露给水管道(生活、消防)防冻保温&#xD;&#xA;2、绝热材料品种：橡塑管壳&#xD;&#xA;3、绝热厚度：30mm" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="0.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="319" Qdbm="031208007002" Mc="防潮层、保护层" Xmtz="1、名称：室外明露给水管道(生活、消防)防冻保温&#xD;&#xA;2、保护层：外包0.5mm厚铝箔保护" Gcnr="" Jsgz="1.以立方米计算，按图示表面积加绝热层厚度及调整系数计算2.以千克计量，按图示金属结构质量计算" Dw="m2" Sl="6.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="320" Qdbm="WB031202001001" Mc="埋地金属管道防腐" Xmtz="1、名称：埋地金属管道防腐&#xD;&#xA;2、油漆品种：做加强防腐处理" Gcnr="" Jsgz="按设计图示表面积计算" Dw="m2" Sl="20.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="321" Qdbm="030901003001" Mc="水喷淋（雾）喷头" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质、型号、规格：直立型标准响应喷头 K=80&#xD;&#xA;3、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2555" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="322" Qdbm="030901003002" Mc="水喷淋（雾）喷头" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质、型号、规格：干式下垂型标准响应喷头 K=80&#xD;&#xA;3、连接形式：螺纹连接&#xD;&#xA;4、装饰盘设计要求：含装饰盘" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="323" Qdbm="031003001010" Mc="螺纹阀门" Xmtz="1、类型：不锈钢自动排气阀 DN25&#xD;&#xA;2、连接形式：丝扣连接&#xD;&#xA;3、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="324" Qdbm="031003001011" Mc="自动排气阀" Xmtz="1、类型：快速排气阀&#xD;&#xA;2、规格、压力等级：DN32&#xD;&#xA;3、连接形式：螺纹连接&#xD;&#xA;4、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="325" Qdbm="031003001012" Mc="螺纹阀门" Xmtz="1、类型：电磁阀&#xD;&#xA;2、规格、压力等级：DN32&#xD;&#xA;3、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="326" Qdbm="ZB040502011008" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN200&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="327" Qdbm="ZB040502011009" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="328" Qdbm="ZB040502011010" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="329" Qdbm="ZB040502011011" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN80&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="330" Qdbm="ZB040502011012" Mc="补偿器（波纹管）" Xmtz="1、类型：不锈钢波纹软管&#xD;&#xA;2、规格、压力等级：DN50&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含补偿器、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="331" Qdbm="031003003012" Mc="焊接法兰阀门" Xmtz="1、类型：把手型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN80&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="332" Qdbm="031003003013" Mc="焊接法兰阀门" Xmtz="1、类型：涡轮型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="333" Qdbm="031003003014" Mc="焊接法兰阀门" Xmtz="1、类型：闸阀&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="334" Qdbm="031003003015" Mc="焊接法兰阀门" Xmtz="1、类型：信号阀&#xD;&#xA;2、规格、压力等级：DN200&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="335" Qdbm="031003003016" Mc="焊接法兰阀门" Xmtz="1、类型：信号阀&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="336" Qdbm="030901007001" Mc="减压孔板" Xmtz="1、类型：减压孔板&#xD;&#xA;2、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="337" Qdbm="030901007002" Mc="减压孔板" Xmtz="1、类型：减压孔板&#xD;&#xA;2、规格：DN200" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="338" Qdbm="030901006001" Mc="水流指示器" Xmtz="1、类型：水流指示器 DN150&#xD;&#xA;2、连接形式：法兰连接&#xD;&#xA;3、含法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="339" Qdbm="030901006002" Mc="水流指示器" Xmtz="1、类型：水流指示器 DN200&#xD;&#xA;2、连接形式：法兰连接&#xD;&#xA;3、含法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="340" Qdbm="030901004001" Mc="报警装置" Xmtz="1、名称：湿式报警阀组&#xD;&#xA;2、型号、规格：DN200&#xD;&#xA;3、含报警阀、水力警铃、信号阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="341" Qdbm="030901004002" Mc="报警装置" Xmtz="1、名称：预作用报警阀组&#xD;&#xA;2、型号、规格：DN150&#xD;&#xA;3、含报警阀、水力警铃、信号阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="342" Qdbm="030110001001" Mc="空压机" Xmtz="1、名称：空压机&#xD;&#xA;2、型号、规格：排气量0.5m3/min，功率3KW&#xD;&#xA;3、含连接管、止回阀、过滤器、压力开关等全套安装附件" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="343" Qdbm="030503006001" Mc="传感器、变送器" Xmtz="1、名称：电子流量计24V&#xD;&#xA;2、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="支(台)" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="344" Qdbm="030901008001" Mc="末端试水装置" Xmtz="1、名称：末端试水装置&#xD;&#xA;2、规格：DN25 &#xD;&#xA;3、组装形式：成套组装，含截止阀、压力表、试水接头，阀门箱上锁并设置标识" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="345" Qdbm="031003001013" Mc="螺纹阀门" Xmtz="1、类型：支管放水阀&#xD;&#xA;2、规格、压力等级：DN50&#xD;&#xA;3、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="346" Qdbm="030601002002" Mc="压力仪表" Xmtz="1、名称：压力表&#xA;2、型号：满足设计要求&#xD;&#xA;3、压力等级：0~1.0MPa&#xA;4、备注：自带弯管及检修阀" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="347" Qdbm="031004008002" Mc="通气帽" Xmtz="1、材质：通气帽&#xD;&#xA;2、规格、类型：DN80&#xD;&#xA;3、附件名称、数量：含安装附件等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="348" Qdbm="030817005001" Mc="钢制排水漏斗制作安装" Xmtz="1、名称：钢制排水漏斗&#xD;&#xA;2、规格：DN80" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="349" Qdbm="031002003025" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道D200&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="350" Qdbm="030905002002" Mc="水灭火系统控制装置调试" Xmtz="1、名称：自动喷淋系统调试" Gcnr="" Jsgz="按控制装置的点数计算" Dw="点" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.3" Mc="消防电系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="351" Qdbm="040504002001" Mc="电缆手孔井" Xmtz="1、名称：弱电手孔井&#xD;&#xA;2、规格：1000*1000*1200&#xD;&#xA;3、作法参07SD101-8所示 P121&#xD;&#xA;4、含手孔井砌筑、模板支护、钢筋绑扎、井壁抹面、井盖、铁件预埋、接地等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="352" Qdbm="030411001016" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、敷设方式：埋地" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="68.10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="353" Qdbm="031002003026" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN50&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="354" Qdbm="030411001017" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="3174.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="355" Qdbm="030411001018" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="5829.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="356" Qdbm="030411001019" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="22.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="357" Qdbm="030411001020" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="162.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="358" Qdbm="030411001021" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="12.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="359" Qdbm="030411003010" Mc="桥架" Xmtz="1、名称：火警专用防火金属线槽&#xD;&#xA;2、规格：(50+50+50)*100&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="557.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="360" Qdbm="030411003011" Mc="桥架" Xmtz="1、名称：消防应急广播专用防火金属线槽&#xD;&#xA;2、规格：50*25&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="59.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="361" Qdbm="030413001003" Mc="铁构件" Xmtz="1、材质：型钢、角钢&#xD;&#xA;2、名称：桥架支撑架&#xD;&#xA;3、制作、安装" Gcnr="" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="0.626" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="362" Qdbm="030408008002" Mc="防火堵洞" Xmtz="1、名称：桥架、电缆等防火堵洞&#xD;&#xA;2、备注：包含本系统所有防火堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="9.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="363" Qdbm="030411004006" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="9486.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="364" Qdbm="030411004007" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="459.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="365" Qdbm="030411004008" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、型号：ZBN-RVS-2X1.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="8626.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="366" Qdbm="030411004009" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="2642.67" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="367" Qdbm="030411004010" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="2211.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="368" Qdbm="030411004011" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVSP-4x1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="470.29" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="369" Qdbm="030408002006" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-4x1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="1243.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="370" Qdbm="030408002007" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-24x1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="1283.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="371" Qdbm="030404032001" Mc="端子箱" Xmtz="1、名称：接线端子箱&#xD;&#xA;2、安装部位：墙上安装,底距地+2.4m&#xD;&#xA;3、成套采购，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="372" Qdbm="030411005001" Mc="接线箱" Xmtz="1、名称：中转箱&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="373" Qdbm="030904008001" Mc="模块（模块箱）" Xmtz="1、名称：模块箱&#xD;&#xA;2、安装部位：墙上安装,底距地+2.4m&#xD;&#xA;3、成套采购，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（台）" Sl="9.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="374" Qdbm="030904008002" Mc="模块" Xmtz="1、名称：短路隔离器&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="51" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="375" Qdbm="030904001001" Mc="点型探测器" Xmtz="1、名称：智能感烟探测器&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="822" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="376" Qdbm="WB030904017001" Mc="防爆设备" Xmtz="1、名称：智能感烟探测器（防爆型）&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="377" Qdbm="030904001002" Mc="点型探测器" Xmtz="1、名称：智能感温探测器&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="378" Qdbm="030507001001" Mc="入侵探测设备" Xmtz="1、名称：线型光束感烟探测器&#xD;&#xA;2、安装方式：墙上安装,光束轴线距顶0.3~1.0m&#xD;&#xA;3、含发射单元、反射单元" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="379" Qdbm="030904003001" Mc="按钮" Xmtz="1、名称：消火栓报警按钮&#xD;&#xA;2、规格：消火栓箱内安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="380" Qdbm="WB030904017002" Mc="防爆设备" Xmtz="1、名称：消火栓报警按钮（防爆型）&#xD;&#xA;2、规格：消火栓箱内安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="381" Qdbm="030904007001" Mc="消防广播（扬声器）" Xmtz="1、名称：壁挂扬声器(6W)&#xD;&#xA;2、安装方式：离地2.3~2.6米安装&#xD;&#xA;3、阻燃材料,或具有阻燃后罩结构" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="104" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="382" Qdbm="030904005001" Mc="声光报警器" Xmtz="1、名称：声光报警器&#xD;&#xA;2、安装方式：墙装,底距地+2.3~3.0m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="383" Qdbm="030904003002" Mc="按钮" Xmtz="1、名称：手动火灾报警按钮&#xD;&#xA;2、规格：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="384" Qdbm="030904006001" Mc="消防报警电话插孔（电话）" Xmtz="1、名称：消防电话插孔&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="385" Qdbm="WB030904002001" Mc="火灾显示盘" Xmtz="1、名称：楼层显示器/区域显示器&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="386" Qdbm="030904006002" Mc="消防报警电话插孔（电话）" Xmtz="1、名称：固定式火警电话机&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="387" Qdbm="030904008003" Mc="模块（模块箱）" Xmtz="1、名称：输入输出模块&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="102" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="388" Qdbm="030904008004" Mc="模块（模块箱）" Xmtz="1、名称：输入模块&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="389" Qdbm="030411006004" Mc="接线盒" Xmtz="1、名称：接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1161" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="390" Qdbm="030411006005" Mc="接线盒" Xmtz="1、名称：防爆接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="391" Qdbm="030905001001" Mc="自动报警系统装置调试" Xmtz="1、名称：自动报警系统调试&#xD;&#xA;2、点数：2000点以内" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="392" Qdbm="WB030905001001" Mc="火灾事故广播、消防通信系统调试" Xmtz="1、名称：消防广播、电话插孔调试" Gcnr="" Jsgz="按系统的点数计算" Dw="只（部）" Sl="146.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="393" Qdbm="WB030905001002" Mc="火灾事故广播、消防通信系统调试" Xmtz="1、名称：火灾报警电话调试" Gcnr="" Jsgz="按系统的点数计算" Dw="只（部）" Sl="9.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="394" Qdbm="030905003001" Mc="防火控制装置联动调试" Xmtz="1、名称：防火阀联动调试" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（部）" Sl="85.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="395" Qdbm="030411004012" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：WDZ-RYJS-2X2.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="358.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="396" Qdbm="WB030904010001" Mc="消防电源监控设备" Xmtz="1、名称：消防电源监控器&#xD;&#xA;2、型号规格：AFPM3-3AVML" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="397" Qdbm="030905001002" Mc="自动报警系统装置调试" Xmtz="1、名称：消防电源监控系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="398" Qdbm="030411004013" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：WDZ-RYJS-2X2.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="358.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="399" Qdbm="WB030904010002" Mc="消防电源监控设备" Xmtz="1、名称：电气火灾监控器" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="400" Qdbm="030905001003" Mc="自动报警系统装置调试" Xmtz="1、名称：电气火灾监控系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="401" Qdbm="030411004014" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVVSP-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="460.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="402" Qdbm="030905001004" Mc="自动报警系统装置调试" Xmtz="1、名称：应急照明系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="403" Qdbm="030411001022" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="154.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="404" Qdbm="030411004015" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="453.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="405" Qdbm="030411004016" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="320.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="406" Qdbm="WB030904006001" Mc="防火门监控设备" Xmtz="1、名称：常闭单门防火门监控模块&#xD;&#xA;2、安装：门框上侧安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="407" Qdbm="030507001002" Mc="入侵探测设备" Xmtz="1、名称：门磁开关&#xD;&#xA;2、门框上侧安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="408" Qdbm="030905001005" Mc="自动报警系统装置调试" Xmtz="1、名称：防火门监控系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="409" Qdbm="030411001023" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="149.19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="410" Qdbm="030411001024" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="45.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="411" Qdbm="030411004017" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="202.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="412" Qdbm="030411004018" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="604.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="413" Qdbm="030904009001" Mc="区域报警控制箱" Xmtz="1、名称：气体灭火控制器&#xD;&#xA;2、成套采购，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="414" Qdbm="030904003003" Mc="按钮" Xmtz="1、名称：气灭紧急启停按钮&#xD;&#xA;2、安装部位：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="415" Qdbm="030404019001" Mc="控制开关" Xmtz="1、名称：手自动转换开关&#xD;&#xA;2、安装部位：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="416" Qdbm="030904005002" Mc="声光报警器" Xmtz="1、名称：气灭声光报警器&#xD;&#xA;2、安装方式：门框上安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="417" Qdbm="030904004001" Mc="消防警铃" Xmtz="1、名称：气灭警铃&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="418" Qdbm="030904001003" Mc="点型探测器" Xmtz="1、名称：智能感烟探测器&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="419" Qdbm="030904001004" Mc="点型探测器" Xmtz="1、名称：智能感温探测器&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="420" Qdbm="030412004002" Mc="装饰灯" Xmtz="1、名称：气灭气体释放灯&#xD;&#xA;2、安装方式：门框上安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="421" Qdbm="030904008005" Mc="模块（模块箱）" Xmtz="1、名称：输入输出模块&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="422" Qdbm="030411006006" Mc="接线盒" Xmtz="1、名称：接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒&#xD;&#xA;4、安装方式：暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="423" Qdbm="030411001025" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="54.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="424" Qdbm="030411001026" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="45.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="425" Qdbm="030411004019" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="107.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="426" Qdbm="030411004020" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="560.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="427" Qdbm="030904009002" Mc="区域报警控制箱" Xmtz="1、名称：可燃气体报警控制器&#xD;&#xA;2、控制器自带蓄电池，可持续供电时间≥3H" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="428" Qdbm="WB030904017003" Mc="防爆设备" Xmtz="1、名称：可燃气体探测器（防爆型）&#xD;&#xA;2、安装方式：设置在可能产生可燃气体部位附近" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="429" Qdbm="WB030904017004" Mc="防爆设备" Xmtz="1、名称：声光警报器（防爆型）&#xD;&#xA;2、安装方式：墙装,底距地+2.3~3.0m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="430" Qdbm="030904008006" Mc="模块（模块箱）" Xmtz="1、名称：输入输出模块&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="431" Qdbm="030411006007" Mc="接线盒" Xmtz="1、名称：防爆接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="432" Qdbm="030411001027" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="14.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="433" Qdbm="030411004021" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="15.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="434" Qdbm="030411004022" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="452.35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="435" Qdbm="WB030904004001" Mc="吸气式感烟火灾探测器" Xmtz="1、名称：空气采样早期报警探测器&#xD;&#xA;2、安装方式：挂墙安装,底距地+1.5m" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="436" Qdbm="WB030904003001" Mc="空气采样管" Xmtz="1、名称：空气采样侦测管路(ABS25)&#xD;&#xA;2、材质：ABS管φ25&#xD;&#xA;3、含采样孔" Gcnr="" Jsgz="按设计图示长度计算" Dw="m" Sl="151.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.1" Mc="通风系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="437" Qdbm="WB030701004001" Mc="通风机安装" Xmtz="1、名称：PF-1-1低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量800m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="438" Qdbm="WB030701004002" Mc="通风机安装" Xmtz="1、名称：PF-1-2低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量900m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="439" Qdbm="WB030701004003" Mc="通风机安装" Xmtz="1、名称：PF-1-3低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量1300m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="440" Qdbm="WB030701004004" Mc="通风机安装" Xmtz="1、名称：PF-1-4低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量800m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="441" Qdbm="WB030701004005" Mc="通风机安装" Xmtz="1、名称：PF-1-5低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量600m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="442" Qdbm="WB030701004006" Mc="通风机安装" Xmtz="1、名称：PF-1-6低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量600m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="443" Qdbm="WB030701004007" Mc="通风机安装" Xmtz="1、名称：PF-1-7低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量1900m3/h，静压250Pa，电动机功率0.75KW，转速1450rpm，噪声限值74dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="444" Qdbm="WB030701004008" Mc="通风机安装" Xmtz="1、名称：PF-1-8低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量9700m3/h，静压300Pa，电动机功率2.2KW，转速1450rpm，噪声限值75dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="445" Qdbm="WB030701004009" Mc="通风机安装" Xmtz="1、名称：PF-1-9低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量1300m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="446" Qdbm="WB030701004010" Mc="通风机安装" Xmtz="1、名称：PF-2-1低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量6800m3/h，静压300Pa，电动机功率1.5KW，转速1450rpm，噪声限值75dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="447" Qdbm="WB030701004011" Mc="通风机安装" Xmtz="1、名称：PF-2-2低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量800m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="448" Qdbm="WB030701004012" Mc="通风机安装" Xmtz="1、名称：PF-2-3低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量900m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="449" Qdbm="WB030701004013" Mc="通风机安装" Xmtz="1、名称：PF-2-4低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量1300m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="450" Qdbm="WB030701004014" Mc="通风机安装" Xmtz="1、名称：PF-3-1低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量800m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="451" Qdbm="WB030701004015" Mc="通风机安装" Xmtz="1、名称：PF-3-2低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量900m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="452" Qdbm="WB030701004016" Mc="通风机安装" Xmtz="1、名称：PF-3-3低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量1300m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="453" Qdbm="WB030701004017" Mc="通风机安装" Xmtz="1、名称：PF-4-1低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量800m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="454" Qdbm="WB030701004018" Mc="通风机安装" Xmtz="1、名称：PF-4-2低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量900m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="455" Qdbm="WB030701004019" Mc="通风机安装" Xmtz="1、名称：PF-4-3低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量1300m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="456" Qdbm="WB030701004020" Mc="通风机安装" Xmtz="1、名称：SEF-250D4边墙风机&#xD;&#xA;2、设备主要参数：风量1000m3/h，静压70Pa，电动机功率0.125KW，转速1450rpm，噪声限值55dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目),自带防雨百叶&#xD;&#xA;4、安装形式：边墙安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="457" Qdbm="WB030701004021" Mc="通风机安装" Xmtz="1、名称：SEF-300D4边墙风机&#xD;&#xA;2、设备主要参数：风量1400m3/h，静压80Pa，电动机功率0.125KW，转速1450rpm，噪声限值57dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目),自带防雨百叶&#xD;&#xA;4、安装形式：边墙安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="458" Qdbm="WB030701004022" Mc="通风机安装" Xmtz="1、名称：SEF-350D4边墙风机&#xD;&#xA;2、设备主要参数：风量1700m3/h，静压90Pa，电动机功率0.25KW，转速1450rpm，噪声限值61dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目),自带防雨百叶&#xD;&#xA;4、安装形式：边墙安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="459" Qdbm="WB030701004023" Mc="通风机安装" Xmtz="1、名称：SEF-500D4边墙风机&#xD;&#xA;2、设备主要参数：风量7400m3/h，静压100Pa，电动机功率0.37KW，转速1450rpm，噪声限值73dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目),自带防雨百叶&#xD;&#xA;4、安装形式：边墙安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="460" Qdbm="WB030701004024" Mc="通风机安装" Xmtz="1、名称：PF(SG)-1-1低噪音箱式管道离心风机(事故)&#xD;&#xA;2、设备主要参数：风量12000m3/h，静压350Pa，电动机功率4.0KW，转速800rpm，噪声限值73dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="461" Qdbm="WB030701004025" Mc="通风机安装" Xmtz="1、名称：PF(SG)-1-2低噪音箱式管道离心风机(防爆型)(事故)&#xD;&#xA;2、设备主要参数：风量1900m3/h，静压300Pa，电动机功率0.75KW，转速1450rpm，噪声限值70dB(A)，效率≥75%，防爆等级Ex dⅡCT4&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="462" Qdbm="030702001001" Mc="碳钢通风管道" Xmtz="1、名称：通风风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：1000&lt;b≤1500&#xD;&#xA;5、厚度：1.0mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰安装所需一切附件" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="148.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="463" Qdbm="030702001002" Mc="碳钢通风管道" Xmtz="1、名称：通风风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：450&lt;b≤1000&#xD;&#xA;5、厚度：0.75mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="41.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="464" Qdbm="030702001003" Mc="碳钢通风管道" Xmtz="1、名称：通风风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：450&lt;b≤630&#xD;&#xA;5、厚度：0.6mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="57.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="465" Qdbm="030702001004" Mc="碳钢通风管道" Xmtz="1、名称：通风风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：b≤450&#xD;&#xA;5、厚度：0.5mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="86.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="466" Qdbm="030702009001" Mc="弯头导流叶片" Xmtz="1、名称：导流叶片&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="5.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="467" Qdbm="WB030702001001" Mc="软管接口" Xmtz="1、名称：风管软管接头&#xD;&#xA;2、材质：不燃浸胶机布" Gcnr="" Jsgz="按设计图示以展开面积计算" Dw="m2" Sl="13.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="468" Qdbm="030703007001" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：1200*500&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="469" Qdbm="030703007002" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：250*250&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="470" Qdbm="030703007003" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：300*300&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="471" Qdbm="030703007004" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：350*350&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="472" Qdbm="030703007005" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：400*400&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="473" Qdbm="030703007006" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：500*500&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="474" Qdbm="030703007007" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：550*550&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="475" Qdbm="030703007008" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：800*400&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="476" Qdbm="030703007009" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：800*600&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="477" Qdbm="030703001001" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：1250*500&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="478" Qdbm="030703001002" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：320*320&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="479" Qdbm="030703001003" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：500*500&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="480" Qdbm="030703001004" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：800*500&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="481" Qdbm="030703001005" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：800*500&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="482" Qdbm="030703001006" Mc="碳钢阀门安装" Xmtz="1、名称：电动风阀(开关型)&#xD;&#xA;2、规格：1250*500" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="483" Qdbm="030703001007" Mc="碳钢阀门安装" Xmtz="1、名称：电动风阀(开关型)&#xD;&#xA;2、规格：500*320" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="484" Qdbm="030703001008" Mc="碳钢阀门安装" Xmtz="1、名称：电动风阀(开关型)&#xD;&#xA;2、规格：1100*2000" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="485" Qdbm="030703001009" Mc="碳钢阀门安装" Xmtz="1、名称：单向阀&#xD;&#xA;2、规格：1000*400" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="486" Qdbm="030703001010" Mc="碳钢阀门安装" Xmtz="1、名称：单向阀&#xD;&#xA;2、规格：500*250" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="487" Qdbm="030703001011" Mc="碳钢阀门安装" Xmtz="1、名称：单向阀&#xD;&#xA;2、规格：500*320" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="488" Qdbm="WB030701005001" Mc="设备支架制作安装" Xmtz="1、名称：设备支吊架&#xD;&#xA;2、材质：型钢" Gcnr="1、制作、安装" Jsgz="按设计图示质量计算" Dw="kg" Sl="760.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="489" Qdbm="031002001005" Mc="风管支架刷漆" Xmtz="1、名称：风管及设备支吊架刷漆&#xD;&#xA;2、做法：除锈后刷防锈底漆二道,调和面漆二道" Gcnr="1、制作、安装&#xD;&#xA;2、除锈、刷油" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="1939.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.2" Mc="防排烟系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="490" Qdbm="WB030701004026" Mc="通风机安装" Xmtz="1、名称：PY-R-1消防型管道轴流风机&#xD;&#xA;2、设备主要参数：风量113640m3/h，静压1470Pa，电动机功率75KW，转速1450rpm，噪声限值92dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件&#xD;&#xA;4、安装形式：落地安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="491" Qdbm="030702001005" Mc="碳钢通风管道" Xmtz="1、名称：防排烟风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：2000&lt;b≤4000&#xD;&#xA;5、厚度：2.0mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="959.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="492" Qdbm="030702001006" Mc="碳钢通风管道" Xmtz="1、名称：防排烟风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：1500&lt;b≤2000&#xD;&#xA;5、厚度：1.5mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="2067.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="493" Qdbm="030702001007" Mc="碳钢通风管道" Xmtz="1、名称：防排烟风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：1000&lt;b≤1500&#xD;&#xA;5、厚度：1.2mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="1243.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="494" Qdbm="030702001008" Mc="碳钢通风管道" Xmtz="1、名称：防排烟风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：450&lt;b≤1000&#xD;&#xA;5、厚度：1.0mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="19.69" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="495" Qdbm="WB030702001002" Mc="软管接口" Xmtz="1、名称：风管软管接头&#xD;&#xA;2、材质：不燃浸胶机布" Gcnr="" Jsgz="按设计图示以展开面积计算" Dw="m2" Sl="2.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="496" Qdbm="030702009002" Mc="弯头导流叶片" Xmtz="1、名称：导流叶片&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="25.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="497" Qdbm="030703007010" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排烟风口&#xD;&#xA;2、规格：1000*800&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="498" Qdbm="030703007011" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排烟风口&#xD;&#xA;2、规格：1200*1000&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="499" Qdbm="030703007012" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排烟风口&#xD;&#xA;2、规格：600*600&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="500" Qdbm="030703007013" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排烟风口&#xD;&#xA;2、规格：800*800&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="501" Qdbm="030703001012" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1000*320&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="502" Qdbm="030703001013" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1250*320&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="503" Qdbm="030703001014" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1250*400&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="504" Qdbm="030703001015" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1400*400&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="505" Qdbm="030703001016" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1600*400&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="506" Qdbm="030703001017" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1600*500&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="507" Qdbm="030703001018" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：2000*550&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="508" Qdbm="030703001019" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：2000*750&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="509" Qdbm="030703001020" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：2100*700&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="510" Qdbm="030703001021" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：2100*750&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="511" Qdbm="030703001022" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1000*320&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="512" Qdbm="030703001023" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1250*320&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="513" Qdbm="030703001024" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1250*400&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="514" Qdbm="030703001025" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1400*400&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="515" Qdbm="030703001026" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1600*400&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="516" Qdbm="030703001027" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1600*500&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="517" Qdbm="030703001028" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：2100*700&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="518" Qdbm="030703001029" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：2100*750&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="519" Qdbm="031208003001" Mc="通风管道绝热" Xmtz="1、绝热材料品种：金属风管外包防排烟专用岩棉复合铝箔&#xD;&#xA;2、绝热厚度：50mm以上&#xD;&#xA;3、材料类型：岩棉板采用防火黑棉，容重(60kg/m³)" Gcnr="" Jsgz="1．以立方米计算，按图示表面积加绝热层厚度及调整系数计算2．以立方米计量，按图示表面积及调整系数计算" Dw="m3" Sl="4.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="520" Qdbm="031208003002" Mc="通风管道绝热" Xmtz="1、绝热材料品种：金属风管外包防排烟专用岩棉复合铝箔&#xD;&#xA;2、绝热厚度：65mm以上&#xD;&#xA;3、材料类型：岩棉板采用防火黑棉，容重(100kg/m³)" Gcnr="" Jsgz="1．以立方米计算，按图示表面积加绝热层厚度及调整系数计算2．以立方米计量，按图示表面积及调整系数计算" Dw="m3" Sl="304.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="521" Qdbm="WB030701005002" Mc="设备支架制作安装" Xmtz="1、名称：设备支吊架&#xD;&#xA;2、材质：型钢" Gcnr="1、制作、安装" Jsgz="按设计图示质量计算" Dw="kg" Sl="40.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="522" Qdbm="031002001006" Mc="风管支架刷漆" Xmtz="1、名称：风管及设备支吊架刷漆&#xD;&#xA;2、做法：除锈后刷防锈底漆二道,调和面漆二道" Gcnr="1、制作、安装&#xD;&#xA;2、除锈、刷油" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="18112.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="523" Qdbm="WB030906007001" Mc="挡烟垂壁" Xmtz="1、名称：固定式挡烟垂壁&#xD;&#xA;2、材质：无机防火布" Gcnr="" Jsgz="按设计图示面积数量计算" Dw="m2" Sl="3188.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="524" Qdbm="ZB010101001001" Mc="电梯工程" Xmtz="1、名称：厂房三3T货梯&#xD;&#xA;2、参数：载重量3000KG，速度0.5m/s，层站数4，井道净尺寸(扣梁柱)3400x3300，门洞尺寸2400x2550，提升高度19m&#xD;&#xA;3、说明：包含全新的电梯主体设施设备，电气设备，控制系统，曳引系统，安全设备及构件，外罩配套按钮及显示，轿厢内通风、照明，层门及门坎门楣，五方对讲等&#xD;&#xA;4、含安装费、吊运费、安装调试" Gcnr="" Jsgz="" Dw="部" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="525" Qdbm="ZB010101001002" Mc="电梯工程" Xmtz="1、名称：厂房三5T货梯&#xD;&#xA;2、参数：载重量5000KG，速度0.5m/s，层站数4，井道净尺寸(扣梁柱)4100x4050，门洞尺寸2800x3050，提升高度19m&#xD;&#xA;3、说明：包含全新的电梯主体设施设备，电气设备，控制系统，曳引系统，安全设备及构件，外罩配套按钮及显示，轿厢内通风、照明，层门及门坎门楣，五方对讲等&#xD;&#xA;4、含安装费、吊运费、安装调试" Gcnr="" Jsgz="" Dw="部" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="526" Qdbm="010101003001" Mc="挖沟槽土方" Xmtz="1、土壤类别：自行勘测&#xD;&#xA;2、挖沟深度：2米以内&#xD;&#xA;3、回填要求：夯填" Gcnr="" Jsgz="按设计图示尺寸沟槽长度乘以沟槽断面积，以体积计算" Dw="m3" Sl="215.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="527" Qdbm="ZB010101001003" Mc="消防水箱系统迁移" Xmtz="1、名称：消防水箱系统迁移&#xD;&#xA;2、说明：含不锈钢消防水箱、消火栓及喷淋泵组、气压罐、阀门、管道附件、管道等保护性拆除、搬运、吊装、安装、保温、支墩、调试、原管道封堵等相关工作，投标人自行考虑相关报价，中标后不予调整" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="528" Qdbm="031301017001" Mc="脚手架搭拆" Xmtz="1、内容：脚手架搭拆费用&#xD;&#xA;2、投标人综合考虑报价，中标后不予调整&#xD;&#xA;" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="529" Qdbm="WB031301002001" Mc="操作高度增加费" Xmtz="1、内容：操作高度增加费 &#xD;&#xA;2、投标人综合考虑报价，中标后不予调整&#xD;&#xA;" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="530" Qdbm="031301012001" Mc="工程系统检测、检验" Xmtz="1、名称：暖通系统调试费&#xD;&#xA;2、投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="531" Qdbm="WB031301001001" Mc="建筑物超高增加费" Xmtz="1、名称：建筑物超高增加费&#xD;&#xA;2、投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
  </Dxgcxx>
  <Dxgcxx Dxgcmc="电芯库" Dxgcbh="dx002" Je="0" Bkjzf="0" Aqwmf="0" Zgj="0" Jzmj="4936" Aqsczrbxf="0">
    <Dwgcxx Dwgcbh="00003" Dwgcmc="电芯库（土建）" Zylb="1" Jzmj="4936" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B9767C6F3B122686496A" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="0101" Mc="土石方工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="010101001001" Mc="平整场地" Xmtz="1．土壤类别：综合，不分类别" Gcnr="" Jsgz="按建筑物首层建筑面积，以面积计算" Dw="m2" Sl="2428.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="010101004001" Mc="挖基坑土方、挖沟槽土方" Xmtz="1．土壤类别：自行考虑&#xD;&#xA;2．挖土深度：5m以内&#xD;&#xA;3．部位：基础、基础梁、集水坑等&#xD;&#xA;4．开挖过程中所遇淤泥、建筑垃圾、房屋基础、设备基础、障碍物等投标单位自行考虑在报价中，中标后不予调整&#xD;&#xA;5．控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示尺寸基坑底面积乘以挖土深度，以体积计算" Dw="m3" Sl="2215.14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="WB010101011001" Mc="人工清底" Xmtz="1．清底范围：按施工所需清底的面积&#xD;&#xA;2．土壤类别：综合，不分类别&#xD;&#xA;3．清底要求：在接近设计标高时必须预留一定厚度的土层使用人工清理，预留土层厚度按施工规范执行，投标单位综合考虑报价，中标后不予调整" Gcnr="" Jsgz="按需清底的范围，以面积计算" Dw="m2" Sl="592.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="010103001001" Mc="回填方" Xmtz="1．部位：基础回填&#xD;&#xA;2．夯填（碾压）:素土夯实,压实系数≥0.94&#xD;&#xA;3．控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示尺寸,以体积计算" Dw="m3" Sl="706.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0103" Mc="桩基工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="5" Qdbm="010301002001" Mc="预制钢筋混凝土管桩（试桩）" Xmtz="1．地层情况：自行考虑&#xD;&#xA;2．桩种类、规格、型号：PHC400AB95&#xD;&#xA;3．混凝土强度等级：C80&#xD;&#xA;4．桩长度：19、20m&#xD;&#xA;5．包含送桩费用" Gcnr="" Jsgz="按设计图示截面积乘以桩长（包括桩尖），以体积计算" Dw="m" Sl="58.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="WB010301007001" Mc="接桩（试桩）" Xmtz="1．桩类型：预应力高强混凝土管桩&#xD;&#xA;2．桩径：400mm&#xD;&#xA;3．预制桩应尽量减少接桩接头数量" Gcnr="" Jsgz="按接头数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="WB010301006001" Mc="管桩填心（试桩）" Xmtz="1．桩种类、规格、型号：PHC400AB95&#xD;&#xA;2．填心深度：不小于2m&#xD;&#xA;3．填心材料：C35微膨胀混凝土" Gcnr="" Jsgz="按设计取土（填土）体积计算" Dw="m3" Sl="0.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="WB010301003001" Mc="钢桩尖制作、安装（试桩）" Xmtz="1．类型：锥形闭口型钢桩尖" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.065" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="010515004001" Mc="钢筋笼制安（试桩）" Xmtz="1．钢筋种类、规格：参图集《先张法预应力混凝土管桩》(23G409)&#xD;&#xA;2．托盘：4-5mm厚圆薄钢板" Gcnr="" Jsgz="按设计图示钢筋（网）长度（面积）乘单位理论质量计算。" Dw="t" Sl="0.093" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="010301004001" Mc="截（凿）桩头（试桩）" Xmtz="1．桩类型、桩头截面：PHC400AB95&#xD;&#xA;2．混凝土强度等级：C80&#xD;&#xA;3．有无钢筋：有&#xD;&#xA;4．含桩头废料的清理、外弃" Gcnr="" Jsgz="1.灌注混凝土桩凿桩头，按设计桩截面乘以桩头长度，以体积计算2.预制方（管）桩截（凿）桩头，按设计图示数量计算" Dw="根" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="010301002002" Mc="预制钢筋混凝土管桩" Xmtz="1．地层情况：自行考虑&#xD;&#xA;2．桩种类、规格、型号：PHC400AB95&#xD;&#xA;3．混凝土强度等级：C80&#xD;&#xA;4．桩长度：19、20m&#xD;&#xA;5．包含送桩费用" Gcnr="" Jsgz="按设计图示截面积乘以桩长（包括桩尖），以体积计算" Dw="m" Sl="2166.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="WB010301007002" Mc="接桩" Xmtz="1．桩类型：预应力高强混凝土管桩&#xD;&#xA;2．桩径：400mm&#xD;&#xA;3．预制桩应尽量减少接桩接头数量" Gcnr="" Jsgz="按接头数量计算" Dw="个" Sl="113" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="WB010301006002" Mc="管桩填心" Xmtz="1．桩种类、规格、型号：PHC400AB95&#xD;&#xA;2．填心深度：不小于2m&#xD;&#xA;3．填心材料：C35微膨胀混凝土" Gcnr="" Jsgz="按设计取土（填土）体积计算" Dw="m3" Sl="7.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="WB010301003002" Mc="钢桩尖制作、安装" Xmtz="1．类型：锥形闭口型钢桩尖" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="2.441" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="010515004002" Mc="钢筋笼制安" Xmtz="1．钢筋种类、规格：参图集《先张法预应力混凝土管桩》(23G409)&#xD;&#xA;2．托盘：4-5mm厚圆薄钢板" Gcnr="" Jsgz="按设计图示钢筋（网）长度（面积）乘单位理论质量计算。" Dw="t" Sl="3.495" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="010301004002" Mc="截（凿）桩头" Xmtz="1．桩类型、桩头截面：PHC400AB95&#xD;&#xA;2．混凝土强度等级：C80&#xD;&#xA;3．有无钢筋：有&#xD;&#xA;4．含桩头废料的清理、外弃" Gcnr="" Jsgz="1.灌注混凝土桩凿桩头，按设计桩截面乘以桩头长度，以体积计算2.预制方（管）桩截（凿）桩头，按设计图示数量计算" Dw="根" Sl="113" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="010904002001" Mc="预制管桩头防水" Xmtz="1．涂膜厚度、遍数：2.0厚水泥基防水涂料&#xD;&#xA;2．钢筋混凝土桩头(清理干净)" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="71.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0104" Mc="砌筑工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="18" Qdbm="010401001001" Mc="砖基础" Xmtz="1．部位：地面以下或防潮层以下直接与土接触的墙体&#xD;&#xA;2．砖品种、规格、强度级：MU20的混凝土普通实心砖&#xD;&#xA;3．砂浆强度级：DM M10预拌砂浆砌筑" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="65.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="010401001002" Mc="砖胎膜" Xmtz="1．砖品种、规格、强度级：非黏土实心砖&#xD;&#xA;2．砂浆强度级：DM M10预拌砂浆砌筑" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="10.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="010402001001" Mc="砌块墙" Xmtz="1．部位：内外隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以下）&#xD;&#xA;4．砂浆强度级：M5.0专用混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="213.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="010402001002" Mc="砌块墙" Xmtz="1．部位：内外隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以上）&#xD;&#xA;4．砂浆强度级：M5.0专用混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="160.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="010402001003" Mc="砌块墙" Xmtz="1．部位：卫生间隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以内）&#xD;&#xA;4．砂浆强度级：M5.0混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="12.38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="010402001004" Mc="砌块墙" Xmtz="1．部位：卫生间隔墙&#xD;&#xA;2．砌块品种、规格、强度级：蒸压加气混凝土砌块A5.0(B06)&#xD;&#xA;3．墙体类型：200mm(高度3.6m以上）&#xD;&#xA;4．砂浆强度级：M5.0混合砂浆" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="11.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="WB010401016001" Mc="砖砌台阶" Xmtz="1．部位：出屋面台阶&#xD;&#xA;2．砖品种、规格、强度级：MU20页岩多孔砖&#xD;&#xA;3．砂浆强度级：M5.0砌筑砂浆&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="0.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="WB010401015001" Mc="墙基防潮层" Xmtz="1．部位：在室内地坪下0.06m处&#xD;&#xA;2．防潮层材料种类：60厚C20细石混凝土掺4%~5%防水剂" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="76.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0105" Mc="混凝土工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="26" Qdbm="010404001001" Mc="垫层" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．材料品种及比例：C20混凝土" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="48.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="010501003001" Mc="独立基础及桩承台" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C35" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="137.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="010501004001" Mc="满堂基础" Xmtz="1．部位：电梯底板、集水坑底板等&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30防水混凝土，抗渗等级为P6" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="9.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="010501006001" Mc="设备基础" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="010502001001" Mc="矩形柱" Xmtz="1．柱规格形状：矩形1.6m以内&#xD;&#xA;2．周长：1.6m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="17.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="010502001002" Mc="矩形柱" Xmtz="1．柱规格形状：矩形&#xD;&#xA;2．周长：2.4m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="191.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="010502001003" Mc="矩形柱" Xmtz="1．柱规格形状：矩形&#xD;&#xA;2．周长：2.4m以外&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C35" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="4.22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="010501006002" Mc="混凝土包柱脚" Xmtz="1．部位：包柱脚部位&#xD;&#xA;2．混凝土强度等级：C40细石混凝土无收缩高强灌浆料" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="010501006003" Mc="混凝土填实" Xmtz="1．部位：杯口基础与钢柱相交处&#xD;&#xA;2．做法：钢柱定位校正后,，底面及侧面用C40细石混凝土填实" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="010502002001" Mc="构造柱" Xmtz="1．位置：构造柱&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="27.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="010503001001" Mc="基础梁" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="78.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="37" Qdbm="010503002001" Mc="矩形梁" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="6.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="010503004001" Mc="圈梁" Xmtz="1．部位：反坎、门槛、水平系圈梁、电梯圈梁等&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="37.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="010503005001" Mc="过梁" Xmtz="1．部位：门窗洞口过梁&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="2.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="010504001001" Mc="直形墙" Xmtz="1．墙规格：200mm以内&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="60.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="WB010504003001" Mc="电梯井墙" Xmtz="1．墙规格：250mm以内&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30 防水混凝土，抗渗等级为P6" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="6.41" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="010505001001" Mc="有梁板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="556.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="010505001002" Mc="有梁板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30防水混凝土，抗渗等级为P6" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="516.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="010505003001" Mc="平板" Xmtz="1．部位：桁架楼承板&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="6.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="010505008001" Mc="雨篷板" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以伸出外墙部分的水平投影面积计算" Dw="m2" Sl="8.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="010506001001" Mc="直形楼梯" Xmtz="1．混凝土种类：商品混凝土&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="" Dw="m2" Sl="92.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="010507005001" Mc="扶手、压顶" Xmtz="1．部位：压顶&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C25" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="17.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="010507003001" Mc="地沟、电缆沟" Xmtz="1．部位：排水沟&#xD;&#xA;2．混凝土种类：商品混凝土&#xD;&#xA;3．混凝土强度等级：C20" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="2.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="010507001001" Mc="散水" Xmtz="1．基层处理：素土夯实，向外坡5%，夯实系数0.95&#xD;&#xA;2．混凝土强度等级：50厚C20细石混凝土随捣随抹,撒1:1水泥砂子压实赶光，150厚3:7灰土，宽出面层100&#xD;&#xA;3．从建筑边缘向外找坡5%,每隔6-10m设置一道伸缩缝。缝宽20mm,散水与外墙间设通缝,缝宽20mm,转角处设置45°缝,缝内填沥青胶泥。" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="169.10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="50" Qdbm="010507001002" Mc="坡道" Xmtz="1．基层处理：素土夯实&#xD;&#xA;2．混凝土强度等级：300厚1:2夯实砂石,压实系数不小于0.94&#xD;&#xA;3．随捣随抹,表面压出横道&#xD;&#xA;4．200厚C30混凝土&#xD;&#xA;5．30厚沥青混凝土面层碾压&#xD;&#xA;6．与室内地面间设缝,缝宽20mm,缝内填沥青砂浆" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="174.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="010515001001" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HPB300级钢&#xD;&#xA;2．钢筋规格：Φ6&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="2.875" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="010515001002" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HPB300级钢&#xD;&#xA;2．钢筋规格：Φ8&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.950" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="010515001003" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ6&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.262" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="010515001004" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ8&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="76.330" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="010515001005" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ10&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="27.396" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="010515001006" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ12&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="11.909" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="010515001007" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ14&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="1.871" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="010515001008" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ16&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="5.839" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="010515001009" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ18&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="15.361" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="010515001010" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ20&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="16.964" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="010515001011" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ22&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="28.427" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="010515001012" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ25&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="52.262" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="010516002001" Mc="预埋铁" Xmtz="1．钢材种类：预埋铁件制作&#xD;&#xA;2．铁件尺寸：角钢、钢板等预埋件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="7.036" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="010516003001" Mc="钢筋连接" Xmtz="1．连接方式：电渣压力焊" Gcnr="" Jsgz="按实际数量计算" Dw="个" Sl="1319" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="010516003002" Mc="钢筋连接" Xmtz="1．连接方式：直螺纹套筒连接&#xD;&#xA;2．规格：Φ16以上" Gcnr="" Jsgz="按实际数量计算" Dw="个" Sl="2106" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="WB010516004001" Mc="墙体拉结筋" Xmtz="1．钢筋种类：HRB300&#xD;&#xA;2．钢筋规格：Φ6" Gcnr="" Jsgz="按设计图示钢筋尺寸，以质量计算" Dw="t" Sl="3.010" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="WB010516005001" Mc="墙面钢板（丝）网" Xmtz="1．部位：两种不同基体交界处&#xA;2．钢筋网（钢丝网）种类、规格：不同材质交界处挂宽400mm的密纹钢丝网。钢丝网直径为0.9mm，钢丝网网孔尺寸为12.7mmX12.7mm" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="126.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="WB010516005002" Mc="墙面钢板（丝）网" Xmtz="1．钢筋网（钢丝网）种类、规格：楼梯间及人流密集通道的填充墙采用钢丝网砂浆面层加强，钢丝网直径0.9mm,钢丝网网孔尺寸为12.7mmx12.7mm" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="755.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="WB010516005003" Mc="墙面钢板（丝）网）" Xmtz="1．钢筋网（钢丝网）种类、规格：外墙面满铺&#xD;&#xA;2．耐碱玻纤网格布" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="921.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0106" Mc="金属结构工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="70" Qdbm="WB010603001001" Mc="钢柱" Xmtz="1．柱类型：钢柱&#xA;2．钢柱材质：Q355B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．含依附于钢柱上的牛腿、女儿墙钢柱、连接板、加劲板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="16.754" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="71" Qdbm="010604001001" Mc="钢梁" Xmtz="1．梁类型：钢梁&#xA;2．钢梁材质：Q355B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．含依附于钢梁上的连接板、加劲板等&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="" Dw="t" Sl="24.277" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="010606001001" Mc="钢支撑、钢拉条" Xmtz="1．类型：雨棚钢支撑、系杆等&#xD;&#xA;2．钢材材质：Q355B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;5．含依附于钢支撑上的连接板、加劲板、节点板等&#xD;&#xA;6．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="2.040" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="010606001002" Mc="钢支撑、钢拉条" Xmtz="1．类型：雨棚钢支撑、系杆等&#xD;&#xA;2．钢材材质：Q235B钢材&#xA;3．除锈形式：抛丸除锈&#xA;4．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;5．含依附于钢支撑上的连接板、加劲板、节点板等&#xD;&#xA;6．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.220" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="010606002001" Mc="钢檩条" Xmtz="1．檩条类型：屋面檩条、墙面檩条、几字檩、门梁、门柱、窗梁、窗柱等&#xD;&#xA;2．钢材材质：Q355B镀锌钢材&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．含依附于梁、柱上的檩托、节点板、加劲肋、隔板、肋板、加强板、连接件等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="29.494" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="010606001003" Mc="钢拉条" Xmtz="1．类型：屋面钢拉条、斜拉条、撑杆、隅撑等&#xD;&#xA;2．钢材材质：Q235B镀锌钢材&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．含依附于钢拉条上的连接板、加劲板、节点板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.260" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="010606001004" Mc="钢拉条" Xmtz="1．类型：墙面钢拉条、斜拉条、撑杆等&#xD;&#xA;2．钢材材质：Q235B&#xD;&#xA;3．普通螺栓应满足设计要求，综合考虑在报价中&#xD;&#xA;4．含依附于钢拉条上的连接板、加劲板、节点板等&#xD;&#xA;5．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="3.090" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="WB011405002001" Mc="金属构件油漆" Xmtz="1．油漆品种、刷漆遍数：环氧富锌(含锌量大于70%)底漆2遍&#xD;&#xA;2．所有非镀锌钢构件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="46.382" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="WB011405002002" Mc="金属构件油漆" Xmtz="1．油漆品种、刷漆遍数：环氧云铁中间涂料2遍&#xD;&#xA;2．所有非镀锌钢构件" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="46.382" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="WB011405002003" Mc="金属构件油漆" Xmtz="1．油漆品种、刷漆遍数：脂肪族聚氨酯面漆3遍&#xD;&#xA;2．所有非镀锌钢构件(防火时，面层不做)" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.570" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="010605001001" Mc="钢板楼板" Xmtz="1．部位：钢筋桁架楼层板&#xD;&#xA;2．楼承板型号：TD5-100&#xD;&#xA;3．楼板厚度：100mm&#xD;&#xA;4．含上弦钢筋、下弦钢筋、腹杆钢筋、底模钢板、侧边钢板包边等固定构件" Gcnr="" Jsgz="" Dw="m²" Sl="112.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="010606011001" Mc="钢天沟" Xmtz="1．类型：1.5mm厚304不锈钢天沟&#xD;&#xA;2．含构件现场倒运、构件微小变形的修理、临时加固、翻身就位、吊装、找正、焊接、连接板安装等一切费用" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.163" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="WB010606016001" Mc="高强螺栓" Xmtz="1．强度：10.9级高强螺栓&#xD;&#xA;2．规格：M20" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="WB010606017001" Mc="栓钉" Xmtz="1．规格型号：Φ19栓钉&#xD;&#xA;2．焊接后长度为100mm" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="728" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="011407005001" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：钢柱、柱间支撑&#xA;2．耐火极限：2.5h&#xD;&#xA;3．非膨胀型防火涂料，防火涂料厚度不小于50mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="902.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="011407005002" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：支撑防火墙、防火卷帘钢梁&#xA;2．耐火极限：3h&#xD;&#xA;3．非膨胀型防火涂料，防火涂料厚度不小于50mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="17.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="011407005003" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：楼面钢梁等&#xA;2．耐火极限：1.5h&#xD;&#xA;3．环氧类膨胀型防火涂料，防火涂料厚度≥5.0mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="177.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="011407005004" Mc="金属构件刷防火涂料" Xmtz="1．喷刷防火涂料构件名称：屋面梁、屋盖支撑、系杆等&#xA;2．耐火极限：1h&#xD;&#xA;3．膨胀型防火涂料，防火涂料厚度≥4.0mm&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="332.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="010605002001" Mc="钢板墙板" Xmtz="1．部位：压型钢板复合保温外墙&#xD;&#xA;2．钢材品种、规格：0.6mm厚双面镀铝锌压型钢板外侧墙板,，镀铝锌量每面镀铝锌量≥180g/㎡，漆膜:正面HDP,厚度25um;背面为PE烤漆,厚度10um&#xD;&#xA;3．透气层：0.5mm防水透气膜 &#xD;&#xA;4．复合板夹芯材料种类、规格：100mm厚玻璃棉，容重≥16kg/m³&#xD;&#xA;5．含附加檩条压型彩钢板窗台板、压顶、包角、包边等构件费用" Gcnr="" Jsgz="按设计图示尺寸，以铺挂面积计算" Dw="m2" Sl="2163.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="89" Qdbm="WB010902005001" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层品种、规格、厚度：0.3mm厚聚脂膜隔汽层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2163.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="010605002002" Mc="钢板墙板" Xmtz="1．部位：压型钢板内墙板&#xD;&#xA;2．钢材品种、规格：0.5厚双面镀铝锌压型钢板内侧墙板，镀铝锌量每面镀铝锌量≥150g/㎡，漆膜:PE烤漆,厚度20/5um&#xD;&#xA;3．含附加檩条压型彩钢板窗台板、包角、包边等构件费用" Gcnr="" Jsgz="按设计图示尺寸，以铺挂面积计算" Dw="m2" Sl="2163.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="WB011209016001" Mc="楼层防火带" Xmtz="1．部位：楼板与板墙交接处&#xD;&#xA;2．骨架材料种类、规格：200高防火岩棉防水透气膜包覆&#xD;&#xA;3．钢板厚度：1.5厚镀锌钢板承托板，防火胶封口，含彩钢收边件" Gcnr="" Jsgz="按设计图示尺寸以延长米计算" Dw="m" Sl="317.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="WB010605003001" Mc="钢结构雨棚" Xmtz="1．清单按水平投影面积计入&#xA;2．0.65mm厚中灰色压型钢板屋面上板，0.40mm厚中灰色细波纹钢板屋面下板&#xD;&#xA;3．含彩钢盖缝板、泛水板、彩板包边、板边处理、阴阳角、洞口收边、闭孔泡沫堵头、拉铆钉连接等" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="92.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="WB010605003002" Mc="钢结构雨棚" Xmtz="1．部位：小雨棚&#xD;&#xA;2．钢板厚度：0.6厚彩钢板+0.6厚彩钢板&#xD;&#xA;3．含彩钢盖缝板、泛水板、彩板包边、板边处理、阴阳角、洞口收边、闭孔泡沫堵头、拉铆钉连接等" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="WB010605003003" Mc="钢板屋面板" Xmtz="1．部位：压型钢板复合保温屋面&#xD;&#xA;2．钢板厚度：0.6厚镀锌压型彩钢板&#xD;&#xA;3．复合板夹芯材料种类、规格：100mm环保玻璃棉保温层,防火A级,容重不小于16kg/m³" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="123.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="95" Qdbm="010902001001" Mc="屋面卷材防水" Xmtz="1．防水层做法：1.5厚玻纤增强高分子防水卷材" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="123.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="WB010902005002" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层品种、规格、厚度：复合YH38高强度聚丙烯贴面" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="123.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="WB010516005004" Mc="钢板（丝）网" Xmtz="1．部位：钢板屋面&#xA;2．钢筋网（钢丝网）种类、规格：不锈钢丝网,钢丝直径1.2,网目为双向200x200" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="123.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0108" Mc="门窗工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="98" Qdbm="010804003001" Mc="成品钢质平开门" Xmtz="1．门名称：成品钢质平开门&#xA;2．门材质：镀锌钢框、粉末喷涂钢制门扇&#xA;3．钢门框壁厚不小于1.6mm,钢门扇面板壁厚不小于1.0mm&#xD;&#xA;4.五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="" Dw="m2" Sl="31.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="010802003001" Mc="钢质防火门" Xmtz="1．门名称：成品钢质甲级防火门&#xD;&#xA;2．门材质：钢框或镀锌钢框、钢质防火门扇&#xD;&#xA;3．观察窗：防火玻璃&#xD;&#xA;4．钢门框壁厚不小于1.6mm,钢门扇面板壁厚不小于1.0mm&#xD;&#xA;5.五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、防火合页、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="28.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="010802003002" Mc="钢质防火门" Xmtz="1．门名称：成品钢质乙级防火门&#xD;&#xA;2．门材质：镀锌钢框、钢质防火门扇&#xD;&#xA;3．观察窗：防火玻璃&#xD;&#xA;4．钢门框壁厚不小于1.6mm,钢门扇面板壁厚不小于1.0mm&#xD;&#xA;5.五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、防火合页、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="24.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="010802003003" Mc="钢质防火门" Xmtz="1．门名称：成品钢质丙级防火门&#xD;&#xA;2．门材质：钢门框壁厚不小于1.6mm,钢门扇面板壁厚不小于1.0mm&#xD;&#xA;3．五金品种、规格：包含门套、顺序器、液压闭门器、锁具、不锈钢门把手、防火合页、门吸、配套铰链等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="4.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="010801001001" Mc="木质门" Xmtz="1．门代号及洞口尺寸：成品木门&#xD;&#xA;2．实木门框、模压木质门扇&#xD;&#xA;3．门下方设铝合金百叶&#xD;&#xA;4．五金品种、规格：包含门套、锁具、门把手等所有五金配件" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="4.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="010803001001" Mc="电动钢制卷帘门（带防风杆）" Xmtz="1．门代号及洞口尺寸：电动钢制卷帘门&#xD;&#xA;2．门材质：镀锌钢框、1.0厚单层不锈钢&#xD;&#xA;3．卷帘门开启速度速度0.5M/S&#xD;&#xA;4．一层及平台层所有外立面卷帘门均设置，3m≤门宽≤4.7m，5厚80X100Q355镀锌矩形钢管，3m≤门宽≤4.7m，5厚80X100Q355镀锌矩形钢管，安全扣镀锌管φ30*3.5  4个，防风扣镀锌管120*120*3，吊装固定扣φ10钢筋锚入混凝土100&#xD;&#xA;5．五金要求：含安装、打胶、配套所有五金配件&#xD;&#xA;6．清单工程量为卷帘门洞口尺寸（包括卷帘箱高度），卷帘箱及上部封堵、导轨等所有配件，投标人自行综合考虑在报价内" Gcnr="" Jsgz="按设计图纸安装高度乘以门的实际宽度，以面积计算" Dw="m2" Sl="57.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="010803002001" Mc="电动特级防火卷帘门" Xmtz="1．门代号及洞口尺寸：特级防火卷帘门&#xD;&#xA;2．门材质：镀锌钢框，2MM全无机特级防火卷帘片,双层间距450MM&#xD;&#xA;3．五金要求：含安装、打胶、配套所有五金配件&#xD;&#xA;4．清单工程量为卷帘门洞口尺寸（包括卷帘箱高度），卷帘箱及上部封堵、导轨等所有配件，投标人自行综合考虑在报价内" Gcnr="" Jsgz="按设计图纸安装高度乘以门的实际宽度,以面积计算" Dw="m2" Sl="64.95" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="WB010803003001" Mc="金属卷闸门电动装置" Xmtz="1．启动装置品种、规格：电动钢制卷帘门" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="WB010803003002" Mc="防火卷帘门电动装置" Xmtz="1．启动装置品种、规格：电动防火卷帘门" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="010807001001" Mc="金属窗 " Xmtz="1．窗代号及洞口尺寸：80系列断热铝合金中空玻璃窗&#xD;&#xA;2．窗材质：铝合金外窗主型材主要受力部位基材截面最小实测壁厚不应小于1.8mm,内窗主型材最小实测壁厚小于1.4mm，隔热尼龙条,宽度≥24mm（表面粉末喷涂）&#xD;&#xA;3．玻璃品种、厚度：6透明+12空气+6透明钢化安全玻璃（卫生间采用磨砂玻璃，消防救援窗口玻璃应易于破碎）&#xD;&#xA;4．含五金配件、消防救援标识、可开启扇设置限位器、增加防脱落铰链或其他防脱措施由门窗厂家提供" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="45.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="108" Qdbm="010807002001" Mc="金属防火窗" Xmtz="1．窗代号及洞口尺寸：乙级防火窗&#xD;&#xA;2．玻璃品种、厚度：16厚A类防火玻璃&#xD;&#xA;3．防火门窗做法参《12J609防火门窗》&#xD;&#xA;4．含五金配件，可开启扇增加防脱落铰链或其他防脱措施由门窗厂家提供" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="3.36" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="WB010801008001" Mc="五金安装" Xmtz="1．手动开启装置" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="010807003001" Mc="成品铝合金防雨百页窗" Xmtz="1．窗名称：成品隔热铝合金防雨百页窗&#xA;2．窗材质：百叶叶片的厚度要求不小于2厚&#xD;&#xA;3．表面粉末喷涂，含防鼠防虫网" Gcnr="" Jsgz="" Dw="m2" Sl="6.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="111" Qdbm="010807003002" Mc="纱窗" Xmtz="1．窗材质：防虫纱窗" Gcnr="" Jsgz="按设计图示洞口尺寸，以面积计算" Dw="m2" Sl="58.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="112" Qdbm="010808001001" Mc="防火卷帘门门套" Xmtz="1．面层材料品种、规格：12mm厚双层防火板面层，无机涂料面层(两底两面）&#xD;&#xA;2．50*100x3、50*100*3镀锌方管骨架，缝隙采用防火岩棉填塞&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以展开面积计算" Dw="m2" Sl="20.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0109" Mc="屋面及防水工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="113" Qdbm="010902003001" Mc="屋面刚性层" Xmtz="1．刚性层厚度：40厚C25配筋细石混凝土(掺减水剂,) &#xD;&#xA;2．钢筋规格、型号：双向配Φ6@150,每6米设缝,密封胶嵌缝" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2310.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="114" Qdbm="WB010902005003" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层做法：10厚低强度等级砂浆隔离层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2310.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="115" Qdbm="010902001002" Mc="屋面卷材防水" Xmtz="1．卷材品种、规格、厚度：1.5mm厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2378.32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="116" Qdbm="WB010902005004" Mc="屋面找平层 " Xmtz="1．找平层厚度、砂浆配合比：20厚1:3水泥砂浆找平（掺入聚丙烯）" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2310.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="117" Qdbm="011001001001" Mc="保温隔热屋面" Xmtz="1．保温隔热材料品种、规格、厚度：最薄处30厚LC5.0轻集料混凝土2%找坡(结构找坡无此层) " Gcnr="" Jsgz="1.按设计图示尺寸，以面积计算2.按设计图示尺寸，以体积计算" Dw="m2" Sl="104.35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="118" Qdbm="011001001002" Mc="保温隔热屋面" Xmtz="1．保温隔热材料品种、规格、厚度：70厚高密度挤塑聚苯板(B1级)" Gcnr="" Jsgz="1.按设计图示尺寸，以面积计算2.按设计图示尺寸，以体积计算" Dw="m2" Sl="2310.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="119" Qdbm="010902002001" Mc="屋面涂膜防水" Xmtz="1．防水膜品种：2厚聚合物水泥基防水涂料一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2310.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="120" Qdbm="011201001001" Mc="墙面一般抹灰" Xmtz="1．部位：外墙面&#xD;&#xA;2．底层厚度、砂浆配合比：5mm厚聚合物水泥防水砂浆" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1651.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="121" Qdbm="010903002001" Mc="墙面涂膜防水" Xmtz="1．部位：外墙面&#xD;&#xA;2．涂膜厚度、遍数：2mm厚聚合物水泥防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1651.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="122" Qdbm="010904002002" Mc="楼（地）面涂膜防水" Xmtz="1．部位：卫生间楼地面&#xD;&#xA;2．涂膜厚度、遍数：1.5mm厚聚氨酯防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="46.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="123" Qdbm="010904002003" Mc="楼（地）面涂膜防水" Xmtz="1．部位：卫生间楼地面&#xD;&#xA;2．涂膜厚度、遍数：2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="46.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="124" Qdbm="010903002002" Mc="墙面涂膜防水" Xmtz="1．部位：卫生间墙面&#xD;&#xA;2．涂膜厚度、遍数：1.5厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="152.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="125" Qdbm="010903002003" Mc="天棚涂膜防水" Xmtz="1．部位：卫生间天棚&#xD;&#xA;2．涂膜厚度、遍数：1.2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="56.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="126" Qdbm="010904002004" Mc="楼（地）面涂膜防水" Xmtz="1．部位：地面&#xD;&#xA;2．涂膜厚度、遍数：1.5mm厚聚氨酯防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="22.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="127" Qdbm="010904002005" Mc="楼（地）面涂膜防水" Xmtz="1．部位：地面&#xD;&#xA;2．涂膜厚度、遍数：2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="22.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="128" Qdbm="010904003001" Mc="楼（地）面砂浆防水（防潮）" Xmtz="1．部位：用于报警阀间等无腐蚀性普通室内排水沟&#xD;&#xA;2．防水层做法：1:2.5防水砂浆,最薄处15厚" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="129" Qdbm="010904002006" Mc="楼（地）面涂膜防水" Xmtz="1．部位：雨棚&#xD;&#xA;2．涂膜厚度、遍数：2厚聚合物水泥基防水涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="11.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="130" Qdbm="010904003002" Mc="楼（地）面砂浆防水（防潮）" Xmtz="1．部位：雨棚、风井顶板&#xD;&#xA;2．防水层做法：20厚1:2.5防水砂浆" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="14.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="131" Qdbm="011101006001" Mc="水泥砂浆楼地面找平层 " Xmtz="1．部位：电梯基坑等底板&#xD;&#xA;2．找平层厚度、砂浆配合比：20厚DS M15砂浆(1:3水泥砂浆)找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="30.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="132" Qdbm="010904001001" Mc="楼（地）面卷材防水" Xmtz="1．部位：电梯基坑等底板&#xD;&#xA;2．卷材品种、规格、厚度：1.5厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="30.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="133" Qdbm="WB011101007001" Mc="细石混凝土找平层 " Xmtz="1．部位：电梯基坑等底板&#xD;&#xA;2．找平层厚度、混凝土强度等级：50厚C20细石砼保护层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="30.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="134" Qdbm="010903003001" Mc="墙面砂浆防水（防潮）" Xmtz="1．部位：电梯基坑等侧壁&#xD;&#xA;2．防水层做法：20厚DS M15砂浆(1:3水泥砂浆)找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="44.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="135" Qdbm="010903001001" Mc="墙面卷材防水" Xmtz="1．部位：电梯基坑等侧壁&#xD;&#xA;2．卷材品种、规格、厚度：1.5厚热塑性聚烯烃(TPO)防水卷材两道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="44.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="136" Qdbm="010903005001" Mc="墙面防水保护层" Xmtz="1．部位：电梯基坑等侧壁&#xD;&#xA;2．保护层品种、规格、厚度：30厚挤塑聚苯板保护层,用建筑胶粘贴&#xD;&#xA;3．DP M15砂浆局部找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="44.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="137" Qdbm="010904004001" Mc="楼（地）面变形缝" Xmtz="1．嵌缝材料种类：硬质岩棉填缝,厚度200,外面弹性防火材料封堵&#xD;&#xA;2．止水带材料种类：1.5厚三元乙丙防水卷材&#xD;&#xA;3．盖缝材料：6厚不锈钢板，角钢L70x45x4，PU橡胶" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="18.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="138" Qdbm="010903004001" Mc="外墙面变形缝" Xmtz="1．嵌缝材料种类：内填岩棉&#xD;&#xA;2．止水带材料种类：橡胶止水带&#xD;&#xA;3．盖缝材料：0.6厚镀铝锌彩钢板" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="26.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="139" Qdbm="010904004002" Mc="顶棚变形缝" Xmtz="1．盖缝材料：1厚铝合金盖板&#xD;&#xA;2．防护材料种类：1.5厚镀锌钢板承托板，膨胀螺栓，弹性胶条，铝锚夹" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="18.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="140" Qdbm="ZB010902008001" Mc="屋面变形缝" Xmtz="1．嵌缝材料种类：内填岩棉，聚乙烯泡沬塑料棒&#xD;&#xA;2．盖缝材料：1厚铝合金盖板，1厚铝合金盖板" Gcnr="" Jsgz="按设计图示以长度计算。" Dw="m" Sl="18.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="141" Qdbm="010904004003" Mc="楼（地）面变形缝" Xmtz="1．部位：楼梯滑动支座&#xD;&#xA;2．嵌缝材料种类：缝宽50mm聚苯板填充、钢板之间满铺石墨粉" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="12.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0110" Mc="保温、隔热、防腐工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="142" Qdbm="011001003001" Mc="保温隔热墙面" Xmtz="1．保温隔热部位：外墙面&#xD;&#xA;2．保温隔热材料品种、规格及厚度：50厚岩棉板&#xD;&#xA;3．增强网及抗裂防水砂浆种类：5厚聚合物抗裂砂浆，热镀锌钢网丝&#xD;&#xA;4．锚栓固定（锚栓数量不应小于 6 个/m2。在墙面阴、阳角等部位应适当增加锚栓数量）&#xD;&#xA;5．岩棉板外保温系统参图集10J121第附录3-1~附录3-9页执行" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="921.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0111" Mc="楼地面装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="143" Qdbm="WB010101007001" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="2124.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="144" Qdbm="010404001002" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="637.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="145" Qdbm="010404001003" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="212.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="146" Qdbm="WB010902005005" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层做法：0.5厚双层PE膜" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2124.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="147" Qdbm="011101003001" Mc="混凝土楼地面 " Xmtz="1．面层厚度、混凝土强度等级：200厚C30钢筋混凝土抹平(内配φ10@150双层双向钢筋)" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2124.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="148" Qdbm="WB011101013001" Mc="混凝土地坪密封固化剂面层" Xmtz="1．固化剂用量：表面涂刷混凝土固化剂" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2124.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="149" Qdbm="WB011101008001" Mc="金刚砂耐磨地坪" Xmtz="1．面层厚度、骨料用量：待混凝土面层初凝,面撒水泥原色金刚砂(用量6kg/m2)" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2124.33" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="150" Qdbm="WB010101007002" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="46.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="151" Qdbm="010404001004" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="14.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="152" Qdbm="010404001005" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="4.68" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="153" Qdbm="WB011101007002" Mc="细石混凝土找平层 " Xmtz="1．找平层厚度、混凝土强度等级：最薄处30厚C20细石混凝土找坡层,向地漏找1%坡,随打随抹平。地漏四周及管根部用DS M15砂浆抹小八角字&#xD;&#xA;2．界面剂一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="46.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="154" Qdbm="011102003001" Mc="块料楼地面" Xmtz="1．面层材料品种、规格、颜色：5~10mm厚600x600mm防滑地砖，DTG砂浆擦缝&#xD;&#xA;2．结合层厚度、砂浆配合比或粘接剂种类：20厚1:3干硬性水泥砂浆结合层,表面撒水泥粉&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="46.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="155" Qdbm="WB010101007003" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="22.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="156" Qdbm="010404001006" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="6.73" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="157" Qdbm="010404001007" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="2.24" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="158" Qdbm="WB011101007003" Mc="细石混凝土找平层 " Xmtz="1．找平层厚度、混凝土强度等级：最薄处30厚C20细石混凝土找坡层,向地漏找1%坡,随打随抹平。地漏四周及管根部用DS M15砂浆抹小八角字&#xD;&#xA;2．界面剂一道" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="22.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="159" Qdbm="WB011101007004" Mc="细石混凝土保护层 " Xmtz="1．找平层厚度、混凝土强度等级：35厚C20细石混凝土保护层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="22.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="160" Qdbm="011101001001" Mc="水泥砂浆楼地面" Xmtz="1．面层厚度、砂浆配合比：20厚DS M20砂浆(1:2.5水泥砂浆)面层,表面撒适量水泥粉抹压平整" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="22.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="161" Qdbm="WB010101007004" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="17.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="162" Qdbm="010404001008" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="5.10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="163" Qdbm="010404001009" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="1.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="164" Qdbm="WB010902005006" Mc="隔汽(离)层" Xmtz="1．隔汽（离）层做法：0.5厚双层PE膜" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="17.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="165" Qdbm="011101003002" Mc="混凝土楼地面 " Xmtz="1．面层厚度、混凝土强度等级：100厚C20混凝土" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="17.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="166" Qdbm="WB011101013002" Mc="混凝土地坪密封固化剂面层" Xmtz="1．混凝土固化渗透剂并抛光至1000mu" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="17.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="167" Qdbm="WB011101013003" Mc="混凝土地坪密封固化剂面层" Xmtz="1．固化剂用量：渗透型锂基液体固化剂抛光至1000mu" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2355.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="168" Qdbm="WB011101008002" Mc="金刚砂耐磨地坪" Xmtz="1．面层厚度、骨料用量：混凝土面层初凝,面撒水泥原色金刚砂(用量6kg/m2)" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="2355.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="169" Qdbm="WB011101013004" Mc="混凝土地坪密封固化剂面层" Xmtz="1．固化剂用量：混凝土固化渗透剂并抛光至1000mu" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="70.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="170" Qdbm="011101003003" Mc="混凝土楼地面 " Xmtz="1．面层厚度、混凝土强度等级：100厚C20混凝土" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="70.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="171" Qdbm="WB010101007005" Mc="原土打夯" Xmtz="1．素土夯实，夯实系数≥0.94" Gcnr="" Jsgz="按设计规定的尺寸，以面积计算" Dw="m2" Sl="39.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="172" Qdbm="010404001010" Mc="砂夹石垫层" Xmtz="1．厚度：300mm厚&#xD;&#xA;2．材料品种及比例：300厚级配碎石,压实系数≥0.97 " Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="11.87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="173" Qdbm="010404001011" Mc="垫层" Xmtz="1．厚度：100mm&#xD;&#xA;2．材料品种及比例：C20混凝土垫层，随捣随抹" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="3.96" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="174" Qdbm="011102003002" Mc="块料楼地面" Xmtz="1．面层材料品种、规格、颜色：8mm厚地砖面层,DTG砂浆擦缝 &#xD;&#xA;2．结合层厚度、砂浆配合比或粘接剂种类： 5厚DTA砂浆结合层&#xD;&#xA;3．20厚DS M20砂浆(1:2.5水泥砂浆)找平层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="39.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="175" Qdbm="011106002001" Mc="块料楼梯面层 " Xmtz="1．面层材料品种、规格、颜色：8mm厚地砖面层,DTG砂浆擦缝 &#xD;&#xA;2．结合层厚度、砂浆配合比或粘接剂种类： 5厚DTA砂浆结合层&#xD;&#xA;3．20厚DS M20砂浆(1:2.5水泥砂浆)找平层，界面剂一道&#xD;&#xA;4．含楼梯防滑条" Gcnr="" Jsgz="按设计图示尺寸，以楼梯（包括踏步、休息平台及≤500mm的楼梯井）水平投影面积计算" Dw="m2" Sl="92.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="176" Qdbm="011105001001" Mc="水泥砂浆踢脚线 " Xmtz="1．踢脚线高度：120mm&#xD;&#xA;2．面层厚度、砂浆配合比：10厚DP M15砂浆(1:3水泥砂浆)抹光&#xD;&#xA;3．底层厚度、砂浆配合比：8厚DP M5砂浆(1:1水泥石灰砂浆)打底并划出纹道&#xD;&#xA;4．基层处理：界面剂一道" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="640.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="177" Qdbm="011105003001" Mc="块料踢脚线 " Xmtz="1．踢脚线高度：120mm&#xD;&#xA;2．面层材料品种、规格、颜色：10mm厚釉面砖,DTG砂浆勾缝&#xD;&#xA;3．粘贴层厚度、材料种类：5mm厚DTA砂浆粘贴;&#xD;&#xA;4．10mm厚DP M5砂浆1:1:6水泥石灰砂浆)打底并划出纹道;&#xD;&#xA;5．界面剂1道" Gcnr="" Jsgz="按设计图示尺寸，以长度计算" Dw="m" Sl="165.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0112" Mc="墙、柱面装饰与隔断、幕墙工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="178" Qdbm="011201001002" Mc="墙面一般抹灰" Xmtz="1．部位：砖胎膜&#xD;&#xA;2．底层厚度、砂浆配合比：20厚1:2.5水泥砂浆" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="44.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="179" Qdbm="011201001003" Mc="墙面一般抹灰" Xmtz="1．部位：外墙面1&#xD;&#xA;2．底层厚度、砂浆配合比：10厚1:3水泥砂浆找平(加5%防水剂)&#xD;&#xA;3．专用砂浆或界面剂一道甩毛&#xD;&#xA;4．水泥砂浆中加入杜拉纤维,增强抗裂性能" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="921.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="180" Qdbm="011201001004" Mc="墙面一般抹灰" Xmtz="1．部位：外墙面2&#xD;&#xA;2．底层厚度、砂浆配合比：9厚1:3水泥砂浆找平(加5%防水剂)&#xD;&#xA;3．专用砂浆或界面剂一道甩毛&#xD;&#xA;4．水泥砂浆中加入杜拉纤维,增强抗裂性能" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="730.43" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="181" Qdbm="011201001005" Mc="墙面一般抹灰" Xmtz="1．部位：内墙面1&#xD;&#xA;2．底层厚度、砂浆配合比：8厚DP M5砂浆(1:1:6水泥石灰膏砂浆)打底抹平&#xD;&#xA;3．界面剂一道&#xD;&#xA;4．用修补砂浆局部修补墙面,DP砂浆勾实接缝并拉毛" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4021.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="182" Qdbm="011201001006" Mc="墙面一般抹灰" Xmtz="1．部位：内墙面2&#xD;&#xA;2．挂金属网,8厚DP M20(1:2.5水泥砂浆)压实抹平&#xD;&#xA;3．底层厚度、砂浆配合比：6厚DP M5砂浆(1:1:6水泥石灰膏砂浆)打底扫毛或划出纹道 &#xD;&#xA;4．界面剂一道&#xD;&#xA;5．用修补砂浆局部修补墙面,DP砂浆勾实接缝并拉毛" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="152.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="183" Qdbm="011204003001" Mc="块料墙面" Xmtz="1．部位：卫生间墙面&#xD;&#xA;2．面层材料品种、规格、品牌、颜色：10厚300*600陶瓷墙砖&#xD;&#xA;3．结合层材料种类：5厚DTA砂浆&#xD;&#xA;4．缝宽、嵌缝材料种类：白水泥擦缝 " Gcnr="" Jsgz="按设计图示尺寸，以镶贴表面积计算" Dw="m2" Sl="152.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0113" Mc="天棚工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="184" Qdbm="011301001001" Mc="天棚清理" Xmtz="1．板底原浆抹平，表面清扫干净" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="6623.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="185" Qdbm="011301001002" Mc="天棚抹灰" Xmtz="1．部位：混凝土雨棚&#xD;&#xA;2．抹灰厚度、材料种类：7厚水泥纸筋石灰砂浆打底，5厚水泥细纸筋石灰粉面" Gcnr="" Jsgz="按设计图示尺寸，以水平投影面积计算" Dw="m2" Sl="9.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="186" Qdbm="WB011302005001" Mc="硅酸钙板吊顶" Xmtz="1．部位：吊顶1&#xD;&#xA;2．面层材料品种、规格：12厚硅酸钙板面层,规格600x600&#xD;&#xA;3．吊顶形式、吊杆规格、高度：φ6钢筋吊杆,双向中距≤1200,吊杆上部与板底预留吊环(勾)或膨胀螺栓固定，钢筋混凝土楼板内预留φ8钢筋吊环(勾),或在板底钻孔固定镀锌膨胀螺栓间距≤1200&#xD;&#xA;4．龙骨：T型次龙骨,间距600,用吊件与主龙骨连接 ，T型主龙骨,间距≤1200,用垂直吊挂件或卡簧式吊件与钢筋吊杆连接后找平&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以展开面积计算" Dw="m2" Sl="73.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="187" Qdbm="WB011302005002" Mc="铝合金方板扣板吊顶" Xmtz="1．部位：吊顶2&#xD;&#xA;2．面层材料品种、规格：0.8mm铝合金方板600*600mm&#xD;&#xA;3．龙骨：与安装型式配套的专用上层主龙骨,间距≤1200用吊件与钢筋吊杆联结后找平 ，与铝合金方板配套的专用下层副龙骨联结,间距≤600 &#xD;&#xA;4．吊顶形式、吊杆规格、高度：Φ6钢筋吊杆,双向中距≤1200,吊杆上部与预留钢筋吊环固定&#xD;&#xA;5．板内预留Φ8钢筋吊环双向中距≤1200;" Gcnr="" Jsgz="按设计图示尺寸以展开面积计算" Dw="m2" Sl="47.38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0114" Mc="油漆、涂料、裱糊工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="188" Qdbm="011406003001" Mc="满刮腻子" Xmtz="1．部位：内墙1（含室内柱梁）&#xD;&#xA;2．刮腻子遍数：3厚耐水腻子分遍找平" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4021.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="189" Qdbm="011406001001" Mc="抹灰面油漆" Xmtz="1．部位：内墙1（含室内柱梁）&#xD;&#xA;2．油漆品种、刷漆遍数：无机涂料二遍面层涂料，涂饰一遍底层涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="4021.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="190" Qdbm="011406003002" Mc="满刮腻子" Xmtz="1．部位：顶棚1&#xD;&#xA;2．刮腻子遍数：3厚耐水腻子分遍找平" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6472.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="191" Qdbm="011406001002" Mc="抹灰面油漆" Xmtz="1．部位：顶棚1&#xD;&#xA;2．油漆品种、刷漆遍数：无机涂料二遍面层涂料，涂饰一遍底层涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="6472.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="192" Qdbm="WB011406001001" Mc="外墙涂料" Xmtz="1．部位：外墙（含栏板、节点及外立面水管等）&#xD;&#xA;2．基层类型：外墙耐水腻子2道, 打磨平整&#xD;&#xA;3．油漆品种、刷漆遍数：外墙涂料饰面（一底两面，罩面漆一遍）" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="1651.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0115" Mc="其他装饰工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="193" Qdbm="011503001001" Mc="楼梯栏杆" Xmtz="1．部位：楼梯栏杆&#xD;&#xA;2．高度：900mm&#xD;&#xA;3．做法：φ51*3不锈钢管立柱，φ63*1.5不锈钢管扶手，φ25*1.0不锈钢管立杆，φ38*1.0不锈钢管横杆&#xD;&#xA;4．201不锈钢法兰，预埋件参22J403-1  M3/5-19" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="30.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="194" Qdbm="011503001002" Mc="楼梯栏杆" Xmtz="1．部位：楼梯栏杆&#xD;&#xA;2．高度：1100mm&#xD;&#xA;3．做法：φ51*3不锈钢管立柱，φ63*1.5不锈钢管扶手，φ25*1.0不锈钢管立杆，φ38*1.0不锈钢管横杆&#xD;&#xA;4．201不锈钢法兰，预埋件参22J403-1  M3/5-19" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="3.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="195" Qdbm="011503001003" Mc="可拆卸式不锈钢防护栏杆" Xmtz="1．部位：吊装口卷帘门&#xD;&#xA;2．高度：1100mm&#xD;&#xA;3．扶手材料种类、规格、品牌：φ50x1.5不锈钢管&#xD;&#xA;4．栏杆材料种类、规格、品牌：φ50x1.5不锈钢管立柱，φ30*1.5不锈钢管立杆&#xD;&#xA;5．固定配件种类：不锈钢防护栏套管φ80*2.0" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="6.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="196" Qdbm="011503001004" Mc="吊装口防护栏" Xmtz="1．部位：吊装口卷帘门上口100mm&#xD;&#xA;2．扶手材料种类、规格、品牌：DN60*3防撞栏，黑黄色警示漆&#xD;&#xA;" Gcnr="" Jsgz="按设计图示，以扶手中心线长度（包括弯头长度）计算" Dw="m" Sl="6.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="197" Qdbm="040205017001" Mc="防撞柱" Xmtz="1．部位：室内防撞柱&#xD;&#xA;2．高度：高出地面600mm&#xD;&#xA;3．规格、型号：φ80钢管满灌C15砼，外刷黄黑漆（两遍）&#xD;&#xA;4．柱脚C25砼浇筑，预埋300*300*8钢板，M16*150膨胀螺栓固定" Gcnr="" Jsgz="" Dw="个" Sl="40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="198" Qdbm="040205017002" Mc="防撞柱" Xmtz="1．部位：室外防撞柱&#xD;&#xA;2．高度：高出地面600mm&#xD;&#xA;3．规格、型号：φ80钢管满灌C15砼，外刷黄黑漆（两遍）&#xD;&#xA;4．柱脚C25砼浇筑，预埋400*400*8钢板，φ12钢筋焊接固定" Gcnr="" Jsgz="" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="199" Qdbm="ZB010101001001" Mc="排水沟盖板" Xmtz="1．材料种类：40厚不锈钢(玻璃钢)格栅盖板板&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m2" Sl="1.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="200" Qdbm="ZB010101001002" Mc="线性截水槽" Xmtz="1．部位：吊装口&#xD;&#xA;2．规格、材质：1厚304#不锈钢u型槽" Gcnr="" Jsgz="" Dw="m" Sl="14.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="201" Qdbm="WB011209008001" Mc="铝板压顶" Xmtz="1．部位：屋面女儿墙&#xD;&#xA;2．金属板材品种、规格、颜色：3mm厚铝板&#xD;&#xA;3．嵌缝材料:泡沫棒、硅酮耐候胶" Gcnr="" Jsgz="按设计图示尺寸，以展开面积计算" Dw="m2" Sl="108.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="202" Qdbm="040205019001" Mc="成品塑胶缓冲垫" Xmtz="1．部位：吊装口&#xD;&#xA;2．材料品种：成品塑胶缓冲垫,凸出外墙50&#xD;&#xA;3．规格、型号：350宽塑胶缓冲垫（可用道路减速带制作）&#xD;&#xA;4．1.0mm厚铝板(成品)泛水件密封胶封严水泥钉或射钉@500镀锌垫片20x20x0.7" Gcnr="" Jsgz="按设计图示以长度计算" Dw="m" Sl="6.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="203" Qdbm="ZB010101001003" Mc="挡鼠板" Xmtz="1．名称：挡鼠板&#xD;&#xA;2．12厚防火木板,h=600mm，卡槽(6厚扁钢)高600mm,预埋件参06J403-1 M2/161" Gcnr="" Jsgz="" Dw="m2" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="204" Qdbm="011505001001" Mc="大便蹲位" Xmtz="1．部位：大便蹲位&#xD;&#xA;2．做法参16J914-1页XT18节点1" Gcnr="" Jsgz="按设计图示尺寸，以台面展开面积计算，不扣除孔洞、挖弯、削角所占面积" Dw="m2" Sl="10.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="205" Qdbm="011210005001" Mc="成品隔断" Xmtz="1．部位：卫生间隔断、小便斗隔断&#xD;&#xA;2．隔断材料品种、规格、颜色：32mm厚复合树脂板隔断&#xD;&#xA;3．配件品种、规格：含合页、配套显示门锁&#xD;&#xA;4．参16J914-1页XT9" Gcnr="" Jsgz="按设计图示框外围尺寸，以面积计算" Dw="m2" Sl="59.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="206" Qdbm="011505001002" Mc="洗漱台" Xmtz="1．柜体规格：20mm人造大理石台面台面&#xD;&#xA;2．五金种类、规格：包含五金等&#xD;&#xA;3．参16J914-1页XT11相关做法" Gcnr="" Jsgz="按设计图示尺寸，以台面展开面积计算，不扣除孔洞、挖弯、削角所占面积" Dw="m2" Sl="1.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="207" Qdbm="011505010001" Mc="镜面玻璃(卫生间）" Xmtz="1．镜面玻璃品种、规格：5mm镀铝膜银镜面镜&#xD;&#xA;2．高1200mm，镜底距地1200mm,黑色拉丝不锈钢窄边框，安装做法参16J914-1页4/XT25" Gcnr="" Jsgz="" Dw="m2" Sl="2.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="208" Qdbm="ZB010101001004" Mc="溢流口" Xmtz="1．名称：溢水口" Gcnr="" Jsgz="" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="209" Qdbm="ZB010101001005" Mc="簸箕" Xmtz="1．规格、材质：500x500x40mmC20细石混凝土板配6@100X100" Gcnr="" Jsgz="" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="210" Qdbm="ZB010101001006" Mc="电梯召唤盒预留洞" Xmtz="1．电梯召唤盒预留洞" Gcnr="" Jsgz="" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="211" Qdbm="ZB010101001007" Mc="电梯吊钩" Xmtz="1．电梯吊钩" Gcnr="" Jsgz="" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="212" Qdbm="ZB010101001008" Mc="屋面出入口" Xmtz="1．部位：屋面出入口&#xD;&#xA;2．C25混凝土踏步&#xD;&#xA;3．20mm厚1:2防水水泥砂浆粉刷" Gcnr="" Jsgz="" Dw="m2" Sl="0.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="213" Qdbm="ZB010101001009" Mc="电梯口包边" Xmtz="1．部位：电梯口包边&#xD;&#xA;2．10厚光面钢板,面层包1.4不锈钢板&#xD;&#xA;3．6#槽钢骨架@300，膨胀螺丝固定" Gcnr="" Jsgz="" Dw="m2" Sl="8.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="214" Qdbm="ZB010101001010" Mc="防火封堵" Xmtz="1．名称：墙体防火封堵节点一&#xD;&#xA;2．部位：配电房、消控室、楼梯间、弱电间、送排风机房等有防火需求设备用房间&#xD;&#xA;3．材料种类：9厚纤维增强硅酸盐板75厚岩棉9厚纤维增强硅酸盐板&#xD;&#xA;4．附加龙骨，防火岩棉封填密实，50X50镀锌钢板角件，密封膏" Gcnr="" Jsgz="" Dw="m2" Sl="133.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="215" Qdbm="WB010902006001" Mc="屋面排气管" Xmtz="1．排气管品种、规格：50镀锌钢管排期管&#xD;&#xA;2．4厚钢板环与钢管焊接&#xD;&#xA;3．参12J201第A21页" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="0117" Mc="措施项目" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="216" Qdbm="WB011701010001" Mc="单层轻钢厂房脚手架" Xmtz="1．搭设部位：部位：梁柱、屋面板等水平结构&#xD;&#xA;2．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="1.柱梁、屋面瓦等水平结构安装按厂房水平投影面积计算2.墙板、门窗、雨篷等竖向结构按厂房垂直投影面积计算" Dw="m2" Sl="135.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="217" Qdbm="WB011701010002" Mc="单层轻钢厂房脚手架" Xmtz="1．搭设部位：墙板、门窗、雨篷等竖向结构&#xD;&#xA;2．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="1.柱梁、屋面瓦等水平结构安装按厂房水平投影面积计算2.墙板、门窗、雨篷等竖向结构按厂房垂直投影面积计算" Dw="m2" Sl="2163.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="218" Qdbm="011701002001" Mc="外脚手架" Xmtz="1．搭设方式：外脚手架（含电梯井）&#xA;2．脚手架材质：钢管脚手架&#xD;&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="2839.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="219" Qdbm="011701003001" Mc="里脚手架" Xmtz="1．搭设方式：内墙砌筑脚手架、独立柱梁&#xA;2．脚手架材质：钢管脚手架&#xD;&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="4326.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="220" Qdbm="011701006001" Mc="装饰满堂脚手架" Xmtz="1．搭设方式：装饰满堂脚手架&#xA;2．脚手架材质：钢管脚手架&#xD;&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="4470.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="221" Qdbm="011701006002" Mc="基础脚手架" Xmtz="1．搭设方式：：基础脚手架&#xD;&#xA;2．脚手架材质：钢管脚手架&#xA;3．投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="" Dw="m2" Sl="449.05" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="222" Qdbm="011702001001" Mc="基础垫层-模板" Xmtz="1．基础类型：基础垫层&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="161.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="223" Qdbm="011702001002" Mc="基础-模板" Xmtz="1．基础类型：桩承台基础&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="283.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="224" Qdbm="011702001003" Mc="基础-模板" Xmtz="1．基础类型：筏板基础&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="6.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="225" Qdbm="011702001004" Mc="设备基础" Xmtz="1．基础类型：设备基础&#xD;&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="1.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="226" Qdbm="011702002001" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：1.6m以内&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="174.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="227" Qdbm="011702002002" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：2.4m以内&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="191.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="228" Qdbm="011702002003" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：2.4m以外&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="4.22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="229" Qdbm="011702003001" Mc="构造柱-模板" Xmtz="1．构造柱模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="333.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="230" Qdbm="011702005001" Mc="基础梁" Xmtz="1．基础梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="494.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="231" Qdbm="011702006001" Mc="矩形梁" Xmtz="1．矩形梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="51.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="232" Qdbm="011702008001" Mc="圈梁-模板" Xmtz="1．圈梁、反坎等模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="298.38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="233" Qdbm="011702009001" Mc="过梁-模板" Xmtz="1．过梁模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="43.46" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="234" Qdbm="011702011001" Mc="直形墙-模板" Xmtz="1．直行墙等模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="627.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="235" Qdbm="011702013001" Mc="短肢剪力墙、电梯井壁" Xmtz="1．电梯井墙等模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="50.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="236" Qdbm="011702014001" Mc="有梁板" Xmtz="1．有梁板模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="7523.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="237" Qdbm="011702023001" Mc="雨篷、悬挑板、阳台板" Xmtz="1．雨棚模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按设计图示尺寸，以外挑部分水平投影面积计算" Dw="m2" Sl="8.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="238" Qdbm="011702024001" Mc="楼梯" Xmtz="1．楼梯模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按楼梯（包括休息平台、水平梁、斜梁和楼层板的连接梁）的水平投影面积计算" Dw="m2" Sl="92.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="239" Qdbm="011702026001" Mc="电缆沟、地沟" Xmtz="1．排水沟等板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，自行报价，结算不作调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="16.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="240" Qdbm="WB011702039001" Mc="压顶-模板" Xmtz="1．压顶模板&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="186.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="241" Qdbm="WB011702030001" Mc="柱支模超高" Xmtz="1．柱支模超高&#xD;&#xA;2．模板的材质由投标人自行选择、满足混凝土成型质量及安全等要求、自行报价、结算不做调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="766.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="242" Qdbm="WB011702031001" Mc="梁支模超高" Xmtz="1．梁支模超高&#xD;&#xA;2．模板的材质由投标人自行选择、满足混凝土成型质量及安全等要求、自行报价、结算不做调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="215.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="243" Qdbm="WB011702033001" Mc="板支模超高" Xmtz="1．板支模超高&#xD;&#xA;2．模板的材质由投标人自行选择、满足混凝土成型质量及安全等要求、自行报价、结算不做调整" Gcnr="" Jsgz="按超出3.6m部分的模板与现浇混凝土接触面积计算" Dw="m2" Sl="20713.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="244" Qdbm="011703001001" Mc="建筑垂直运输" Xmtz="1．层数：多层厂房&#xA;2．建筑物建筑类型及结构形式：框架结构&#xA;3．建筑物檐口高度、层数：12.3m&#xD;&#xA;" Gcnr="" Jsgz="1.建筑物地下室部分垂直运输按设计室内地坪(±0.00)以下的建筑面积，以面积计算2.建筑物上部建筑部分垂直运输按室内地坪(±0.00)以上的建筑面积总和，以面积计算" Dw="m2" Sl="4936.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="245" Qdbm="011705001001" Mc="大型机械设备进出场及安拆" Xmtz="1．机械设备名称：打桩机、挖掘机、起重机、施工电梯、预拌砂浆罐式搅拌机等机械含基础等、投标人自行根据施工方案考虑、综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按使用机械设备的数量计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="00004" Dwgcmc="电芯库（安装）" Zylb="1" Jzmj="6994.41" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B9767C6F3B122686496A" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="1.1" Mc="强电系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="030404017001" Mc="配电箱" Xmtz="1、名称：电芯库配电箱MP-W1-101&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="030404017002" Mc="配电箱" Xmtz="1、名称：电芯库配电箱MP-W1-102&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="030404017003" Mc="配电箱" Xmtz="1、名称：电芯库配电箱MP-W1-103&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="030404017004" Mc="配电箱" Xmtz="1、名称：电芯库配电箱MCC-W1-101&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="5" Qdbm="030404017005" Mc="配电箱" Xmtz="1、名称：电芯库配电箱MCC-W1-201&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="030404017006" Mc="配电箱" Xmtz="1、名称：电芯库配电箱DT-W0-R01&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="030404017007" Mc="配电箱" Xmtz="1、名称：电芯库配电箱EMCC-W1-201&#xD;&#xA;2、建议尺寸： 800（W）×1000（H）×250（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="030404017008" Mc="配电箱" Xmtz="1、名称：电芯库配电箱AL-W1-101&#xD;&#xA;2、建议尺寸： 500（W）×600（H）×200（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="030404017009" Mc="配电箱" Xmtz="1、名称：电芯库配电箱AL-W1-102&#xD;&#xA;2、建议尺寸： 500（W）×600（H）×200（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="10" Qdbm="030404017010" Mc="配电箱" Xmtz="1、名称：电芯库配电箱EAL-W1-101&#xD;&#xA;2、建议尺寸： 500（W）×600（H）×200（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="030404017011" Mc="配电箱" Xmtz="1、名称：电芯库配电箱EAL-W1-201&#xD;&#xA;2、建议尺寸： 500（W）×600（H）×200（D），具体尺寸以盘柜厂深化为准。&#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="030404017012" Mc="配电箱" Xmtz="1、名称：电芯库配电箱EAL-W1-101A&#xD;&#xA;2、尺寸： 非标 &#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="030404017013" Mc="配电箱" Xmtz="1、名称：电芯库配电箱EAL-W1-201A&#xD;&#xA;2、尺寸： 非标 &#xD;&#xA;3、安装方式：挂墙明装&#xD;&#xA;4、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="030404032001" Mc="端子箱" Xmtz="1、名称：T接箱&#xD;&#xA;2、含成套箱体、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="030404017014" Mc="配电箱" Xmtz="1、名称：卷帘门控制箱&#xD;&#xA;2、安装方式：明装&#xD;&#xA;3、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="030404017015" Mc="配电箱" Xmtz="1、名称：电梯控制箱（设备自带，仅计安装费）&#xD;&#xA;2、安装方式：明装&#xD;&#xA;3、成品成套配电箱，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="030411001001" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN100&#xD;&#xA;4、敷设方式：明敷&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="41.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="18" Qdbm="030411001002" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN65&#xD;&#xA;4、敷设方式：明敷&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="9.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="030411001003" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、敷设方式：明敷&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="20.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="030411001004" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN32&#xD;&#xA;4、敷设方式：明敷&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="19.21" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="030411001005" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：明敷&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="828.27" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="030411001006" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：明敷&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="177.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="030411001007" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：JDG20&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="1064.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="030411001008" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：JDG25&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="240.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="030411001009" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="92.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="030411001010" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="127.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="030411001011" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：JDG20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="2483.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="030411001012" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：JDG25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="560.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="031002003001" Mc="套管制作与安装" Xmtz="1、名称：预埋强电入户管&#xD;&#xA;2、规格：SC100&#xD;&#xA;3、含套管预埋、孔洞预留" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="030411003001" Mc="桥架" Xmtz="1、名称：热浸镀锌梯式桥架&#xD;&#xA;2、规格：300*100&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="225.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="030411003002" Mc="桥架" Xmtz="1、名称：热浸镀锌梯式桥架&#xD;&#xA;2、规格：600*150&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="7.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="030411003003" Mc="桥架" Xmtz="1、名称：热浸镀锌梯式桥架&#xD;&#xA;2、规格：800*200&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="75.81" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="030411003004" Mc="桥架" Xmtz="1、名称：耐火线槽&#xD;&#xA;2、规格：200*100&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="152.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="030413001001" Mc="铁构件" Xmtz="1、材质：型钢、角钢&#xD;&#xA;2、名称：桥架支撑架&#xD;&#xA;3、制作、安装" Gcnr="" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="0.750" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="030408008001" Mc="防火堵洞" Xmtz="1、名称：桥架、电缆等防火堵洞&#xD;&#xA;2、备注：包含本系统所有防火堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="14.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="030408001001" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-3*70+2*35&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="138.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="37" Qdbm="030408001002" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：RTTZ-4*4+1*4&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="90.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="030408001003" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*150+1*70&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="293.97" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="030408001004" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*95+1*50&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="399.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="030408001005" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZBN-YJV-3*50+1*25&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="16.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="030408001006" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-4*16+1*16&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="170.88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="030408001007" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：NH-YJV-5*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="405.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="030408001008" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZBN-YJV-3*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="57.20" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="030408001009" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="146.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="030408001010" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*2.5+1*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="293.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="030408001011" Mc="电力电缆" Xmtz="1、名称：电力电缆&#xD;&#xA;2、规格型号：ZB-YJV-3*2.5+2*2.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="135.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="030408002001" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZB-KVV-6*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="213.67" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="030408002002" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZB-KVV-2*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="54.82" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="030408002003" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-2*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="11.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="50" Qdbm="030408002004" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-4*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="288.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="030408002005" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-14*1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="9.03" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="030408007001" Mc="控制电缆头" Xmtz="1、名称：控制电缆头&#xD;&#xA;2、规格型号：≤6芯&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="030408007002" Mc="控制电缆头" Xmtz="1、名称：控制电缆头&#xD;&#xA;2、规格型号：≤14芯&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="030408006001" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：240mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="030408006002" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：120mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="030408006003" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：70mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="030408006004" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：50mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="030408006005" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：16mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="030408006006" Mc="电力电缆头" Xmtz="1、名称：电缆终端头&#xD;&#xA;2、规格型号：10mm2内&#xD;&#xA;3、材质、类型：铜芯&#xD;&#xA;4、电压等级（kV)：1.0&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="030411004001" Mc="配线" Xmtz="1、名称：照明配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-BV2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="419.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="030411004002" Mc="配线" Xmtz="1、名称：照明配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZB-BV2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="6623.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="030411004003" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZB-BV4&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="2415.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="030411004004" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-B2-RVS-2*2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="1926.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="030412005001" Mc="荧光灯" Xmtz="1、名称：LED单管壁灯&#xD;&#xA;2、规格：1x18W LED 光通量1890lm&#xD;&#xA;3、安装形式：壁装，距地2.6m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="030412001001" Mc="普通灯具" Xmtz="1、名称：LED单管灯&#xD;&#xA;2、规格：1x18W LED 光通量1890lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="030412001002" Mc="普通灯具" Xmtz="1、名称：LED双管灯&#xD;&#xA;2、规格：2x18W LED 光通量3780lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="44" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="030412001003" Mc="普通灯具" Xmtz="1、名称：三防LED双管灯&#xD;&#xA;2、规格：2x18W LED 光通量3780lm&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="030412001004" Mc="普通灯具" Xmtz="1、名称：防水防尘灯&#xD;&#xA;2、规格：1x11W LED 光通量1155lm，防护等级：IP54&#xD;&#xA;3、安装方式：吸顶" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="030412001005" Mc="普通灯具" Xmtz="1、名称：广照型工矿灯（带灯罩）&#xD;&#xA;2、规格：1X200W&#xD;&#xA;3、安装方式：吊装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="51" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="70" Qdbm="030412005002" Mc="荧光灯" Xmtz="1、名称：节能LED灯（附带红外线光控带延时开关）&#xD;&#xA;2、规格：1x14W,LED 光通量1470lm&#xD;&#xA;3、安装形式：吸顶" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="71" Qdbm="030412001006" Mc="普通灯具" Xmtz="1、名称：电梯井道灯具&#xD;&#xA;2、型号：防水、防尘、带防护罩灯具，内设13W LED灯&#xD;&#xA;3、安装形式：壁装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="WB030904013001" Mc="智能照明灯/指示灯" Xmtz="1、名称：安全疏散方向标志灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：距地0.5米或吊装（安装高度小于3.5m）" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="WB030904013002" Mc="智能照明灯/指示灯" Xmtz="1、名称：安全疏散方向标志灯-(双面单向）&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：距地0.5米或吊装（安装高度小于3.5m）" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="74" Qdbm="WB030904013003" Mc="智能照明灯/指示灯" Xmtz="1、名称：安全出口标志灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：门框上沿0.1m明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="WB030904013004" Mc="智能照明灯/指示灯" Xmtz="1、名称：楼层指示指示灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="WB030904013005" Mc="智能照明灯/指示灯" Xmtz="1、名称：疏散出口指示灯&#xD;&#xA;2、规格：DC36V,1*1W,LED&#xD;&#xA;3、安装方式：门框上沿0.1m明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="WB030904013006" Mc="智能照明灯/指示灯" Xmtz="1、名称：消防应急照明灯&#xD;&#xA;2、规格：DC36V,1*6W,LED 光通量720lm&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="WB030904013007" Mc="智能照明灯/指示灯" Xmtz="1、名称：消防应急照明灯（IP67）&#xD;&#xA;2、规格：DC36V,1*6W,LED 光通量720lm&#xD;&#xA;3、安装方式：距地2.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="030404034001" Mc="照明开关" Xmtz="1、名称：单联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="030404034002" Mc="照明开关" Xmtz="1、名称：双联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="030404034003" Mc="照明开关" Xmtz="1、名称：三联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="030404034004" Mc="照明开关" Xmtz="1、名称：四联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="030404034005" Mc="照明开关" Xmtz="1、名称：单联双控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="030404034006" Mc="照明开关" Xmtz="1、名称：密闭单联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="030404034007" Mc="照明开关" Xmtz="1、名称：密闭三联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="030404034008" Mc="照明开关" Xmtz="1、名称：密闭防水二联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="030404034009" Mc="照明开关" Xmtz="1、名称：密闭防水三联单控开关&#xD;&#xA;2、规格：AC250V,10A&#xD;&#xA;3、安装方式：距地1.3m暗装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="88" Qdbm="030404034010" Mc="照明开关" Xmtz="1、名称：风机盘管三速开关&#xD;&#xA;2、安装方式：距地1.3m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="89" Qdbm="030404034011" Mc="照明开关" Xmtz="1、名称：卫生间洗手池、小便池感应开关电源" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="030404031001" Mc="小电器" Xmtz="1、名称：控制按钮盒（两个按钮）&#xD;&#xA;2、安装方式：距地1.5明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（套、台）" Sl="16.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="030404031002" Mc="小电器" Xmtz="1、名称：控制按钮盒（两个按钮，1个检修按钮）&#xD;&#xA;2、安装方式：距地1.5明装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（套、台）" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="030404035001" Mc="插座" Xmtz="1、名称：单相二、三眼插座&#xD;&#xA;2、规格：AC250V,10A，安全型&#xD;&#xA;3、安装方式：距地0.3m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="030404035002" Mc="插座" Xmtz="1、名称：单相二、三眼插座（密闭型）&#xD;&#xA;2、规格：AC250V,10A，安全型&#xD;&#xA;3、安装方式：距地0.3m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="030404035003" Mc="插座" Xmtz="1、名称：烘手器插座&#xD;&#xA;2、规格：AC250V,16A，安全型&#xD;&#xA;3、安装方式：距地1.5m暗装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="95" Qdbm="030411006001" Mc="接线盒" Xmtz="1、名称：开关盒（插座盒）&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="88" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="030411006002" Mc="接线盒" Xmtz="1、名称：接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="312" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="030414002001" Mc="送配电装置系统" Xmtz="1、名称：送配电装置系统调试&#xD;&#xA;2、电压等级（KV)：1KV以下&#xD;&#xA;" Gcnr="" Jsgz="按设计图示系统计算" Dw="系统" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="030414004001" Mc="自动投入装置" Xmtz="1、名称：自动切换电源系统调试&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="系统（台、套）" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.2" Mc="防雷接地" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="99" Qdbm="030409005001" Mc="避雷网" Xmtz="1、名称：避雷网&#xD;&#xA;2、材质：Φ12热镀锌圆钢&#xD;&#xA;3、安装形式：明敷 " Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="729.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="030409005002" Mc="避雷网" Xmtz="1、名称：避雷网&#xD;&#xA;2、材质：25*4热镀锌扁钢&#xD;&#xA;3、安装形式：明敷 " Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="30.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="030409003001" Mc="避雷引下线" Xmtz="1、名称：引下线&#xD;&#xA;2、安装形式：利用钢柱或柱内两根≥中16的主筋上端与屋面接闪器相连，下端与基础接地装置可靠焊接。" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="436.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="102" Qdbm="WB030409002001" Mc="柱主筋与圈梁钢筋焊接" Xmtz="1、名称：柱主筋与圈梁钢筋焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="58.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="030409002001" Mc="接地母线" Xmtz="1、名称：接地母线&#xD;&#xA;2、材质：热镀锌扁钢&#xD;&#xA;3、规格：-25*4" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="71.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="030409002002" Mc="接地母线" Xmtz="1、名称：接地母线&#xD;&#xA;2、材质：热镀锌扁钢&#xD;&#xA;3、规格：-40*4" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="29.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="030409002003" Mc="接地母线" Xmtz="1、名称：接地母线&#xD;&#xA;2、材质：热镀铜扁钢&#xD;&#xA;3、规格：-40*4" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="379.38" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="030409004001" Mc="基础梁接地线" Xmtz="1、名称：接地网&#xD;&#xA;2、安装形式：利用基础梁内两根&gt;16主钢筋(无钢筋处采用-40*4热镀铜扁钢)组成接地网&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="323.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="030409008001" Mc="等电位端子箱、测试板" Xmtz="1、名称：总等电位箱MEB&#xD;&#xA;2、材质：金属" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="108" Qdbm="030409008002" Mc="等电位端子箱、测试板" Xmtz="1、名称：局部等电位箱LEB&#xD;&#xA;2、材质：金属" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="030409008003" Mc="等电位端子箱、测试板" Xmtz="1、名称：辅助等电位箱SEB&#xD;&#xA;2、材质：金属" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="030409008004" Mc="等电位端子箱、测试板" Xmtz="1、名称：接地箱&#xD;&#xA;2、安装：安装于地面上0.3m或天花上0.3m" Gcnr="1、采购、安装" Jsgz="按设计图示数量计算" Dw="个" Sl="14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="111" Qdbm="030409001001" Mc="接地极" Xmtz="1、名称：预埋接地钢板&#xD;&#xA;2、规格、材质：100*100*8" Gcnr="" Jsgz="按设计图示数量计算" Dw="块" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="112" Qdbm="030411001013" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：PC&#xD;&#xA;3、规格：40&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="22.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="113" Qdbm="030411004005" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：穿管敷设&#xD;&#xA;3、规格：BVR-1*35&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="22.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="114" Qdbm="030414011001" Mc="接地装置" Xmtz="1、名称：接地系统测试" Gcnr="" Jsgz="1．以系统计量，按设计图示系统计算2．以组计量，按设计图示数量计算。" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.1" Mc="给水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="115" Qdbm="031001007001" Mc="复合管" Xmtz="1、安装部位：室外&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：钢丝网骨架增加聚乙烯复合管 DN40&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="116" Qdbm="031001007002" Mc="复合管" Xmtz="1、安装部位：室外&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：钢丝网骨架增加聚乙烯复合管 DN25&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="117" Qdbm="031001007003" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN40&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="31.61" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="118" Qdbm="031001007004" Mc="复合管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：热镀锌衬塑钢管 DN25&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="30.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="119" Qdbm="031001006001" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De20&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="93.63" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="120" Qdbm="031001006002" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De25&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="10.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="121" Qdbm="031001006003" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De32&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="3.45" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="122" Qdbm="031001006004" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：S5级PP-R管 De50&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件 刷色环 消毒冲洗" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="10.04" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="123" Qdbm="031003001001" Mc="螺纹阀门" Xmtz="1、类型：截止阀DN40&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="124" Qdbm="031003001002" Mc="螺纹阀门" Xmtz="1、类型：截止阀DN25&#xD;&#xA;2、材质：不锈钢&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="125" Qdbm="031003001003" Mc="螺纹阀门" Xmtz="1、类型：压力型真空破坏器&#xD;&#xA;2、规格：DN25&#xD;&#xA;3、连接形式：丝扣连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="126" Qdbm="031003001004" Mc="螺纹阀门" Xmtz="1、类型：不锈钢自动排气阀 DN20&#xD;&#xA;2、连接形式：丝扣连接&#xD;&#xA;3、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="127" Qdbm="031003013001" Mc="水表" Xmtz="1、名称：远传水表 DN40&#xD;&#xA;2、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="128" Qdbm="031003013002" Mc="水表" Xmtz="1、名称：远传水表 DN25&#xD;&#xA;2、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="129" Qdbm="031002003002" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN80&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="130" Qdbm="031002003003" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="131" Qdbm="031002003004" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN25&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="132" Qdbm="031002003005" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN40&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="133" Qdbm="031002003006" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN50以下" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="134" Qdbm="031002001001" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="175.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="135" Qdbm="031201003001" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后防锈漆二道,再刷灰色调和漆二道。" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="175.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="136" Qdbm="031201001001" Mc="管道刷油" Xmtz="1、油漆品种：银粉漆&#xD;&#xA;2、涂刷遍数、漆膜厚度：2道" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="7.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="137" Qdbm="031208002001" Mc="管道绝热" Xmtz="1、名称：吊顶内架空充水给水管道防结露&#xD;&#xA;2、绝热材料品种：橡塑管壳&#xD;&#xA;3、绝热厚度：保温厚度20mm&#xD;&#xA;" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="0.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="138" Qdbm="031208002002" Mc="管道绝热" Xmtz="1、名称：室外管道保温、防结露&#xD;&#xA;2、绝热材料品种：橡塑管壳30mm，外包0.5mm厚铝箔保护&#xD;&#xA;3、绝热厚度：" Gcnr="" Jsgz="按图示表面积加绝热层厚度及调整系数计算" Dw="m3" Sl="0.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="139" Qdbm="WB031002009001" Mc="凿槽、刨沟" Xmtz="1、名称：管道剔堵沟槽&#xD;&#xA;2、墙体类型：砖墙&#xD;&#xA;3、尺寸：70*70以内" Gcnr="" Jsgz="按设计图示长度计算" Dw="m" Sl="90.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.2" Mc="污废水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="140" Qdbm="031001006005" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De110&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="32.31" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="141" Qdbm="031001006006" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De75&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="8.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="142" Qdbm="031001006007" Mc="塑料管" Xmtz="1、名称：UPVC承压管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De50&#xD;&#xA;5、连接形式：专用胶黏剂粘接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="12.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="143" Qdbm="031001001001" Mc="镀锌钢管" Xmtz="1、名称：内外壁热浸镀锌钢管&#xD;&#xA;2、安装部位：室内&#xD;&#xA;3.介质：污废水&#xD;&#xA;4、规格、压力等级：De160&#xD;&#xA;5、连接形式：法兰或沟槽连接&#xD;&#xA;6、压力试验及吹洗设计要求：含管道及管件安装、水压试验及通球试验等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="7.44" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="144" Qdbm="WB031002001001" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN100" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="145" Qdbm="WB031002001002" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN75" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="146" Qdbm="WB031002001003" Mc="成品管卡安装" Xmtz="1、名称：成品管卡&#xD;&#xA;2、型号、规格：DN50" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="147" Qdbm="031002001002" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="35.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="148" Qdbm="031201003002" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后防锈漆二道,再刷灰色调和漆二道。" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="35.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="149" Qdbm="WB031202001001" Mc="埋地金属管道防腐" Xmtz="1、名称：埋地金属管道防腐&#xD;&#xA;2、油漆品种：做加强防腐处理" Gcnr="" Jsgz="按设计图示表面积计算" Dw="m2" Sl="3.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="150" Qdbm="031004014001" Mc="给、排水附（配）件" Xmtz="1、名称：不锈钢防臭式地漏&#xD;&#xA;2、型号、规格：De50" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="151" Qdbm="031004014002" Mc="给、排水附（配）件" Xmtz="1、名称：大流量地漏&#xD;&#xA;2、型号、规格：De160" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="152" Qdbm="031004014003" Mc="给、排水附（配）件" Xmtz="1、名称：清扫口&#xD;&#xA;2、材质：铜质&#xD;&#xA;3、型号、规格：DN100&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（组）" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="153" Qdbm="031004006001" Mc="大便器" Xmtz="1、名称：低水箱蹲便器&#xD;&#xA;2、材质：陶瓷&#xD;&#xA;3、组装形式：成套&#xD;&#xA;4、附件名称、数量：含给排水附件&#xD;&#xA;5、参考图集09S304/83" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="154" Qdbm="031004003001" Mc="洗脸盆" Xmtz="1、名称：台式洗手盆&#xD;&#xA;2、材质：陶瓷&#xD;&#xA;3、组装形式：成套&#xD;&#xA;4、附件名称、数量：含给排水附件&#xD;&#xA;5、参考图集09S304/39（53）" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="155" Qdbm="031004007001" Mc="小便器" Xmtz="1、名称：感应式落地式小便器&#xD;&#xA;2、材质：陶瓷&#xD;&#xA;3、组装形式：成套&#xD;&#xA;4、附件名称、数量：含给排水附件&#xD;&#xA;5、参考图集09S304/109" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="156" Qdbm="031004008001" Mc="其他成品卫生器具" Xmtz="1、材质：污水池&#xD;&#xA;2、附件名称、数量：含安装附件等全部内容&#xD;&#xA;3、参考图集09S304/20" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="157" Qdbm="031002003007" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="158" Qdbm="031002003008" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.3" Mc="雨水系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="159" Qdbm="031001006008" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De160&#xD;&#xA;4、连接形式：承插电热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="154.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="160" Qdbm="031001006009" Mc="塑料管" Xmtz="1、安装部位：室内&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De110&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="55.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="161" Qdbm="031001006010" Mc="塑料管" Xmtz="1、安装部位：室外&#xD;&#xA;2、介质：雨水&#xD;&#xA;3、规格、压力等级：HDPE排水塑料管De110（防紫外线型）&#xD;&#xA;4、连接形式：热熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件安装 刷色环&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="24.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="162" Qdbm="031201001002" Mc="管道刷油" Xmtz="1、油漆品种：调和漆&#xD;&#xA;2、涂刷遍数、漆膜厚度：2道" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="104.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="163" Qdbm="WB031002001004" Mc="成品管卡安装" Xmtz="1．名称：成品管卡&#xD;&#xA;2．型号、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="164" Qdbm="WB031002001005" Mc="成品管卡安装" Xmtz="1．名称：成品管卡&#xD;&#xA;2．型号、规格：DN100" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="27" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="165" Qdbm="031004014004" Mc="给、排水附（配）件" Xmtz="1、型号、规格：87型雨水斗De160" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="166" Qdbm="031004014005" Mc="给、排水附（配）件" Xmtz="1、型号、规格：87型雨水斗De110" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="167" Qdbm="031004014006" Mc="给、排水附（配）件" Xmtz="1、型号、规格：侧排雨水斗De110" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="168" Qdbm="031002003009" Mc="溢流口" Xmtz="1、名称：溢流口&#xD;&#xA;2、规格：200PVC" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="169" Qdbm="031002003010" Mc="溢流口" Xmtz="1、名称：不锈钢溢流口&#xD;&#xA;2、规格：200*150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="170" Qdbm="031002003011" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="171" Qdbm="031002003012" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="172" Qdbm="031002003013" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN100&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="173" Qdbm="031002003014" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.1" Mc="消火栓系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="174" Qdbm="031001007005" Mc="复合管" Xmtz="1、安装部位：室外&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：钢丝网骨架增加聚乙烯复合管 DN150&#xD;&#xA;4、连接形式：电熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="10.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="175" Qdbm="030901002001" Mc="消火栓钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸镀锌钢管&#xD;&#xA;3、规格：DN65&#xD;&#xA;4、连接形式：卡箍连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等&#xD;&#xA;" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="157.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="176" Qdbm="030901002002" Mc="消火栓钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸镀锌钢管&#xD;&#xA;3、规格：DN150&#xD;&#xA;4、连接形式：卡箍连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="224.87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="177" Qdbm="031002001003" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="331.09" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="178" Qdbm="031201003003" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后防锈漆二道,再刷灰色调和漆二道。" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="331.09" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="179" Qdbm="031201001003" Mc="管道刷油" Xmtz="1、名称：消火栓管道刷油&#xD;&#xA;2、油漆品种：除锈后刷红色调和漆二道。" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="146.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="180" Qdbm="031003001005" Mc="螺纹阀门" Xmtz="1、类型：不锈钢自动排气阀 DN25&#xD;&#xA;2、连接形式：丝扣连接&#xD;&#xA;3、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="181" Qdbm="031003003001" Mc="焊接法兰阀门" Xmtz="1、类型：涡轮型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、沟槽法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="182" Qdbm="030901010001" Mc="室内消火栓" Xmtz="1、名称：SNZW65-III型减压稳压消火栓&#xD;&#xA;2、箱内配置：采用甲型单栓带灭火器箱组合式消防柜,单栓箱内设有中Φ65消火栓1只Φ65x19水枪1只、Φ65x25m长衬胶水带1根。在每个消火栓处设置一个消火栓的按钮,作为发出报警信号的开关。箱体材质采用铝合金-钢制,箱内设有:室内减压稳压消火栓,出水口压力为0.35Mpa,选用消火栓栓口与墙面成90°角且箱体厚度为240mm的消防箱。暗装在防火上消火栓箱,箱体背面砌体应满足耐火极限不小于3小时;暗装在其他墙体上的箱体，其背面应保留100mm厚以上同材质的砌体;否则应在箱体背面采用不低于该墙体耐火极限(参《民用建筑构件防火设计用料表》)的防火板封堵。采用减压稳压型消火栓。消火栓箱门不应被装饰物遮掩,消火栓箱门四周的装修材料颜色应与消火栓箱门的颜色有明显区别或在消火栓箱门表面设置发光标志。&#xD;&#xA;3、含软包防撞处理、灭火器" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="183" Qdbm="030901010002" Mc="室内消火栓" Xmtz="1、名称：SNZW65-III型减压稳压消火栓内设压力表兼做试验消火栓&#xD;&#xA;2、箱内配置：采用甲型单栓带灭火器箱组合式消防柜,单栓箱内设有中Φ65消火栓1只Φ65x19水枪1只、Φ65x25m长衬胶水带1根。在每个消火栓处设置一个消火栓的按钮,作为发出报警信号的开关。箱体材质采用铝合金-钢制,箱内设有:室内减压稳压消火栓,出水口压力为0.35Mpa,选用消火栓栓口与墙面成90°角且箱体厚度为240mm的消防箱。暗装在防火上消火栓箱,箱体背面砌体应满足耐火极限不小于3小时;暗装在其他墙体上的箱体，其背面应保留100mm厚以上同材质的砌体;否则应在箱体背面采用不低于该墙体耐火极限(参《民用建筑构件防火设计用料表》)的防火板封堵。采用减压稳压型消火栓。消火栓箱门不应被装饰物遮掩,消火栓箱门四周的装修材料颜色应与消火栓箱门的颜色有明显区别或在消火栓箱门表面设置发光标志。&#xD;&#xA;3、含软包防撞处理、灭火器" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="184" Qdbm="030901013001" Mc="灭火器箱" Xmtz="1、名称：灭火器箱&#xA;2、规格、型号：可放置两具灭火器" Gcnr="" Jsgz="" Dw="套" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="185" Qdbm="030901013002" Mc="灭火器" Xmtz="1、名称：磷酸铵盐干粉灭火器&#xA;2、规格、型号：MF/ABC4" Gcnr="" Jsgz="" Dw="具" Sl="12.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="186" Qdbm="030901013003" Mc="灭火器" Xmtz="1、名称：超细干粉自动灭火装置/悬挂式&#xA;2、规格、型号：10KG" Gcnr="" Jsgz="按设计图示数量计算" Dw="具" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="187" Qdbm="031002003015" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="188" Qdbm="031002003016" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="189" Qdbm="031002003017" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="190" Qdbm="031002003018" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN65&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="191" Qdbm="030905002001" Mc="水灭火系统控制装置调试" Xmtz="1、名称：消火栓系统调试" Gcnr="" Jsgz="按控制装置的点数计算" Dw="点" Sl="20.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.2" Mc="喷淋系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="192" Qdbm="031001007006" Mc="复合管" Xmtz="1、安装部位：室外&#xD;&#xA;2、介质：给水&#xD;&#xA;3、规格、压力等级：钢丝网骨架增加聚乙烯复合管 DN150&#xD;&#xA;4、连接形式：电熔连接&#xD;&#xA;5、压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6、说明：含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="6.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="193" Qdbm="030901001001" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="607.67" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="194" Qdbm="030901001002" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN32&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="542.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="195" Qdbm="030901001003" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN40&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="222.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="196" Qdbm="030901001004" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、连接形式：螺纹连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="338.23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="197" Qdbm="030901001005" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN65&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="40.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="198" Qdbm="030901001006" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN80&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="78.35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="199" Qdbm="030901001007" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN100&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="36.59" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="200" Qdbm="030901001008" Mc="水喷淋钢管" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质：热浸锌镀锌钢管&#xD;&#xA;3、规格：DN150&#xD;&#xA;4、连接形式：沟槽连接&#xD;&#xA;5、含管件、卡箍、机械开孔等所有管件，含管道标识（底色、色环、标识）等" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="195.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="201" Qdbm="031002001004" Mc="管道支吊架制作与安装" Xmtz="1、名称：管道支吊架&#xD;&#xA;2、管架形式：综合" Gcnr="" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="1591.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="202" Qdbm="031201003004" Mc="金属结构刷油" Xmtz="1、名称：管道支架刷油&#xD;&#xA;2、油漆品种：除锈后刷防锈漆二道,再刷灰色调和漆二道" Gcnr="" Jsgz="1．以平方米计量，按设计图示表面积尺寸以面积计算2．以千克计量，按金属结构的理论质量计算" Dw="kg" Sl="1591.17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="203" Qdbm="031201001004" Mc="管道刷油" Xmtz="1、名称：喷淋管道刷油&#xD;&#xA;2、油漆品种：除锈后刷红色调和漆二道。" Gcnr="" Jsgz="1.以平方米计量，按设计图示表面积尺寸以面积计算2.以米计算，按设计图示尺寸以长度计算" Dw="m2" Sl="360.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="204" Qdbm="030901003001" Mc="水喷淋（雾）喷头" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质、型号、规格：直立型标准响应喷头 K=80&#xD;&#xA;3、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="524" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="205" Qdbm="030901003002" Mc="水喷淋（雾）喷头" Xmtz="1、安装部位：室内&#xD;&#xA;2、材质、型号、规格：干式下垂型标准响应喷头 K=80&#xD;&#xA;3、连接形式：螺纹连接&#xD;&#xA;4、装饰盘设计要求：含装饰盘" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="206" Qdbm="031003001006" Mc="自动排气阀" Xmtz="1、类型：快速排气阀&#xD;&#xA;2、规格、压力等级：DN32&#xD;&#xA;3、连接形式：螺纹连接&#xD;&#xA;4、含截止阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="207" Qdbm="031003001007" Mc="螺纹阀门" Xmtz="1、类型：不锈钢电磁阀&#xD;&#xA;2、规格、压力等级：DN32&#xD;&#xA;3、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="208" Qdbm="031003003002" Mc="焊接法兰阀门" Xmtz="1、类型：把手型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN50&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="209" Qdbm="031003003003" Mc="焊接法兰阀门" Xmtz="1、类型：涡轮型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN100&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="210" Qdbm="031003003004" Mc="焊接法兰阀门" Xmtz="1、类型：涡轮型对夹式蝶阀&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="211" Qdbm="031003003005" Mc="焊接法兰阀门" Xmtz="1、类型：信号阀&#xD;&#xA;2、规格、压力等级：DN150&#xD;&#xA;3、连接形式：法兰连接&#xD;&#xA;4、含阀门、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="212" Qdbm="030901007001" Mc="减压孔板" Xmtz="1、类型：减压孔板&#xD;&#xA;2、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="213" Qdbm="030901006001" Mc="水流指示器" Xmtz="1、类型：水流指示器 DN150&#xD;&#xA;2、连接形式：法兰连接&#xD;&#xA;3、含法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="214" Qdbm="030901004001" Mc="报警装置" Xmtz="1、名称：预作用报警阀组&#xD;&#xA;2、型号、规格：DN150&#xD;&#xA;3、含报警阀、水力警铃、信号阀" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="215" Qdbm="030110001001" Mc="空压机" Xmtz="1、名称：空压机&#xD;&#xA;2、型号、规格：排气量0.2m3/min，功率3KW&#xD;&#xA;3、含连接管、止回阀、过滤器、压力开关等全套安装附件" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="216" Qdbm="030503006001" Mc="传感器、变送器" Xmtz="1、名称：电子流量计24V&#xD;&#xA;2、规格：DN150" Gcnr="" Jsgz="按设计图示数量计算" Dw="支(台)" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="217" Qdbm="030901008001" Mc="末端试水装置" Xmtz="1、名称：末端试水装置&#xD;&#xA;2、规格：DN25&#xD;&#xA;3、组装形式：成套组装，含截止阀、压力表、试水接头，阀门箱上锁并设置标识" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="218" Qdbm="031003001008" Mc="螺纹阀门" Xmtz="1、类型：末端试水阀&#xD;&#xA;2、规格、压力等级：DN25&#xD;&#xA;3、连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="219" Qdbm="030601002001" Mc="压力仪表" Xmtz="1、名称：压力表&#xA;2、型号：满足设计要求&#xD;&#xA;3、压力等级：0~1.0MPa&#xA;4、备注：自带弯管及检修阀" Gcnr="" Jsgz="" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="220" Qdbm="031004008002" Mc="通气帽" Xmtz="1、材质：通气帽&#xD;&#xA;2、规格、类型：DN80&#xD;&#xA;3、附件名称、数量：含安装附件等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="221" Qdbm="030817005001" Mc="钢制排水漏斗制作安装" Xmtz="1、名称：钢制排水漏斗&#xD;&#xA;2、规格：DN80" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="222" Qdbm="031002003019" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN25&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="223" Qdbm="031002003020" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN50&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="224" Qdbm="031002003021" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN80&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="225" Qdbm="031002003022" Mc="套管制作与安装" Xmtz="1、名称：钢套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;3、含预留孔洞、堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="226" Qdbm="031002003023" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN150&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="227" Qdbm="031002003024" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN80&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="228" Qdbm="030905002002" Mc="水灭火系统控制装置调试" Xmtz="1、名称：自动喷淋系统调试" Gcnr="" Jsgz="按控制装置的点数计算" Dw="点" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="3.3" Mc="消防电系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="229" Qdbm="040504002001" Mc="电缆手孔井" Xmtz="1、名称：弱电手孔井&#xD;&#xA;2、规格：1000*1000*1200&#xD;&#xA;3、作法参07SD101-8所示 P121&#xD;&#xA;4、含手孔井砌筑、模板支护、钢筋绑扎、井壁抹面、井盖、铁件预埋、接地等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="230" Qdbm="030411001014" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN50&#xD;&#xA;4、敷设方式：埋地" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="9.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="231" Qdbm="031002003025" Mc="套管制作与安装" Xmtz="1、名称：刚性防水套管&#xD;&#xA;2、规格：介质管道DN50&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="232" Qdbm="030411001015" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="1009.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="233" Qdbm="030411001016" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="1294.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="234" Qdbm="030411001017" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="30.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="235" Qdbm="030411001018" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="39.58" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="236" Qdbm="030411001019" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN25&#xD;&#xA;4、敷设方式：明配&#xD;&#xA;5、接地要求：含接地、支架、刷防火漆等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="50.49" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="237" Qdbm="030411003005" Mc="桥架" Xmtz="1、名称：火警专用防火金属线槽&#xD;&#xA;2、规格：(50+50+50)*100&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="142.75" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="238" Qdbm="030411003006" Mc="桥架" Xmtz="1、名称：消防应急广播专用防火金属线槽&#xD;&#xA;2、规格：50*25&#xD;&#xA;3、材质：金属&#xD;&#xA;4、含组对、焊接、桥架开孔、隔板与盖板安装、接地、附件安装、修理、基础等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="113.85" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="239" Qdbm="030413001002" Mc="铁构件" Xmtz="1、材质：型钢、角钢&#xD;&#xA;2、名称：桥架支撑架&#xD;&#xA;3、制作、安装" Gcnr="" Jsgz="按设计图示尺寸以质量计算" Dw="t" Sl="0.249" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="240" Qdbm="030408008002" Mc="防火堵洞" Xmtz="1、名称：桥架、电缆等防火堵洞&#xD;&#xA;2、备注：包含本系统所有防火堵洞" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="6.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="241" Qdbm="030411004006" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="2097.10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="242" Qdbm="030411004007" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="252.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="243" Qdbm="030411004008" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、型号：ZBN-RVS-2X1.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="1592.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="244" Qdbm="030411004009" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="640.48" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="245" Qdbm="030411004010" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X4&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="128.70" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="246" Qdbm="030411004011" Mc="配线" Xmtz="1、名称：消防配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="432.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="247" Qdbm="030408002006" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-4x1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="1024.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="248" Qdbm="030408002007" Mc="控制电缆" Xmtz="1、名称：控制电缆&#xD;&#xA;2、规格型号：ZBN-KVV-24x1.5&#xD;&#xA;3、材质：铜芯&#xD;&#xA;4、敷设方式、部位：桥架或配管敷设&#xD;&#xA;5、电压等级：1.0KV&#xD;&#xA;" Gcnr="" Jsgz="按设计图示尺寸以单相长度计算（含预留长度及附加长度）" Dw="m" Sl="248.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="249" Qdbm="030404032002" Mc="端子箱" Xmtz="1、名称：接线端子箱&#xD;&#xA;2、安装部位：墙上安装,底距地+2.4m&#xD;&#xA;3、成套采购，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="250" Qdbm="030904008001" Mc="模块（模块箱）" Xmtz="1、名称：模块箱&#xD;&#xA;2、安装部位：墙上安装,底距地+2.4m&#xD;&#xA;3、成套采购，含箱体内所有电器元件、接线端子、接地等辅材安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（台）" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="251" Qdbm="030904008002" Mc="模块" Xmtz="1、名称：短路隔离器&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="252" Qdbm="030904001001" Mc="点型探测器" Xmtz="1、名称：智能感烟探测器&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="163" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="253" Qdbm="030904001002" Mc="点型探测器" Xmtz="1、名称：智能感温探测器&#xD;&#xA;2、安装方式：吸顶安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="254" Qdbm="030904003001" Mc="按钮" Xmtz="1、名称：消火栓报警按钮&#xD;&#xA;2、规格：消火栓箱内安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="255" Qdbm="030904007001" Mc="消防广播（扬声器）" Xmtz="1、名称：壁挂扬声器(6W)&#xD;&#xA;2、安装方式：离地2.3~2.6米安装&#xD;&#xA;3、阻燃材料,或具有阻燃后罩结构" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="19" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="256" Qdbm="030904005001" Mc="声光报警器" Xmtz="1、名称：声光报警器&#xD;&#xA;2、安装方式：墙装,底距地+2.3~3.0m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="257" Qdbm="030904003002" Mc="按钮" Xmtz="1、名称：手动火灾报警按钮&#xD;&#xA;2、规格：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="258" Qdbm="030904006001" Mc="消防报警电话插孔（电话）" Xmtz="1、名称：消防电话插孔&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="259" Qdbm="WB030904002001" Mc="火灾显示盘" Xmtz="1、名称：楼层显示器/区域显示器&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="260" Qdbm="030904006002" Mc="消防报警电话插孔（电话）" Xmtz="1、名称：固定式火警电话机&#xD;&#xA;2、安装方式：墙上安装,底距地+1.4m" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="261" Qdbm="030904008003" Mc="模块（模块箱）" Xmtz="1、名称：输入输出模块&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="262" Qdbm="030904008004" Mc="模块（模块箱）" Xmtz="1、名称：输入模块&#xD;&#xA;2、安装于模块箱内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="263" Qdbm="030411006003" Mc="接线盒" Xmtz="1、名称：接线盒&#xD;&#xA;2、材质：钢制&#xD;&#xA;3、规格：86盒" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="312" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="264" Qdbm="030411005001" Mc="接线箱" Xmtz="1、名称：中转箱&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="265" Qdbm="030905001001" Mc="自动报警系统装置调试" Xmtz="1、名称：自动报警系统调试&#xD;&#xA;2、点数：500点以内" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="266" Qdbm="WB030905001001" Mc="火灾事故广播、消防通信系统调试" Xmtz="1、名称：消防广播、电话插孔调试" Gcnr="" Jsgz="按系统的点数计算" Dw="只（部）" Sl="30.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="267" Qdbm="WB030905001002" Mc="火灾事故广播、消防通信系统调试" Xmtz="1、名称：火灾报警电话调试" Gcnr="" Jsgz="按系统的点数计算" Dw="只（部）" Sl="3.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="268" Qdbm="030905003001" Mc="防火控制装置联动调试" Xmtz="1、名称：防火阀联动调试" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（部）" Sl="18.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="269" Qdbm="030411004012" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVVSP-2*2.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="281.98" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="270" Qdbm="030411001020" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="68.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="271" Qdbm="WB030904010001" Mc="消防电源监控设备" Xmtz="1、名称：消防电源监控器&#xD;&#xA;2、型号规格：AFPM3-3AVML" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="272" Qdbm="030905001002" Mc="自动报警系统装置调试" Xmtz="1、名称：消防电源监控系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="273" Qdbm="030411004013" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVVSP-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="233.86" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="274" Qdbm="030411001021" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：SC&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="22.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="275" Qdbm="030905001003" Mc="自动报警系统装置调试" Xmtz="1、名称：应急照明系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="276" Qdbm="030411001022" Mc="配管" Xmtz="1、名称：电气配管&#xD;&#xA;2、材质：JDG&#xD;&#xA;3、规格：DN20&#xD;&#xA;4、敷设方式：暗敷&#xD;&#xA;5、含剔补沟槽、防腐接地等" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="72.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="277" Qdbm="030411004014" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVV-2X1.5&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="273.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="278" Qdbm="030411004015" Mc="配线" Xmtz="1、名称：配线&#xD;&#xA;2、配线形式：桥架或穿管敷设&#xD;&#xA;3、规格型号：ZBN-RVS-2X1.0&#xD;&#xA;4、材质：铜芯" Gcnr="" Jsgz="按设计图示尺寸以单线长度计算（含预留长度）" Dw="m" Sl="198.89" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="279" Qdbm="WB030904006001" Mc="防火门监控设备" Xmtz="1、名称：常闭单门防火门监控模块&#xD;&#xA;2、安装：门框上侧安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="280" Qdbm="030507001001" Mc="入侵探测设备" Xmtz="1、名称：门磁开关&#xD;&#xA;2、门框上侧安装" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="8" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="281" Qdbm="030904008005" Mc="模块（模块箱）" Xmtz="1、名称：防火门监控中继器" Gcnr="" Jsgz="按设计图示数量计算" Dw="个（台）" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="282" Qdbm="030905001004" Mc="自动报警系统装置调试" Xmtz="1、名称：防火门监控系统调试" Gcnr="" Jsgz="按系统计算" Dw="系统" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.1" Mc="通风系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="283" Qdbm="WB030701004001" Mc="通风机安装" Xmtz="1、名称：PF-1-1低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量800m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="284" Qdbm="WB030701004002" Mc="通风机安装" Xmtz="1、名称：PF-1-2、3低噪音箱式管道离心风机&#xD;&#xA;2、设备主要参数：风量900m3/h，静压250Pa，电动机功率0.55KW，转速1450rpm，噪声限值68dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目)&#xD;&#xA;4、安装形式：吊装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="285" Qdbm="WB030701004003" Mc="通风机安装" Xmtz="1、名称：SEF-250D4边墙风机&#xD;&#xA;2、设备主要参数：风量1000m3/h，静压70Pa，电动机功率0.125KW，转速1450rpm，噪声限值55dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目),自带防雨百叶&#xD;&#xA;4、安装形式：边墙安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="286" Qdbm="WB030701004004" Mc="通风机安装" Xmtz="1、名称：SEF-350D4边墙风机&#xD;&#xA;2、设备主要参数：风量2500m3/h，静压70Pa，电动机功率0.25KW，转速1450rpm，噪声限值62dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件,进出口带防鼠网(≥40目),自带防雨百叶&#xD;&#xA;4、安装形式：边墙安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="287" Qdbm="030702001001" Mc="碳钢通风管道" Xmtz="1、名称：通风风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：450&lt;b≤630&#xD;&#xA;5、厚度：0.6mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="3.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="288" Qdbm="030702001002" Mc="碳钢通风管道" Xmtz="1、名称：通风风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：b≤450&#xD;&#xA;5、厚度：0.5mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="34.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="289" Qdbm="030702009001" Mc="弯头导流叶片" Xmtz="1、名称：导流叶片&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="0.08" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="290" Qdbm="WB030702001001" Mc="软管接口" Xmtz="1、名称：风管软管接头&#xD;&#xA;2、材质：不燃浸胶机布" Gcnr="" Jsgz="按设计图示以展开面积计算" Dw="m2" Sl="2.78" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="291" Qdbm="030703007001" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：250*250&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="292" Qdbm="030703007002" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：350*350&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="293" Qdbm="030703007003" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排风口（带调节阀）&#xD;&#xA;2、规格：400*400&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="294" Qdbm="030703001001" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：320*320&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="295" Qdbm="030703001002" Mc="碳钢阀门安装" Xmtz="1、名称：70℃防火阀&#xD;&#xA;2、规格：500*500&#xD;&#xA;3、平时常开,70度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="296" Qdbm="WB030701005001" Mc="设备支架制作安装" Xmtz="1、名称：设备支吊架&#xD;&#xA;2、材质：型钢" Gcnr="1、制作、安装" Jsgz="按设计图示质量计算" Dw="kg" Sl="120.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="297" Qdbm="031002001005" Mc="风管支架刷漆" Xmtz="1、名称：风管及设备支吊架刷漆&#xD;&#xA;2、做法：除锈后刷灰色磁性漆两道" Gcnr="1、制作、安装&#xD;&#xA;2、除锈、刷油" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="256.16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4.2" Mc="防排烟系统" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="298" Qdbm="WB030701004005" Mc="通风机安装" Xmtz="1、名称：PY-R-1消防型管道轴流风机&#xD;&#xA;2、设备主要参数：风量92100m3/h，静压1250Pa，电动机功率55KW，转速1450rpm，噪声限值91dB(A)，效率≥75%&#xD;&#xA;3、备注：含配套控制箱、电动机检查接线、减震装置等安装所需附件&#xD;&#xA;4、安装形式：落地安装&#xD;&#xA;" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="299" Qdbm="030702001003" Mc="碳钢通风管道" Xmtz="1、名称：防排烟风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：1500&lt;b≤2000&#xD;&#xA;5、厚度：1.5mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件&#xD;&#xA;" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="718.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="300" Qdbm="030702001004" Mc="碳钢通风管道" Xmtz="1、名称：防排烟风管&#xD;&#xA;2、形状：矩形&#xD;&#xA;3、材质：镀锌钢板&#xD;&#xA;4、规格：1000&lt;b≤1500&#xD;&#xA;5、厚度：1.2mm&#xD;&#xA;6、接口形式：法兰连接&#xD;&#xA;7、含风管管件、法兰、支架等安装所需一切附件" Gcnr="" Jsgz="按设计图示内径尺寸以展开面积计算" Dw="m2" Sl="84.47" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="301" Qdbm="WB030702001002" Mc="软管接口" Xmtz="1、名称：风管软管接头&#xD;&#xA;2、材质：不燃浸胶机布" Gcnr="" Jsgz="按设计图示以展开面积计算" Dw="m2" Sl="2.10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="302" Qdbm="030702009002" Mc="弯头导流叶片" Xmtz="1、名称：导流叶片&#xD;&#xA;" Gcnr="" Jsgz="" Dw="m2" Sl="4.29" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="303" Qdbm="030703007004" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排烟风口&#xD;&#xA;2、规格：1000*800&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="304" Qdbm="030703007005" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：单层百叶排烟风口&#xD;&#xA;2、规格：1200*1000&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="9" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="305" Qdbm="030703007006" Mc="碳钢风口、散流器、百叶窗" Xmtz="1、名称：防雨百叶风口&#xD;&#xA;2、规格：2500*2000&#xD;&#xA;3、材质：铝合金" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="306" Qdbm="030703001003" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1250*400&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="307" Qdbm="030703001004" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1250*450&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="308" Qdbm="030703001005" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1600*400&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="309" Qdbm="030703001006" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1600*450&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="310" Qdbm="030703001007" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：1600*500&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="311" Qdbm="030703001008" Mc="碳钢阀门安装" Xmtz="1、名称：280℃排烟防火阀&#xD;&#xA;2、规格：2000*630&#xD;&#xA;3、平时常开,280度熔断,输出熔断信号" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="312" Qdbm="030703001009" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1250*450&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="313" Qdbm="030703001010" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1250*400&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="314" Qdbm="030703001011" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1600*400&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="315" Qdbm="030703001012" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1600*450&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="316" Qdbm="030703001013" Mc="碳钢阀门安装" Xmtz="1、名称：常闭排烟阀&#xD;&#xA;2、规格：1600*500&#xD;&#xA;3、含防火阀、手动控制器&#xD;&#xA;4、平时常闭,火灾时可手动、电动启闭" Gcnr="" Jsgz="分别按图示规格尺寸（直径或周长），以“个”为计量单位计算." Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="317" Qdbm="031208003001" Mc="通风管道绝热" Xmtz="1、绝热材料品种：金属风管外包防排烟专用岩棉复合铝箔&#xD;&#xA;2、绝热厚度：50mm以上&#xD;&#xA;3、材料类型：岩棉板采用防火黑棉，容重(60kg/m³)" Gcnr="" Jsgz="1．以立方米计算，按图示表面积加绝热层厚度及调整系数计算2．以立方米计量，按图示表面积及调整系数计算" Dw="m3" Sl="7.87" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="318" Qdbm="031208003002" Mc="通风管道绝热" Xmtz="1、绝热材料品种：金属风管外包防排烟专用岩棉复合铝箔&#xD;&#xA;2、绝热厚度：65mm以上&#xD;&#xA;3、材料类型：岩棉板采用防火黑棉，容重(100kg/m³)" Gcnr="" Jsgz="1．以立方米计算，按图示表面积加绝热层厚度及调整系数计算2．以立方米计量，按图示表面积及调整系数计算" Dw="m3" Sl="40.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="319" Qdbm="WB030701005002" Mc="设备支架制作安装" Xmtz="1、名称：设备支吊架&#xD;&#xA;2、材质：型钢" Gcnr="1、制作、安装" Jsgz="按设计图示质量计算" Dw="kg" Sl="40.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="320" Qdbm="031002001006" Mc="风管支架刷漆" Xmtz="1、名称：风管及设备支吊架刷漆&#xD;&#xA;2、做法：除锈后刷灰色磁性漆两道" Gcnr="1、制作、安装&#xD;&#xA;2、除锈、刷油" Jsgz="以千克计量，按设计图示质量计算" Dw="kg" Sl="3581.56" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="321" Qdbm="WB030906007001" Mc="挡烟垂壁" Xmtz="1、名称：固定式挡烟垂壁&#xD;&#xA;2、材质：不燃防火玻璃" Gcnr="" Jsgz="按设计图示面积数量计算" Dw="m2" Sl="229.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="322" Qdbm="030701003001" Mc="空调器" Xmtz="1、名称：柜式分体空调KT-1&#xD;&#xA;2、参数：额定制冷量7.1KW，额定制热量8.6KW，额定制冷耗电量2.1KW&#xD;&#xA;3、落地安装、含槽钢基础、配套管道、支架等材料。" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="323" Qdbm="030701003002" Mc="空调器" Xmtz="1、名称：柜式分体空调KT-2&#xD;&#xA;2、参数：额定制冷量8.82KW，额定制热量11.2KW，额定制冷耗电量2.8KW&#xD;&#xA;3、落地安装、含槽钢基础、配套管道、支架等材料。" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="324" Qdbm="ZB010101001001" Mc="电梯工程" Xmtz="1、名称：电芯库3T货梯&#xD;&#xA;2、参数：载重量3000KG，速度0.5m/s，层站数2，井道净尺寸(扣梁柱)3400x3550，门洞尺寸1800x2500，提升高度6m&#xD;&#xA;3、说明：包含全新的电梯主体设施设备，电气设备，控制系统，曳引系统，安全设备及构件，外罩配套按钮及显示，轿厢内通风、照明，层门及门坎门楣，五方对讲等&#xD;&#xA;4、含安装费、吊运费、安装调试" Gcnr="" Jsgz="" Dw="部" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="325" Qdbm="WB031002008001" Mc="抗震支架安装" Xmtz="1、名称：抗震支架&#xD;&#xA;2、管架形式：建筑机电工程（电气工程、给排水工程、暖通工程、消防工程等）等工程需设置抗震支架的全部内容抗震支吊架&#xD;&#xA;3、其他：抗震支吊架需通过相关认证，且认证项目为抗震支吊架项目&#xD;&#xA;4、本项目范围内所涉及的所专业的抗震支架，不仅限于本次招标范围内的专业。&#xD;&#xA;5、由施工承包单位负责委托具有资质的设计单位进行深化设计，并组织专家论证，以确保安全性&#xD;&#xA;6、设计、论证、施工、检验监测等所需全部费用由投标人综合考虑在包括在投标报价内，（包括后期所有的抗震支架）按一项列入, 投标单位根据现场、图纸、招标文件和所有施工规范等资料,充分考虑,投标人综合报价，一次性包死，中标后不予调整 " Gcnr="" Jsgz="按设计图示数量计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="326" Qdbm="010101003001" Mc="挖沟槽土方" Xmtz="1、土壤类别：自行勘测&#xD;&#xA;2、挖沟深度：2米以内&#xD;&#xA;3、回填要求：夯填" Gcnr="" Jsgz="按设计图示尺寸沟槽长度乘以沟槽断面积，以体积计算" Dw="m3" Sl="100.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="327" Qdbm="031301017001" Mc="脚手架搭拆" Xmtz="1、内容：脚手架搭拆费用&#xD;&#xA;2、投标人综合考虑报价，中标后不予调整&#xD;&#xA;" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="328" Qdbm="WB031301002001" Mc="操作高度增加费" Xmtz="1、内容：操作高度增加费 &#xD;&#xA;2、投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="329" Qdbm="031301012001" Mc="工程系统检测、检验" Xmtz="1、名称：暖通系统调试费&#xD;&#xA;2、投标人综合考虑报价，中标后不予调整" Gcnr="" Jsgz="" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
  </Dxgcxx>
  <Dxgcxx Dxgcmc="室外工程" Dxgcbh="dx003" Je="0" Bkjzf="0" Aqwmf="0" Zgj="0" Jzmj="0" Aqsczrbxf="0">
    <Dwgcxx Dwgcbh="00005" Dwgcmc="室外道路工程" Zylb="1" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B976FE032D1D161821B5" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="SF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <Qdmx Xh="1" Qdbm="040101001001" Mc="挖一般土方" Xmtz="1．土壤类别：自行考虑&#xD;&#xA;2．部位：主楼土方平衡至室内层底、清表土方等&#xD;&#xA;3．开挖过程中所遇淤泥、建筑垃圾、障碍物等投标单位自行考虑在报价中，中标后不予调整&#xD;&#xA;4．控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="10821.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="2" Qdbm="040101001002" Mc="挖一般土方" Xmtz="1．土壤类别：自行考虑&#xD;&#xA;2．部位：道路（土方平衡至底层）、清表土方、篮球场等&#xD;&#xA;3．开挖过程中所遇淤泥、建筑垃圾、障碍物等投标单位自行考虑在报价中，中标后不予调整&#xD;&#xA;4．控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="5656.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="3" Qdbm="040103001001" Mc="回填方" Xmtz="1．部位：道路等回填&#xD;&#xA;2．夯填（碾压）:压实系数≥0.94&#xD;&#xA;3．控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="1786.64" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="4" Qdbm="040202001001" Mc="路床(槽)碾压检验" Xmtz="1．部位：新建沥青路面&#xD;&#xA;2．土基压实 (重型标准:压实度≥0.94)" Gcnr="" Jsgz="按设计道路底基层图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="2941.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="5" Qdbm="040202008001" Mc="砖渣" Xmtz="1．石料规格：50cm 砖渣压实(压实度≥0.94)" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="2762.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="6" Qdbm="040202011001" Mc="碎石" Xmtz="1．石料规格：20cm 级配碎石找平层" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="2762.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="7" Qdbm="040203007001" Mc="水泥混凝土" Xmtz="1．混凝土强度等级：22cm C30混凝土 " Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2645.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="8" Qdbm="WB040203014001" Mc="养生" Xmtz="1．养生形式：薄膜洒水养护" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2645.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="9" Qdbm="WB040203009001" Mc="模板" Xmtz="1．厚度：22cm" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2645.77" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="10" Qdbm="040203003001" Mc="透层" Xmtz="1．4mm乳化沥青" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2579.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="11" Qdbm="040203004001" Mc="封层" Xmtz="1．4mm乳化沥青" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2579.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="12" Qdbm="040203006001" Mc="沥青混凝土" Xmtz="1．沥青混凝土种类：AC-20 中粒式沥青砼 &#xD;&#xA;2．厚度：6cm  " Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2579.15" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="13" Qdbm="040203003002" Mc="粘层" Xmtz="1．粘层0.4L/m2" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2404.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="14" Qdbm="040203006002" Mc="沥青混凝土" Xmtz="1．沥青混凝土种类： AC-13 细粒式沥青砼&#xD;&#xA;2．厚度：4cm " Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="2404.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="15" Qdbm="040202001002" Mc="路床(槽)碾压检验" Xmtz="1．部位：装卸货区域&#xD;&#xA;2．土基压实 (重型标准:压实度≥0.94)" Gcnr="" Jsgz="按设计道路底基层图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="92.57" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="16" Qdbm="040202008002" Mc="砖渣" Xmtz="1．石料规格：50cm 砖渣压实(压实度≥0.94)" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="90.37" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="17" Qdbm="040202011002" Mc="碎石" Xmtz="1．石料规格：20cm 级配碎石找平层" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="90.14" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="18" Qdbm="040203007002" Mc="水泥混凝土" Xmtz="1．混凝土强度等级：22cm C30混凝土 面层内配钢筋网片 C 8单层双向@200x200" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="88.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="19" Qdbm="WB040203014002" Mc="养生" Xmtz="1．养生形式：薄膜洒水养护" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="88.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="20" Qdbm="WB040203009002" Mc="模板" Xmtz="1．厚度：22cm" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="88.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="21" Qdbm="040202001003" Mc="路床(槽)碾压检验" Xmtz="1．部位：场地硬化&#xD;&#xA;2．素土夯实(压实度≥0.94)" Gcnr="" Jsgz="按设计道路底基层图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="267.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="22" Qdbm="040202008003" Mc="砖渣" Xmtz="1．石料规格：50cm 砖渣压实(压实度≥0.94)" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="267.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="23" Qdbm="040202011003" Mc="碎石" Xmtz="1．石料规格：20cm 级配碎石找平层" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="267.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="24" Qdbm="040203007003" Mc="水泥混凝土" Xmtz="1．混凝土强度等级：25cm厚c30混凝土随捣随抹光,内配钢筋网片C12单层双向@200x200(需切缝,4米*6米,弯拉强度4.5MPa)" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="267.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="25" Qdbm="WB040203014003" Mc="养生" Xmtz="1．养生形式：薄膜洒水养护" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="267.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="26" Qdbm="WB040203009003" Mc="模板" Xmtz="1．厚度：25cm" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="267.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="27" Qdbm="040204004001" Mc="安砌混凝土侧石" Xmtz="1．材料品种、规格：C30预制混凝土道牙12x35x99.5cm&#xD;&#xA;2．55mm1:3干硬性水泥砂浆&#xD;&#xA;3．两节路缘石之间采用1:3水泥砂浆挤浆安装后勾缝,缝宽0.5cm" Gcnr="" Jsgz="按设计图示中心线长度计算" Dw="m" Sl="681.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="28" Qdbm="040204004002" Mc="安砌混凝土侧石" Xmtz="1．材料品种、规格：C30预制混凝土道牙12x35x99.5cm&#xD;&#xA;2．20mm1:3干硬性水泥砂浆&#xD;&#xA;3．两节路缘石之间采用1:3水泥砂浆挤浆安装后勾缝,缝宽0.5cm" Gcnr="" Jsgz="按设计图示中心线长度计算" Dw="m" Sl="22.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="29" Qdbm="WB040204011001" Mc="靠背" Xmtz="1．材料品种：C20混凝土" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="29.99" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="30" Qdbm="011702001001" Mc="靠背模板" Xmtz="1．基础类型：靠背模板" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="199.93" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="31" Qdbm="040203006003" Mc="沥青混凝土" Xmtz="1．部位：新老路连接处&#xD;&#xA;2．所需破除、外运等均包含在报价内&#xD;&#xA;3．满足业主及设计要求，投标人综合考虑报价" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="32" Qdbm="WB040203013001" Mc="路面刻痕" Xmtz="1．部位：混凝土路面&#xD;&#xA;2．刻痕：刻纹采用机械刻纹,平均纹理深度为1-2mm" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="349.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="33" Qdbm="WB040203012001" Mc="伸缩缝" Xmtz="1．类型：缩缝\横缝&#xD;&#xA;2．材料品种：聚氨酯&#xD;&#xA;3．规格：4~6mm\4~8mm*6mm" Gcnr="" Jsgz="按设计图示尺寸以缝的断面积计算" Dw="m2" Sl="7.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="34" Qdbm="WB040203012002" Mc="伸缩缝" Xmtz="1．类型：胀缝、纵缝&#xD;&#xA;2．材料品种：填缝板、聚氨酯&#xD;&#xA;3．规格：20*4mm、4~8mm*6mm" Gcnr="" Jsgz="按设计图示尺寸以缝的断面积计算" Dw="m2" Sl="3.42" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="35" Qdbm="WB040203010001" Mc="传力杆（构造筋、钢筋网）制作、安装" Xmtz="1．材质：拉杆(14螺纹钢)杆长70cm,拉杆间距90cm&#xD;&#xA;2．10cm长涂沥青两道" Gcnr="" Jsgz="按设计配合比以重量计算" Dw="t" Sl="0.382" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="36" Qdbm="WB040203010002" Mc="传力杆（构造筋、钢筋网）制作、安装" Xmtz="1．材质：传力杆25(圆钢),杆长450mm杆间距300mm&#xD;&#xA;2．涂沥青两道" Gcnr="" Jsgz="按设计配合比以重量计算" Dw="t" Sl="2.933" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="37" Qdbm="WB040203010003" Mc="传力杆（构造筋、钢筋网）制作、安装" Xmtz="1．材质：传力杆25(圆钢),杆长450mm杆间距300mm&#xD;&#xA;2．涂沥青两道&#xD;&#xA;3．滑动传力杆套管内填木屑" Gcnr="" Jsgz="按设计配合比以重量计算" Dw="t" Sl="1.358" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="38" Qdbm="040205018001" Mc="防撞栏杆" Xmtz="1．120镀锌钢管,涂黑黄相间警示漆，灌C20砼&#xD;&#xA;2．80防撞柱横杆涂黑黄相间警示漆&#xD;&#xA;3．预埋件：400x400x12钢板；a12钢筋焊接,共4根&#xD;&#xA;4．C30砼基础（含模板）&#xD;&#xA;5．所需模板、挖土方、回填方、外运等均包含在报价内" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="39" Qdbm="010516002001" Mc="预埋铁件" Xmtz="1．钢材种类：采用L50X5mm角钢护边,锚筋直径8@250,长150mm" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="1.015" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="40" Qdbm="040205006001" Mc="标线" Xmtz="1．材料品种：沥青漆喷涂&#xD;&#xA;2．膜厚度1.5mm~2.0mm&#xD;&#xA;3．热熔漆&#xD;&#xA;4．部位：标线、消防通道划线、人行道划线、行车箭头" Gcnr="" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="126.22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="41" Qdbm="490106009001" Mc="施工围栏搭拆" Xmtz="1．原厂区围栏需拆除至指定区域恢复安装&#xD;&#xA;2．投标人综合考虑报价" Gcnr="" Jsgz="按设计图示以长度计算" Dw="m" Sl="60.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="42" Qdbm="040204001001" Mc="人行道整形、碾压" Xmtz="1．素土夯实(夯实系数大于93%)" Gcnr="" Jsgz="按设计人行道图示尺寸以面积计算，不扣除侧石、树池及各类井所占面积" Dw="m2" Sl="649.90" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="43" Qdbm="040202009001" Mc="砂石" Xmtz="1．石料规格：100厚砂石垫层" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积" Dw="m2" Sl="613.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="44" Qdbm="WB040204009001" Mc="人行道混凝土垫层" Xmtz="1．材料品种：200厚C25混凝土" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="122.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="45" Qdbm="WB040204010001" Mc="现浇混凝土人行道模板" Xmtz="1．厚度：20cm" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，但应扣除侧石、树池所占面积" Dw="m2" Sl="613.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="46" Qdbm="WB040203014004" Mc="养生" Xmtz="1．养生形式：薄膜洒水养护" Gcnr="" Jsgz="按设计图示尺寸以面积计算，不扣除各类井所占面积，带平石的面层应扣除平石所占面积" Dw="m2" Sl="613.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="47" Qdbm="011003003001" Mc="涂料" Xmtz="1．涂料品种、涂刷遍数：1.5mm丙烯酸面层涂料" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="613.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="48" Qdbm="011103002001" Mc="橡胶板卷材楼地面 " Xmtz="1．面层材料品种、规格、颜色：3mm厚硅PU球场面层" Gcnr="" Jsgz="按设计图示尺寸，以面积计算" Dw="m2" Sl="613.11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="49" Qdbm="010401014001" Mc="砖地沟、明沟" Xmtz="1．620*840*120混凝土沟盖板；内配a6钢筋网&#xD;&#xA;2．20厚1:2.5水泥砂浆面层(掺3%防水剂)&#xD;&#xA;3．MU10砖,m7.5砂浆砌&#xD;&#xA;4．100厚C15混凝土垫层&#xD;&#xA;5．素土夯实&#xD;&#xA;6．所需模板、挖土方、回填方、外运等均包含在报价内" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m" Sl="102.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="50" Qdbm="040205006002" Mc="标线" Xmtz="1．材料品种：50mm宽白色涂料" Gcnr="" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="10.29" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <QdBt Bm="2" Mc="围网" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="51" Qdbm="010101004001" Mc="挖基坑土方、挖沟槽土方" Xmtz="1．土壤类别：自行考虑&#xD;&#xA;2．挖土深度：3m以内&#xD;&#xA;3．部位：基础等&#xD;&#xA;4．开挖过程中所遇淤泥、建筑垃圾、房障碍物等投标单位自行考虑在报价中，中标后不予调整" Gcnr="" Jsgz="按设计图示尺寸基坑底面积乘以挖土深度，以体积计算" Dw="m3" Sl="726.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="010103001001" Mc="回填方" Xmtz="1．部位：基础回填&#xD;&#xA;2．夯填（碾压）:素土夯实,压实系数≥0.92" Gcnr="" Jsgz="按设计图示尺寸,以体积计算" Dw="m3" Sl="672.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="WB010101013001" Mc="机械运土方" Xmtz="1．余方弃置&#xD;&#xA;2．土壤类别：综合，不分类别&#xD;&#xA;3．运距：控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按需运输土方，以天然密实体积计算" Dw="m3" Sl="54.74" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="010404001001" Mc="垫层" Xmtz="1．材料品种及比例：150厚级配碎石垫层" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="14.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="010501003001" Mc="独立基础" Xmtz="1．混凝土种类：商品砼&#xD;&#xA;2．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="30.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="56" Qdbm="010501006001" Mc="设备基础" Xmtz="1．部位：包角&#xD;&#xA;2．混凝土种类：商品砼&#xD;&#xA;3．混凝土强度等级：C25混凝土" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="0.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="010502001001" Mc="矩形柱" Xmtz="1．柱规格形状：矩形1.6m以内&#xD;&#xA;2．周长：2.4m以内&#xD;&#xA;3．混凝土种类：商品混凝土&#xD;&#xA;4．混凝土强度等级：C30" Gcnr="" Jsgz="按设计图示尺寸，以体积计算" Dw="m3" Sl="9.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="011702001002" Mc="基础" Xmtz="1．基础类型：独立基础&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="81.60" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="011702001003" Mc="基础" Xmtz="1．基础类型：包角基础&#xA;2．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="3.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="011702002001" Mc="矩形柱-模板" Xmtz="1．矩形柱模板&#xA;2．周长：2.4m以内&#xA;3．模板的材质由投标人自行选择，满足混凝土成型质量及安全等要求，投标单位综合考虑自行报价，中标后不得调整" Gcnr="" Jsgz="按模板与现浇混凝土接触面积计算" Dw="m2" Sl="82.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="010515001001" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ8&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.816" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="010515001002" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ12&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.850" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="010515001003" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ16&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.816" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="010515001004" Mc="现浇构件钢筋" Xmtz="1．钢筋种类：HRB400级钢&#xD;&#xA;2．钢筋规格：Φ18&#xD;&#xA;3．含钢筋运输、制作、安装等全部工作内容" Gcnr="" Jsgz="按设计图示钢筋长度乘以单位理论质量计算" Dw="t" Sl="0.510" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="010516002002" Mc="预埋铁件" Xmtz="1．钢材种类：220x220x14厚钢板，60x50x6厚三角铁等" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.005" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="010516001001" Mc="螺栓" Xmtz="1．钢材种类：M14柱脚锚栓(带调节螺母)" Gcnr="" Jsgz="按设计图示尺寸，以质量计算" Dw="t" Sl="0.082" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="WB011701011001" Mc="围网" Xmtz="1．高度：4.13m&#xD;&#xA;2．骨架：75x5镀锌钢管,墨绿色氟碳漆喷涂；75x5镀锌钢管门框,墨绿色氟碳漆喷涂，成品专用合页安装门框；20X4扁铝,墨绿色氟碳漆饰面&#xD;&#xA;3．围网:优质低碳钢丝,编织焊接,墨绿色PE钢丝3.8,网孔:50x50&#xD;&#xA;4．所需围网门、配置成品锁等均包含在报价内" Gcnr="" Jsgz="1.按设计立挂的垂直投影面积计算2.按设计搭设的水平投影面积计算" Dw="m2" Sl="443.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="011705001001" Mc="大型机械设备进出场及安拆" Xmtz="1．机械设备名称：挖掘机、摊铺机、压路机等、投标人自行根据施工方案考虑、综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按使用机械设备的数量计算" Dw="项" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="5800000" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje>
    <ZljeMx Xh="1" Mc="暂列金" Dw="" Zdje="5800000" Bz="" />
  </Zlje>
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="00006" Dwgcmc="绿化工程" Zylb="1" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B9767C6F3B122686496A" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <Qdmx Xh="1" Qdbm="050101010001" Mc="整理绿化用地" Xmtz="1．平整后绿化带土方应低于周边路缘石3—5cm&#xD;&#xA;2．场地标高及平整度应无积水、坑&#xD;&#xA;3．无直径大于5cm的砖(石)块、宿根性杂草、树根及其他有害污染物,清理物应及时外运,不得就地填埋等" Gcnr="" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="2963.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="2" Qdbm="050101009001" Mc="种植土回（换）填" Xmtz="1．绿化带(除乔木种植处)表层30cm为种植土进行虚铺折实,种植乔木处的种植土厚度不得低于1.2m&#xD;&#xA;2．运距：控制价按5KM计入，投标人自行勘察现场，综合考虑报价，结算时不予调整" Gcnr="" Jsgz="按设计图示回填面积乘以回填厚度以体积计算" Dw="m3" Sl="889.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    <Qdmx Xh="3" Qdbm="050102012001" Mc="铺种草皮" Xmtz="1．草皮种类：百慕大草&#xD;&#xA;2．铺种方式：满铺&#xD;&#xA;3．养护期：成活100%；成活养护一个月、保存养护3个月，日常养护20个月&#xD;&#xA;4．养护等级：二级养护" Gcnr="" Jsgz="按设计图示尺寸以面积计算" Dw="m2" Sl="2963.94" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
    <Dwgcxx Dwgcbh="00007" Dwgcmc="室外安装工程" Zylb="1" Jzmj="0" SoftName="国泰新点软件股份有限公司" SoftNum="30A18A095B562D6D1D04C7B5BE1B051052574F2E81B810E060A95DCE14113946FA64C5B68D57B9767C6F3B122686496A" DogNum="9733c80100070200b83a0008000d003f" MachineKey="84A93837B4EF">
  <Bkjzf>
    <BkjzfMx Xh="1.1" Bm="JF-01" Mc="    环境保护费" Qfjs="0" Fl="3.28" Je="0" Fyxlb="1.1" />
    <BkjzfMx Xh="1.2" Bm="JF-02" Mc="    文明施工费" Qfjs="0" Fl="5.12" Je="0" Fyxlb="1.2" />
    <BkjzfMx Xh="1.3" Bm="JF-03" Mc="    安全施工费" Qfjs="0" Fl="4.13" Je="0" Fyxlb="1.3" />
    <BkjzfMx Xh="1.4" Bm="JF-04" Mc="    临时设施费" Qfjs="0" Fl="8.1" Je="0" Fyxlb="1.4" />
    <BkjzfMx Xh="2.2" Bm="JF-05" Mc="    环境保护税" Qfjs="0" Fl="0" Je="0" Fyxlb="2.2" />
  </Bkjzf>
  <Aqsczrbxf>
    <AqsczrbxfMx Xh="1" Mc="安全生产责任保险费" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费" Fl="0.165" Je="0" />
  </Aqsczrbxf>
  <Sj>
    <SjMx Xh="1" Mc="增值税" Qfjs="0" Jsjc="分部分项工程费+措施项目费+不可竞争费+其他项目费+安全生产责任保险费" Fl="9" Je="0" Fyxlb="1" />
  </Sj>
  <Qdxm>
    <QdBt Bm="1.1" Mc="给水土石方工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="1" Qdbm="040101002001" Mc="挖沟槽土方" Xmtz="1．名称：挖沟槽土方&#xD;&#xA;2．土壤类别：综合考虑&#xD;&#xA;3．挖土深度：1.5m内" Gcnr="" Jsgz="按设计图示尺寸沟槽长度乘以沟槽断面积，以体积计算" Dw="m3" Sl="3103.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="2" Qdbm="WB010101011001" Mc="人工清底" Xmtz="1．名称：人工清底&#xD;&#xA;2．土壤类别：综合考虑" Gcnr="" Jsgz="按需清底的范围，以面积计算" Dw="m2" Sl="1347.35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="3" Qdbm="WB040501021001" Mc="管道垫层" Xmtz="1．名称：中粗砂垫层&#xD;&#xA;2．垫层材质及厚度：100mm厚" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="70.02" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="4" Qdbm="WB040501021002" Mc="管道垫层" Xmtz="1．名称：混凝土垫层&#xD;&#xA;2．垫层材质及厚度：100mm厚&#xD;&#xA;3．商品混凝土强度等级：C30商品混凝土&#xD;&#xA;4．含管道垫层、垫层模版等全部内容" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="64.71" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="5" Qdbm="WB040501023001" Mc="非定型混凝土管道基础" Xmtz="1．基础材质及厚度：过路管道满包至管顶20cm&#xD;&#xA;2．商品混凝土强度等级：C30商品混凝土" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="156.73" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="6" Qdbm="WB040501024001" Mc="管道基础模板" Xmtz="1．名称：管道包封模板" Gcnr="" Jsgz="按设计图示尺寸按混凝土和模版的接触面以平方米计算" Dw="m2" Sl="911.07" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="7" Qdbm="040103001001" Mc="回填方" Xmtz="1．填方材料要求：素土回填" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="2273.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="8" Qdbm="040103001002" Mc="回填方" Xmtz="1．填方材料要求：中粗砂" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="515.54" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="9" Qdbm="040103002001" Mc="余方弃置" Xmtz="1．废弃料品种：余方弃置&#xD;&#xA;2．运距：5km" Gcnr="" Jsgz="按挖方清单项目工程量减利用回填方体积（正数）计算" Dw="m3" Sl="829.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.2" Mc="给水工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="10" Qdbm="040501004001" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.0)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN200" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="227.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="11" Qdbm="040501004002" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.0)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN150" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="100.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="12" Qdbm="040501004003" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.0)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN80" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="5.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="13" Qdbm="040501004004" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.0)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN50" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="85.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="14" Qdbm="040501004005" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.0)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN40" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="1.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="15" Qdbm="040501004006" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.0)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN25" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="10.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="16" Qdbm="WB030817014001" Mc="管道消毒冲洗" Xmtz="1．规格、型号：DN250&#xD;&#xA;2．管内介质：水" Gcnr="" Jsgz="按规范或设计要求计算" Dw="m" Sl="227.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="17" Qdbm="WB030817014002" Mc="管道消毒冲洗" Xmtz="1．规格、型号：DN150&#xD;&#xA;2．管内介质：水" Gcnr="" Jsgz="按规范或设计要求计算" Dw="m" Sl="100.79" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="18" Qdbm="WB030817014003" Mc="管道消毒冲洗" Xmtz="1．规格、型号：DN85&#xD;&#xA;2．管内介质：水" Gcnr="" Jsgz="按规范或设计要求计算" Dw="m" Sl="5.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="19" Qdbm="WB030817014004" Mc="管道消毒冲洗" Xmtz="1．规格、型号：DN50&#xD;&#xA;2．管内介质：水" Gcnr="" Jsgz="按规范或设计要求计算" Dw="m" Sl="85.30" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="20" Qdbm="WB030817014005" Mc="管道消毒冲洗" Xmtz="1．规格、型号：DN40&#xD;&#xA;2．管内介质：水" Gcnr="" Jsgz="按规范或设计要求计算" Dw="m" Sl="1.34" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="21" Qdbm="WB030817014006" Mc="管道消毒冲洗" Xmtz="1．规格、型号：DN25&#xD;&#xA;2．管内介质：水" Gcnr="" Jsgz="按规范或设计要求计算" Dw="m" Sl="10.72" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="22" Qdbm="031003003001" Mc="焊接法兰阀门" Xmtz="1．类型：闸阀&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN200&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="23" Qdbm="031003003002" Mc="焊接法兰阀门" Xmtz="1．类型：闸阀&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN150&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="24" Qdbm="031003003003" Mc="焊接法兰阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN80&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="25" Qdbm="031003003004" Mc="焊接法兰阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN65&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="26" Qdbm="031003001001" Mc="螺纹阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN40&#xD;&#xA;4．连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="27" Qdbm="031003001002" Mc="螺纹阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN32&#xD;&#xA;4．连接形式：螺纹连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="28" Qdbm="031003012001" Mc="倒流防止器" Xmtz="1．材质：不锈钢&#xD;&#xA;2．规格：DN200&#xD;&#xA;3．连接形式：法兰连接&#xD;&#xA;4．说明：含倒流防止器、水表、闸阀*2、法兰" Gcnr="" Jsgz="按设计图示数量计算" Dw="组" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="29" Qdbm="031003011001" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN200&#xD;&#xA;4．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="30" Qdbm="031003011002" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．规格、压力等级：DN150&#xD;&#xA;3．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="4.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="31" Qdbm="031003011003" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．规格、压力等级：DN80&#xD;&#xA;3．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="32" Qdbm="031003011004" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．规格、压力等级：DN65&#xD;&#xA;3．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="33" Qdbm="040504002001" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1100mm*1100mm*1200mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="34" Qdbm="040504002002" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1300mm*1300mm*1500mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="35" Qdbm="040504002003" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1300mm*1300mm*1800mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="36" Qdbm="040504002004" Mc="混凝土检查井" Xmtz="1．名称：混凝土水表井&#xD;&#xA;2．规格：2750mm*1300mm*1400mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.3" Mc="消火栓工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="37" Qdbm="040501004007" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN200" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="445.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="38" Qdbm="040501004008" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN150" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="24.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="39" Qdbm="040501004009" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN100" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="131.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="40" Qdbm="031003003005" Mc="焊接法兰阀门" Xmtz="1．类型：闸阀&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN200&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="41" Qdbm="031003003006" Mc="焊接法兰阀门" Xmtz="1．类型：闸阀&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN150&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="42" Qdbm="031003003007" Mc="焊接法兰阀门" Xmtz="1．类型：闸阀&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN100  MZ45X-16Q&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="43" Qdbm="031003003008" Mc="焊接法兰阀门" Xmtz="1．类型：减压孔板&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN100&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="44" Qdbm="031003003009" Mc="焊接法兰阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN150  &#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="45" Qdbm="031003003010" Mc="焊接法兰阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN100&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="46" Qdbm="031003011005" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN200&#xD;&#xA;4．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="47" Qdbm="031003011006" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN150&#xD;&#xA;4．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="48" Qdbm="031003011007" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN100&#xD;&#xA;4．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="49" Qdbm="040504002005" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1100mm*1100mm*1200mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="50" Qdbm="040504002006" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1300mm*1300mm*1500mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="51" Qdbm="040504002007" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1300mm*1300mm*1800mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="52" Qdbm="030901013001" Mc="灭火器" Xmtz="1．形式：磷酸铵盐推车灭火器&#xD;&#xA;2．规格、型号：MFT/ABC20" Gcnr="" Jsgz="按设计图示数量计算" Dw="具" Sl="6.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="53" Qdbm="030901010001" Mc="室内消火栓" Xmtz="1．安装方式：全铝消防箱&#xD;&#xA;2．型号、规格：1800mm*700mm*240mm&#xD;&#xA;3．附件材质、规格：全铝消防箱，箱内配置2股25m长水带+2个水枪" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="54" Qdbm="030901011001" Mc="室外消火栓" Xmtz="1．安装方式：地上式室外消火栓&#xD;&#xA;2．型号、规格：SSF100/65-1.6" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="55" Qdbm="030901011002" Mc="闸阀套筒" Xmtz="1．安装方式：闸阀套筒&#xD;&#xA;2．做法：含闸阀套筒、基础等安装内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1.4" Mc="喷淋工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="56" Qdbm="040501004010" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN250" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="507.32" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="57" Qdbm="040501004011" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN200" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="15.65" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="58" Qdbm="040501004012" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN150" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="31.62" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="59" Qdbm="040501004013" Mc="塑料管铺设" Xmtz="1．管道材质：钢丝网骨架PE给水管(PN1.6)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN100" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="7.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="60" Qdbm="031003003011" Mc="焊接法兰阀门" Xmtz="1．类型：闸阀&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN250&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="61" Qdbm="031003003012" Mc="焊接法兰阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN200&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="62" Qdbm="031003003013" Mc="焊接法兰阀门" Xmtz="1．类型：金属波纹补偿器&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN100&#xD;&#xA;4．连接形式：法兰连接" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="63" Qdbm="031003011008" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN250&#xD;&#xA;4．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="5.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="64" Qdbm="031003011009" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．材质：不锈钢&#xD;&#xA;3．规格、压力等级：DN200&#xD;&#xA;4．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="2.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="65" Qdbm="031003011010" Mc="法兰" Xmtz="1．类型：法兰&#xD;&#xA;2．规格、压力等级：DN100&#xD;&#xA;3．连接形式：焊接" Gcnr="" Jsgz="按设计图示数量计算" Dw="副" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="66" Qdbm="040504002008" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1100mm*1100mm*1200mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="67" Qdbm="040504002009" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1300mm*1300mm*1500mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="68" Qdbm="040504002010" Mc="混凝土检查井" Xmtz="1．名称：混凝土阀门井&#xD;&#xA;2．规格：1300mm*1300mm*1800mm&#xD;&#xA;3．垫层、基础材质及厚度：C15素砼垫层&#xD;&#xA;4．混凝土强度等级：C25混凝土&#xD;&#xA;5．井盖、井圈材质及规格：球磨铸铁&#xD;&#xA;6．说明：含垫层浇筑、井室砌筑、井圈浇筑、井盖安装、套管预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="69" Qdbm="030901012001" Mc="消防水泵接合器" Xmtz="1．安装部位：室外地上&#xD;&#xA;2．型号、规格：SQS150-A型&#xD;&#xA;3．附件材质、规格：含水泵接合器、止回阀、安全阀、闸阀、配套法兰、短管等内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="70" Qdbm="040504001001" Mc="砌筑检查井" Xmtz="1．名称：水泵接合器阀门井&#xD;&#xA;2．做法：99S203" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.1" Mc="照明土石方" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="71" Qdbm="040101002002" Mc="挖沟槽土方" Xmtz="1．沟槽土方&#xD;&#xA;2．土壤类别：三类土&#xD;&#xA;3．挖土深度：1.5m以内" Gcnr="" Jsgz="按设计图示尺寸沟槽长度乘以沟槽断面积，以体积计算" Dw="m3" Sl="764.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="72" Qdbm="040103001003" Mc="回填方" Xmtz="1．基坑、沟槽回填&#xD;&#xA;2．填方材料要求：素土" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="721.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="73" Qdbm="040103002002" Mc="余方弃置" Xmtz="1．废弃料品种：余方弃置&#xD;&#xA;2．运距：5km" Gcnr="" Jsgz="按挖方清单项目工程量减利用回填方体积（正数）计算" Dw="m3" Sl="42.83" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.2" Mc="配电箱及管线" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="74" Qdbm="030404017001" Mc="现状配电箱增容" Xmtz="1．名称：现状配电箱增容&#xD;&#xA;2．含箱体元气期间拆换等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="台" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="75" Qdbm="030408003001" Mc="MPP管" Xmtz="1．名称：MPP管&#xD;&#xA;2．材质：壁厚11mm&#xD;&#xA;3．规格：DN150&#xD;&#xA;4．敷设方式：埋地敷设&#xD;&#xA;5．含管枕" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="831.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="76" Qdbm="030408003002" Mc="镀锌焊接钢管" Xmtz="1．名称：焊接钢管&#xD;&#xA;2．规格：DN150&#xD;&#xA;3．敷设方式：埋地敷设&#xD;&#xA;4．含管枕" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="1273.06" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="77" Qdbm="030408003003" Mc="镀锌焊接钢管" Xmtz="1．名称：焊接钢管&#xD;&#xA;2．规格：DN100&#xD;&#xA;3．敷设方式：埋地敷设&#xD;&#xA;4．含管枕" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="653.28" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="78" Qdbm="030408003004" Mc="镀锌焊接钢管" Xmtz="1．名称：焊接钢管&#xD;&#xA;2．规格：DN50&#xD;&#xA;3．敷设方式：埋地敷设&#xD;&#xA;4．含管枕" Gcnr="" Jsgz="按设计图示尺寸以长度计算" Dw="m" Sl="274.57" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="79" Qdbm="030408003005" Mc="电缆保护管" Xmtz="1．名称：过路保护管&#xD;&#xA;2．材质：SC&#xD;&#xA;3．规格：DN15&#xD;&#xA;4．敷设方式：埋地敷设" Gcnr="" Jsgz="" Dw="m" Sl="131.66" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="80" Qdbm="030408001001" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：ZC-YJV-3x2.5&#xD;&#xA;3．敷设方式、部位：穿管敷设" Gcnr="" Jsgz="" Dw="m" Sl="296.76" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="81" Qdbm="030408001002" Mc="电力电缆" Xmtz="1．名称：电力电缆&#xD;&#xA;2．规格：ZB-YJV-4x16+1x16&#xD;&#xA;3．敷设方式、部位：穿管敷设" Gcnr="" Jsgz="" Dw="m" Sl="159.09" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="82" Qdbm="030408006001" Mc="电力电缆头" Xmtz="1．名称：电力电缆头&#xD;&#xA;2．规格：10mm2以内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="6" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="83" Qdbm="030408006002" Mc="电力电缆头" Xmtz="1．名称：电力电缆头&#xD;&#xA;2．规格：16mm2以内" Gcnr="" Jsgz="按设计图示数量计算" Dw="个" Sl="2" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="84" Qdbm="040504002011" Mc="电缆手孔井" Xmtz="1．名称：电缆手孔井&#xD;&#xA;2．规格：1500mm*1200mm*1500mm&#xD;&#xA;3．混凝土强度等级：MU20烧结普通砖M7.5水泥砂浆&#xD;&#xA;4．防渗、防水要求：1:2.5水泥砂浆抹面10mm厚&#xD;&#xA;5．含基础浇筑、模板支护、检查井砌筑、钢筋绑扎、井盖安装、防坠网、铁件预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="85" Qdbm="040504002012" Mc="电缆手孔井" Xmtz="1．名称：电缆手孔井&#xD;&#xA;2．规格：1000mm*1200mm*1000mm&#xD;&#xA;3．混凝土强度等级：MU20烧结普通砖M7.5水泥砂浆&#xD;&#xA;4．防渗、防水要求：1:2.5水泥砂浆抹面10mm厚&#xD;&#xA;5．含基础浇筑、模板支护、检查井砌筑、钢筋绑扎、井盖安装、防坠网、铁件预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="7" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="86" Qdbm="040504002013" Mc="电缆手孔井" Xmtz="1．名称：电缆手孔井&#xD;&#xA;2．规格：2500mm*2500mm*1900mm&#xD;&#xA;3．混凝土强度等级：MU20烧结普通砖M7.5水泥砂浆&#xD;&#xA;4．防渗、防水要求：1:2.5水泥砂浆抹面10mm厚&#xD;&#xA;5．含基础浇筑、模板支护、检查井砌筑、钢筋绑扎、井盖安装、防坠网、铁件预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="3" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="87" Qdbm="040504002014" Mc="现状检查井开孔" Xmtz="1．名称：现状检查井开孔&#xD;&#xA;2．做法：新建电力管道接至现状电力检查井开孔、恢复等全部费用" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="4.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2.3" Mc="道路路灯及基础" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="88" Qdbm="030412007001" Mc="一般路灯" Xmtz="1．名称：高杆路灯&#xD;&#xA;2．高度：路灯灯杆高度为9 m&#xD;&#xA;3．光源数量：高压钠灯150瓦  &#xD;&#xA;4．含光源、灯具、灯杆及连接件配件等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="89" Qdbm="030412007002" Mc="一般路灯" Xmtz="1．名称：高杆投光灯&#xD;&#xA;2．高度：路灯灯杆高度为5 m&#xD;&#xA;3．光源数量：高压钠灯150瓦  &#xD;&#xA;4．含光源、灯具、灯杆及连接件配件等" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="4" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="90" Qdbm="040303002001" Mc="混凝土基础" Xmtz="1．名称：路灯基础&#xD;&#xA;2．规格：1200mm*1200mm*2200mm&#xD;&#xA;3．混凝土强度等级：C30商品混凝土（泵送）&#xD;&#xA;4．含基础、预埋构件等内容" Gcnr="" Jsgz="按设计图示尺寸以实体体积计算" Dw="座" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="91" Qdbm="WB040303028001" Mc="基础模板" Xmtz="1．名称：基础模板&#xD;&#xA;2．含模板及支架的制作、安装、拆除、整理堆放、场内外运输、清理模板粘结物、杂物、刷隔离剂等费用，投标单位充分考虑，综合报价" Gcnr="" Jsgz="按混凝土与模板接触面的面积计算" Dw="m2" Sl="1372.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="92" Qdbm="030409002001" Mc="接地母线" Xmtz="1．名称：路灯基础接地&#xD;&#xA;2．材质：热镀锌扁钢&#xD;&#xA;3．规格：40×4mm&#xD;&#xA;4．安装部位：户外" Gcnr="" Jsgz="按设计图示尺寸以长度计算（含附加长度）" Dw="m" Sl="10.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="93" Qdbm="030409001001" Mc="接地极" Xmtz="1．名称：路灯基础接地极&#xD;&#xA;2．材质：镀锌角钢&#xD;&#xA;3．规格：50*5 L=2500" Gcnr="" Jsgz="" Dw="根" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="94" Qdbm="030414011001" Mc="接地装置" Xmtz="1、名称：路灯接地系统测试" Gcnr="" Jsgz="" Dw="系统" Sl="5" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="1" Mc="排水土石方工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="95" Qdbm="040101002003" Mc="挖沟槽土方" Xmtz="1．土壤类别：自行考虑&#xD;&#xA;2．挖土深度：2.5m内" Gcnr="" Jsgz="按设计图示尺寸沟槽长度乘以沟槽断面积，以体积计算" Dw="m3" Sl="6533.53" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="96" Qdbm="WB010101011002" Mc="人工清底" Xmtz="1．名称：人工清底&#xD;&#xA;2．土壤类别：综合考虑" Gcnr="" Jsgz="按需清底的范围，以面积计算" Dw="m2" Sl="1872.52" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="97" Qdbm="WB040501021003" Mc="管道垫层" Xmtz="1．名称：碎石垫层&#xD;&#xA;2．垫层材质及厚度：150mm厚" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="292.40" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="98" Qdbm="WB040501021004" Mc="管道垫层" Xmtz="1．名称：中粗砂垫层&#xD;&#xA;2．垫层材质及厚度：150mm厚" Gcnr="" Jsgz="按设计图示尺寸以体积计算" Dw="m3" Sl="315.18" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="99" Qdbm="040103001004" Mc="回填方" Xmtz="1．填方材料要求：中粗砂" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="2109.22" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="100" Qdbm="040103001005" Mc="回填方" Xmtz="1．填方材料要求：素土回填" Gcnr="" Jsgz="1.按挖方清单项目工程量加原地面线至设计要求标高间的体积，减基础、构筑物等埋入体积计算2.按设计图示尺寸以体积计算" Dw="m3" Sl="3442.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="101" Qdbm="040103002003" Mc="余方弃置" Xmtz="1．废弃料品种：余方弃置&#xD;&#xA;2．运距：5km" Gcnr="" Jsgz="按挖方清单项目工程量减利用回填方体积（正数）计算" Dw="m3" Sl="3091.27" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="2" Mc="雨水工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="102" Qdbm="040501001001" Mc="混凝土管道铺设(人机配合下管)" Xmtz="1．管道类型、管道材质：II级钢筋混凝土管&#xD;&#xA;2．连接方式：柔性承插连接&#xD;&#xA;3．管径：D600&#xD;&#xA;4．含管道胶圈接口等内容" Gcnr="" Jsgz="按设计图示中心线长度扣除井所占长度以延长米计算" Dw="m" Sl="134.25" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="103" Qdbm="040501004014" Mc="塑料管铺设" Xmtz="1．管道材质：实壁PE管(环刚度≥8KN/M2)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN500" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="120.13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="104" Qdbm="040501004015" Mc="塑料管铺设" Xmtz="1．管道材质：实壁PE管(环刚度≥8KN/M2)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN400" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="118.01" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="105" Qdbm="040501004016" Mc="塑料管铺设" Xmtz="1．管道材质：实壁PE管(环刚度≥8KN/M2)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN300" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="342.91" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="106" Qdbm="040501004017" Mc="塑料管铺设" Xmtz="1．安装部位：室外&#xD;&#xA;2．介质：雨水&#xD;&#xA;3．规格、压力等级：HDPE排水塑料管DN200&#xD;&#xA;4．连接形式：热熔连接&#xD;&#xA;5．压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6．说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="9.12" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="107" Qdbm="031001006001" Mc="塑料管" Xmtz="1．安装部位：室外&#xD;&#xA;2．介质：雨水&#xD;&#xA;3．规格、压力等级：HDPE排水塑料管DN150&#xD;&#xA;4．连接形式：热熔连接&#xD;&#xA;5．压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6．说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="161.26" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="108" Qdbm="031001006002" Mc="塑料管" Xmtz="1．安装部位：室外&#xD;&#xA;2．介质：雨水&#xD;&#xA;3．规格、压力等级：HDPE排水塑料管DN100&#xD;&#xA;4．连接形式：热熔连接&#xD;&#xA;5．压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6．说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="61.80" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="109" Qdbm="WB040504011001" Mc="φ800预制装配式钢筋混凝土检查井" Xmtz="1．名称：φ800预制装配式钢筋混凝土检查井&#xD;&#xA;2．规格：φ800mm&#xD;&#xA;3．井深：2m内&#xD;&#xA;4．混凝土强度等级：C40混凝土，抗渗P8&#xD;&#xA;5．钢筋制作、安装：采用-HPB300,-HRB400级钢箔，其性能指标应&#xD;&#xA;6．含检查井安装、井盖安装（材料费另计）、防坠网等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="16" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="110" Qdbm="WB040504011002" Mc="φ1000预制装配式钢筋混凝土检查井" Xmtz="1．名称：φ1000预制装配式钢筋混凝土检查井&#xD;&#xA;2．规格：φ1000mm&#xD;&#xA;3．井深：2.5m内&#xD;&#xA;4．混凝土强度等级：C40混凝土，抗渗P8&#xD;&#xA;5．钢筋制作、安装：采用-HPB300,-HRB400级钢箔，其性能指标应&#xD;&#xA;6．含检查井安装、井盖安装（材料费另计）、防坠网等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="111" Qdbm="040504002015" Mc="闸门井" Xmtz="1．名称：闸门井&#xD;&#xA;2．规格：1500mm*1500mm&#xD;&#xA;3．井深：3.5m内&#xD;&#xA;4．垫层、基础材质及厚度：C15混凝土垫层&#xD;&#xA;5．混凝土强度等级：C30混凝土，抗渗P6&#xD;&#xA;6．含检查井浇筑、模板支护、钢筋绑扎、井盖安装（材料费另计）、防坠网、铁件预埋等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="112" Qdbm="040602031001" Mc="闸门" Xmtz="1．名称：平框无法兰方闸门&#xD;&#xA;2．尺寸：1000mm*1000mm&#xD;&#xA;3．含阀体、启闭机、控制柜等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="1" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="113" Qdbm="040504009001" Mc="砖砌平箅式单箅雨水口" Xmtz="1．雨水箅子及圈口材质、型号、规格：砖砌平箅式单箅雨水口&#xD;&#xA;2．垫层、基础材质及厚度：100mmC20混凝土基础&#xD;&#xA;3．砌筑材料品种、规格、强度等级：M10水泥砂浆砖砌体内侧M10水泥砂浆勾缝&#xD;&#xA;4．雨水箅子材质：球墨铸铁箅子（含配套截污挂篮）" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="35" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="114" Qdbm="040504002016" Mc="检查井加固" Xmtz="1．名称：检查井加固&#xD;&#xA;2．混凝土强度等级：C30混凝土&#xD;&#xA;3．做法：含现状路面切槽、钢筋绑扎、混凝土浇筑等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="115" Qdbm="WB040504020001" Mc="φ700防盗重型球墨铸铁防沉降井盖" Xmtz="1．材质：φ700防盗重型球墨铸铁防沉降井盖" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="11" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="116" Qdbm="WB040504020002" Mc="φ700防盗轻型球墨铸铁井盖" Xmtz="1．材质：φ700防盗轻型球墨铸铁井盖" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="17" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="117" Qdbm="040504002017" Mc="现状检查井开孔" Xmtz="1．名称：现状检查井开孔&#xD;&#xA;2．做法：新建雨水连接管、雨水管道接至现状检查井开孔、恢复等全部费用" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="13.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
    <QdBt Bm="4" Mc="污水工程" Je="0" Zgj="0" Bz="">
      <Qdmx Xh="118" Qdbm="040501004018" Mc="塑料管铺设" Xmtz="1．管道材质：实壁PE管(环刚度≥8KN/M2)&#xD;&#xA;2．连接方式：电热熔连接&#xD;&#xA;3．管径：DN300" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="454.84" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="119" Qdbm="040501004019" Mc="塑料管铺设" Xmtz="1．安装部位：室外&#xD;&#xA;2．介质：雨水&#xD;&#xA;3．规格、压力等级：HDPE排水塑料管DN200&#xD;&#xA;4．连接形式：热熔连接&#xD;&#xA;5．压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6．说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除附属构筑物、管件及阀门等所占长度" Dw="m" Sl="12.55" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="120" Qdbm="031001006003" Mc="塑料管" Xmtz="1．安装部位：室外&#xD;&#xA;2．介质：雨水&#xD;&#xA;3．规格、压力等级：HDPE排水塑料管DN100&#xD;&#xA;4．连接形式：热熔连接&#xD;&#xA;5．压力试验及吹洗设计要求：满足设计规范及要求&#xD;&#xA;6．说明：含管件安装 刷色环" Gcnr="" Jsgz="按设计图示管道中心线以长度计算" Dw="m" Sl="88.92" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="121" Qdbm="WB040501027001" Mc="管道闭水试验" Xmtz="1．管径：D300" Gcnr="" Jsgz="按设计图示中心线长度以延长米计算，不扣除管件及阀门等所占长度" Dw="m" Sl="467.39" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="122" Qdbm="WB040504011003" Mc="φ800预制装配式钢筋混凝土检查井" Xmtz="1．名称：φ800预制装配式钢筋混凝土检查井&#xD;&#xA;2．规格：φ800mm&#xD;&#xA;3．井深：2.5m内&#xD;&#xA;4．混凝土强度等级：C40混凝土，抗渗P8&#xD;&#xA;5．钢筋制作、安装：采用-HPB300,-HRB400级钢箔，其性能指标应&#xD;&#xA;6．含检查井安装、井盖安装（材料费另计）、防坠网等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="23" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="123" Qdbm="WB040504020003" Mc="φ700防盗重型球墨铸铁防沉降井盖" Xmtz="1．材质：φ700防盗重型球墨铸铁防沉降井盖" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="124" Qdbm="WB040504020004" Mc="φ700防盗轻型球墨铸铁井盖" Xmtz="1．材质：φ700防盗轻型球墨铸铁井盖" Gcnr="" Jsgz="按设计图示数量计算" Dw="套" Sl="10" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="125" Qdbm="040504002018" Mc="检查井加固" Xmtz="1．名称：检查井加固&#xD;&#xA;2．混凝土强度等级：C30混凝土&#xD;&#xA;3．做法：含现状路面切槽、钢筋绑扎、混凝土浇筑等全部内容" Gcnr="" Jsgz="按设计图示数量计算" Dw="座" Sl="13" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
      <Qdmx Xh="126" Qdbm="040504002019" Mc="现状检查井开孔" Xmtz="1．名称：现状检查井开孔&#xD;&#xA;2．做法：新建污水管道接至现状检查井开孔、恢复等全部费用" Gcnr="" Jsgz="按设计图示数量计算" Dw="处" Sl="1.00" Zhdj="0" Rgf="0" Zcf="0" Sbf="0" Fcf="0" Clf="0" Jxf="0" Rgjj="0" Zcjj="0" Fcjj="0" Sbjj="0" Cljj="0" Jxjj="0" Zhf="0" Glf="0" Lr="0" Zhhj="0" Zgj="0" Xpsbj="false" Bz="" />
    </QdBt>
  </Qdxm>
  <Csxm>
    <ZjCs>
      <ZjCsMx Xh="1" Xmbm="JC-01" Mc="夜间施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.5" Je="0" Bz="" Cslb="1" />
      <ZjCsMx Xh="2" Xmbm="JC-02" Mc="二次搬运费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="2" />
      <ZjCsMx Xh="3" Xmbm="JC-03" Mc="冬雨季施工增加费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.8" Je="0" Bz="" Cslb="3" />
      <ZjCsMx Xh="4" Xmbm="JC-04" Mc="已完工程及设备保护费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.1" Je="0" Bz="" Cslb="4" />
      <ZjCsMx Xh="5" Xmbm="JC-05" Mc="工程定位复测费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="1" Je="0" Bz="" Cslb="5" />
      <ZjCsMx Xh="6" Xmbm="JC-06" Mc="非夜间施工照明费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0" Je="0" Bz="" Cslb="6" />
      <ZjCsMx Xh="7" Xmbm="JC-07" Mc="临时保护设施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.2" Je="0" Bz="" Cslb="7" />
      <ZjCsMx Xh="8" Xmbm="JC-08" Mc="赶工措施费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="2.2" Je="0" Bz="" Cslb="8" />
      <ZjCsMx Xh="9" Xmbm="JC-09" Mc="智慧工地建设费" Js="0" Jsgs="分部分项人工基价+分部分项机械基价-(大型机械进出场及安拆人工基价+大型机械进出场及安拆机械基价)" Fl="0.57" Je="0" Bz="" Cslb="11" />
    </ZjCs>
  </Csxm>
  <Qtxm>
    <QtxmMx Xh="1" Mc="暂列金额" Dw="项" Je="0" Bz="" Xmlb="1" />
    <QtxmMx Xh="2" Mc="专业工程暂估价" Dw="项" Je="0" Bz="" Xmlb="2" />
    <QtxmMx Xh="3" Mc="计日工" Dw="" Je="0" Bz="" Xmlb="3" />
    <QtxmMx Xh="4" Mc="总承包服务费" Dw="" Je="0" Bz="" Xmlb="4" />
  </Qtxm>
  <Zlje />
  <Clzg />
  <Zygczg />
  <Jrg>
    <JrgBt Xh="一" Mc="人工" Je="0" Lb="1" />
    <JrgBt Xh="二" Mc="材料" Je="0" Lb="2" />
    <JrgBt Xh="三" Mc="施工机械" Je="0" Lb="3" />
  </Jrg>
  <Zcbfwf>
    <ZcbfwfMx Xh="1" Mc="发包人发包专业工程" Xmjz="0" Fwnr="" Fl="0" Je="0" />
    <ZcbfwfMx Xh="2" Mc="发包人供应材料" Xmjz="0" Fwnr="" Fl="0" Je="0" />
  </Zcbfwf>
  <Fbrgycl />
  <CbrgyclCef />
</Dwgcxx>
  </Dxgcxx>
</JingJiBiao>